(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32H503CBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 41.91 0)
		)
		(property "Value" "STM32H503CBTx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -22.86 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h503cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 128KB flash, 32KB RAM, 250 MHz, 35 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H503"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H503CBTx_0_1")
		(symbol "STM32H503CBTx_1_1"
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "39")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "40")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "22")
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "46")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "34")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H503CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 41.91 0)
		)
		(property "Value" "STM32H503CBUx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -22.86 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h503cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 128KB flash, 32KB RAM, 250 MHz, 35 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H503"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H503CBUx_0_1")
		(symbol "STM32H503CBUx_1_1"
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "39")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "40")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "22")
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "46")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "34")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H503EBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "STM32H503EBYx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_2.33x2.24mm_Layout5x5_P0.4mm"
			(at -17.78 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h503eb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 128KB flash, 32KB RAM, 250 MHz, 19 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H503"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.33x2.24mm*Layout5x5*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32H503EBYx_0_1")
		(symbol "STM32H503EBYx_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "A3")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "B5")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "D3")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "C4")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PB5")
				(number "B3")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PB8")
				(number "A5")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin power_out line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "VCAP")
				(number "E2")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "D4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "C3")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "B2")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "E4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "E3")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "C1")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "B1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "A1")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "D2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "C2")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "A2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H503KBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 29.21 0)
		)
		(property "Value" "STM32H503KBUx"
			(at 5.08 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -20.32 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h503kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 128KB flash, 32KB RAM, 250 MHz, 26 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H503"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H503KBUx_0_1")
		(symbol "STM32H503KBUx_1_1"
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "26")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "27")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PB15")
				(number "18")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin power_out line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "VCAP")
				(number "16")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA8")
				(number "19")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA9")
				(number "20")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "23")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "24")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "25")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H503RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H503RBTx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h503rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 128KB flash, 32KB RAM, 250 MHz, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H503"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H503RBTx_0_1")
		(symbol "STM32H503RBTx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM0" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "OPAMP1_VINM1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 41.91 0)
		)
		(property "Value" "STM32H523CCTx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -22.86 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 272KB RAM, 35 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523CCTx_0_1")
		(symbol "STM32H523CCTx_1_1"
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "39")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "40")
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "22")
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "46")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 41.91 0)
		)
		(property "Value" "STM32H523CCUx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -22.86 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 272KB RAM, 35 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523CCUx_0_1")
		(symbol "STM32H523CCUx_1_1"
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "39")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "40")
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "22")
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "46")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523CETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 41.91 0)
		)
		(property "Value" "STM32H523CETx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -22.86 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 35 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523CETx_0_1")
		(symbol "STM32H523CETx_1_1"
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "39")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "40")
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "22")
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "46")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 41.91 0)
		)
		(property "Value" "STM32H523CEUx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -22.86 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 35 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523CEUx_0_1")
		(symbol "STM32H523CEUx_1_1"
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "39")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "40")
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "22")
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "46")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H523RCTx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 272KB RAM, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523RCTx_0_1")
		(symbol "STM32H523RCTx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H523RETx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523RETx_0_1")
		(symbol "STM32H523RETx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523VCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 67.31 0)
		)
		(property "Value" "STM32H523VCIx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 272KB RAM, 80 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523VCIx_0_1")
		(symbol "STM32H523VCIx_1_1"
			(pin input line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin input line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "A3")
			)
			(pin input line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "F2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "B1")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "C1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "B3")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "M6")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "M7")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "L9")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "M10")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "L10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "B9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "A8")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "A7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "B7")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "K12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "J11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "H11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "G11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "G12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "VCAP")
				(number "C4")
			)
			(pin power_out line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "K9")
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "D1")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "D10")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "J3")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "J10")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "C3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C9")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L7")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "L6")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J2")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C8")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "C10")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "L3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "K2")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "K4")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "L2")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "M2")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "M1")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "L4")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "D12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "B12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "B11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "K5")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "L5")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "A5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "B5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "A4")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "A2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "A1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "M11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "M12")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "L12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "G1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "H3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "H1")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "H2")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "M4")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F12")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "A12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523VCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 67.31 0)
		)
		(property "Value" "STM32H523VCTx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 272KB RAM, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523VCTx_0_1")
		(symbol "STM32H523VCTx_1_1"
			(pin input line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "48")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523VEIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 67.31 0)
		)
		(property "Value" "STM32H523VEIx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 80 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523VEIx_0_1")
		(symbol "STM32H523VEIx_1_1"
			(pin input line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin input line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "A3")
			)
			(pin input line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "F2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "B1")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "C1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "B3")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "M6")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "M7")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "L9")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "M10")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "L10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "B9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "A8")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "A7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "B7")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "K12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "J11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "H11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "G11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "G12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "VCAP")
				(number "C4")
			)
			(pin power_out line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "K9")
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "D1")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "D10")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "J3")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "J10")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "C3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C9")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L7")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "L6")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J2")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C8")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "C10")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "L3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "K2")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "K4")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "L2")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "M2")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "M1")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "L4")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "D12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "B12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "B11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "K5")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "L5")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "A5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "B5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "A4")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "A2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "A1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "M11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "M12")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "L12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "G1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "H3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "H1")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "H2")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "M4")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F12")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "A12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 67.31 0)
		)
		(property "Value" "STM32H523VETx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523VETx_0_1")
		(symbol "STM32H523VETx_1_1"
			(pin input line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "48")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523ZCJx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32H523ZCJx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -30.48 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 272KB RAM, 112 GPIO, UFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523ZCJx_0_1")
		(symbol "STM32H523ZCJx_1_1"
			(pin input line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "C4")
			)
			(pin input line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "J3")
			)
			(pin input line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "H4")
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "H2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "M8")
				(alternate "FMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "J7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "H12")
				(alternate "FMC_A12" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "G10")
				(alternate "FMC_A13" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "G11")
				(alternate "FMC_A14" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "F12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "F11")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "F10")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "D7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "B7")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "A7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "D6")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "B6")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "A5")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "E1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "F4")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "F3")
				(alternate "FMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "F2")
				(alternate "FMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "F1")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF6")
				(number "G1")
				(alternate "OCTOSPI1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "G2")
				(alternate "OCTOSPI1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "G4")
				(alternate "OCTOSPI1_IO0" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "G3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "H3")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "L6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "M6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "M7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "L7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "K7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "B2")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "C3")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "C2")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "E4")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "L8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "M9")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "K8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "L9")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "M10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "K9")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "M11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "L10")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "K10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin power_out line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "D5")
			)
			(pin power_out line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "J8")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "E7")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G5")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A12")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C6")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D10")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H5")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M12")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "K3")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H6")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "J4")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C5")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C7")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "C10")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "L3")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K4")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "M2")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "L4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "M4")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "B12")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E9")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "B11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "E8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "J6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K6")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A4")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "E6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "A3")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "B3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "K11")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "H8")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "H9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PC0")
				(number "J2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "K2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "K1")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "L1")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "E12")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "E11")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "E10")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "A11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "D9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "D2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "D8")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "C9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "A10")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "B9")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "A9")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "C8")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "B8")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "A8")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "J10")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "J11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "K12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "G8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "H10")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "J12")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "G9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523ZCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 90.17 0)
		)
		(property "Value" "STM32H523ZCTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 272KB RAM, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523ZCTx_0_1")
		(symbol "STM32H523ZCTx_1_1"
			(pin input line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "OCTOSPI1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "OCTOSPI1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "OCTOSPI1_IO0" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "70")
			)
			(pin power_out line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "133")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "134")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523ZEJx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32H523ZEJx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -30.48 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 112 GPIO, UFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523ZEJx_0_1")
		(symbol "STM32H523ZEJx_1_1"
			(pin input line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "C4")
			)
			(pin input line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "J3")
			)
			(pin input line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "H4")
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "H2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "M8")
				(alternate "FMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "J7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "H12")
				(alternate "FMC_A12" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "G10")
				(alternate "FMC_A13" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "G11")
				(alternate "FMC_A14" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "F12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "F11")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "F10")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "D7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "B7")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "A7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "D6")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "B6")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "A5")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "E1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "F4")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "F3")
				(alternate "FMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "F2")
				(alternate "FMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "F1")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF6")
				(number "G1")
				(alternate "OCTOSPI1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "G2")
				(alternate "OCTOSPI1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "G4")
				(alternate "OCTOSPI1_IO0" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "G3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "H3")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "L6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "M6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "M7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "L7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "K7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "B2")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "C3")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "C2")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "E4")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "L8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "M9")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "K8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "L9")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "M10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "K9")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "M11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "L10")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "K10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin power_out line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "D5")
			)
			(pin power_out line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "J8")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "E7")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G5")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A12")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C6")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D10")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H5")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M12")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "K3")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H6")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "J4")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C5")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C7")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "C10")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "L3")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K4")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "M2")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "L4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "M4")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "B12")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E9")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "B11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "E8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "J6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K6")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A4")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "E6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "A3")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "B3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "K11")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "H8")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "H9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PC0")
				(number "J2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "K2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "K1")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "L1")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "E12")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "E11")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "E10")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "A11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "D9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "D2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "D8")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "C9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "A10")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "B9")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "A9")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "C8")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "B8")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "A8")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "J10")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "J11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "K12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "G8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "H10")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "J12")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "G9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H523ZETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 90.17 0)
		)
		(property "Value" "STM32H523ZETx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h523ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H523ZETx_0_1")
		(symbol "STM32H523ZETx_1_1"
			(pin input line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "OCTOSPI1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "OCTOSPI1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "OCTOSPI1_IO0" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "70")
			)
			(pin power_out line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "133")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "134")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H533CETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 41.91 0)
		)
		(property "Value" "STM32H533CETx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -22.86 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h533ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 35 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H533CETx_0_1")
		(symbol "STM32H533CETx_1_1"
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "39")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "40")
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "22")
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "46")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H533CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 41.91 0)
		)
		(property "Value" "STM32H533CEUx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -22.86 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h533ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 35 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H533CEUx_0_1")
		(symbol "STM32H533CEUx_1_1"
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PB3(JTDO")
				(number "39")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "40")
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "CEC" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "22")
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "46")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H533RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H533RETx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h533re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H533RETx_0_1")
		(symbol "STM32H533RETx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H533VEIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 67.31 0)
		)
		(property "Value" "STM32H533VEIx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h533ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 80 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H533VEIx_0_1")
		(symbol "STM32H533VEIx_1_1"
			(pin input line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin input line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "A3")
			)
			(pin input line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "F2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PE0")
				(number "B1")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "C1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "B3")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "M6")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "M7")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "L9")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "M10")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "L10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "B9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "A9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "A8")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "A7")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "B7")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "B6")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "K12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "J11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "H11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "G11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "G12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "VCAP")
				(number "C4")
			)
			(pin power_out line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "K9")
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "D1")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "D10")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "J3")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "J10")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "C3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C9")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L7")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "L6")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J2")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C8")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "C10")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "L3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "K2")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "K4")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "L2")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "M2")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "M1")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "L4")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "D12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "B12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "B11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "K5")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "L5")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "A5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "B5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "A4")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PB7")
				(number "C5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "A2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "A1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "M11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "M12")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "L12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "G1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "H3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "H1")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "H2")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "M4")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "F12")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "A12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E2")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H533VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 67.31 0)
		)
		(property "Value" "STM32H533VETx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h533ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H533VETx_0_1")
		(symbol "STM32H533VETx_1_1"
			(pin input line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_out line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "48")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H533ZEJx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32H533ZEJx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-144_10x10mm_Layout12x12_P0.8mm"
			(at -30.48 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h533ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 112 GPIO, UFBGA144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout12x12*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32H533ZEJx_0_1")
		(symbol "STM32H533ZEJx_1_1"
			(pin input line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "C4")
			)
			(pin input line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "J3")
			)
			(pin input line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "H4")
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "H2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PG0")
				(number "M8")
				(alternate "FMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PG1")
				(number "J7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PG2")
				(number "H12")
				(alternate "FMC_A12" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PG3")
				(number "G10")
				(alternate "FMC_A13" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG4")
				(number "G11")
				(alternate "FMC_A14" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG6")
				(number "F12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG7")
				(number "F11")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG8")
				(number "F10")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "D7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "B7")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG11")
				(number "A7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "D6")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "B6")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "A5")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "E1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "F4")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "F3")
				(alternate "FMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "F2")
				(alternate "FMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "F1")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF6")
				(number "G1")
				(alternate "OCTOSPI1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "G2")
				(alternate "OCTOSPI1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "G4")
				(alternate "OCTOSPI1_IO0" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "G3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "H3")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "L6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "M6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "M7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "L7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "K7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "B2")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "C3")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "C2")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "E4")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "L8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "M9")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "K8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "L9")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "M10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "K9")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "M11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "L10")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "K10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin power_out line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "D5")
			)
			(pin power_out line
				(at -35.56 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "J8")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "E7")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G5")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A12")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C6")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D10")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H5")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M12")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "K3")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H6")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "J4")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C5")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C7")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "C10")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "L3")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K4")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "M2")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "L4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "M4")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "B12")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E9")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "B11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "E8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "J6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K6")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "B5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A4")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "E6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B4")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "A3")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "B3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L11")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "K11")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "H8")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "H9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PC0")
				(number "J2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "K2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "K1")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "L1")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "E12")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "E11")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "E10")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "A11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "D9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "D2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "D8")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "C9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "A10")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "B9")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "A9")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "C8")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "B8")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "A8")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "J10")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "J11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "K12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "G8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "H10")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "J12")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "G9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H533ZETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 90.17 0)
		)
		(property "Value" "STM32H533ZETx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h533ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 272KB RAM, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H533ZETx_0_1")
		(symbol "STM32H533ZETx_1_1"
			(pin input line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "OCTOSPI1_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "OCTOSPI1_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "OCTOSPI1_IO0" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "70")
			)
			(pin power_out line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "133")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "134")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_NJTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "I3C2_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "I3C2_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562AGIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H562AGIx"
			(at 20.32 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-169_7x7mm_Layout13x13_P0.5mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562ag.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 136 GPIO, UFBGA169"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562AGIx_0_1")
		(symbol "STM32H562AGIx_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "H4")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "B5")
			)
			(pin input line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "L2")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -40.64 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "B13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "B12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "A13")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "C4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "A2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "E3")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI11")
				(number "F4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "H2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PH2")
				(number "K3")
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH3")
				(number "N2")
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH4")
				(number "N1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH5")
				(number "M3")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH6")
				(number "K10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH7")
				(number "L10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH8")
				(number "M10")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH10")
				(number "M11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH11")
				(number "N12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH12")
				(number "N13")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH13")
				(number "D12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH14")
				(number "D10")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH15")
				(number "D11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG0")
				(number "L7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PG1")
				(number "K7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PG2")
				(number "J12")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PG3")
				(number "G9")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG4")
				(number "J13")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG5")
				(number "G10")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG6")
				(number "G11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG7")
				(number "G8")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG8")
				(number "F11")
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG9")
				(number "F7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG10")
				(number "A8")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG11")
				(number "E7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG12")
				(number "C8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG13")
				(number "D7")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG14")
				(number "C7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PG15")
				(number "B6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF0")
				(number "F3")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF1")
				(number "E1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PF2")
				(number "F2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PF3")
				(number "F5")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF4")
				(number "F1")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF5")
				(number "F6")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF6")
				(number "G4")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF7")
				(number "G3")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF8")
				(number "G5")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF9")
				(number "H3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF10")
				(number "G6")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF12")
				(number "N6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF13")
				(number "H7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF14")
				(number "M6")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PF15")
				(number "J7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "B4")
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "N10")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C13")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "L13")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B10")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "K2")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N7")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N11")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "L1")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "A7")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "D13")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "J4")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "J5")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "L3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "N3")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "L4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "M5")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "F13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "E13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A12")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "B11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "L5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "K6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "E6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A6")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "C6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "E5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "L11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "M13")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "J10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "J1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "H5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "G12")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "G13")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "C10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "A11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "B9")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E4")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "B1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "C1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "D9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "E9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "C9")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "A9")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "F8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "D8")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "E8")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "B8")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "J11")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "K12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "K13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "H9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "C5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "D5")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "D4")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "D3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "N8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "G7")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "L8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "H8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "M8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "L9")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "J8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "N9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562AIIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H562AIIx"
			(at 20.32 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-169_7x7mm_Layout13x13_P0.5mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562ai.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 136 GPIO, UFBGA169"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H562"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562AIIx_0_1")
		(symbol "STM32H562AIIx_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "H4")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "B5")
			)
			(pin input line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "L2")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -40.64 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "B13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "B12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "A13")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "C4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "A2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "E3")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI11")
				(number "F4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "H2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PH2")
				(number "K3")
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH3")
				(number "N2")
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH4")
				(number "N1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH5")
				(number "M3")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH6")
				(number "K10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH7")
				(number "L10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH8")
				(number "M10")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH10")
				(number "M11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH11")
				(number "N12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH12")
				(number "N13")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH13")
				(number "D12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH14")
				(number "D10")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH15")
				(number "D11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG0")
				(number "L7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PG1")
				(number "K7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PG2")
				(number "J12")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PG3")
				(number "G9")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG4")
				(number "J13")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG5")
				(number "G10")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG6")
				(number "G11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG7")
				(number "G8")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG8")
				(number "F11")
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG9")
				(number "F7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG10")
				(number "A8")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG11")
				(number "E7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG12")
				(number "C8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG13")
				(number "D7")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG14")
				(number "C7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PG15")
				(number "B6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF0")
				(number "F3")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF1")
				(number "E1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PF2")
				(number "F2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PF3")
				(number "F5")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF4")
				(number "F1")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF5")
				(number "F6")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF6")
				(number "G4")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF7")
				(number "G3")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF8")
				(number "G5")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF9")
				(number "H3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF10")
				(number "G6")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF12")
				(number "N6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF13")
				(number "H7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF14")
				(number "M6")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PF15")
				(number "J7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "B4")
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "N10")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C13")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "L13")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B10")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "K2")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N7")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N11")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "L1")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "A7")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "D13")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "J4")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "J5")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "L3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "N3")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "L4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "M5")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "F13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "E13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A12")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "B11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "L5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "K6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "E6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A6")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "C6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "E5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "L11")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "M13")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "J10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "J1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "H5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "G12")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "G13")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "C10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "A11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "B9")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E4")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "B1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "C1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "D9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "E9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "C9")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "A9")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "F8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "D8")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "E8")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "B8")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "J11")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "K12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "K13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "H9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "C5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "D5")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "D4")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "D3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "N8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "G7")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "L8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "H8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "M8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "L9")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "J8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "N9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562IGKx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H562IGKx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562ig.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562IGKx_0_1")
		(symbol "STM32H562IGKx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "D6")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "P1")
			)
			(pin input line
				(at -43.18 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "N1")
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "E14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "D14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "C14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C13")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "D4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "C4")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "D2")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "D3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "E3")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "E4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "G1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "H1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "F4")
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "G4")
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH4")
				(number "H4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH5")
				(number "J4")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH6")
				(number "M11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH7")
				(number "N12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH10")
				(number "L13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH11")
				(number "L12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH12")
				(number "K12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH13")
				(number "E12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH14")
				(number "E13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 17.78 0)
				(length 5.08)
				(name "PH15")
				(number "D13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG0")
				(number "N7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG1")
				(number "M7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG2")
				(number "L15")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG3")
				(number "K15")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG4")
				(number "K14")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG5")
				(number "K13")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG6")
				(number "J15")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG7")
				(number "J14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG8")
				(number "H14")
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG9")
				(number "C10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG10")
				(number "B10")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG11")
				(number "B9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG13")
				(number "A8")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG14")
				(number "A7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -25.4 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF1")
				(number "H3")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF3")
				(number "J2")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF4")
				(number "J3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF5")
				(number "K3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF6")
				(number "K2")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF7")
				(number "K1")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF8")
				(number "L3")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF9")
				(number "L2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF10")
				(number "L1")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF12")
				(number "P6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF13")
				(number "N6")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -68.58 0)
				(length 5.08)
				(name "PF15")
				(number "P7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "C6")
			)
			(pin power_out line
				(at -43.18 -76.2 0)
				(length 5.08)
				(name "VCAP")
				(number "M10")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C9")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F3")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F13")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M1")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "K4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N8")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N9")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N10")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "R1")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C8")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "H13")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "N3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "N2")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "P2")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "R2")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "N4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "P4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P3")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R3")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "D15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B15")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "A15")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A14")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "R4")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "M6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "A10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A9")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "B5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "A5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "B4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "R12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "R13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "P12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "P13")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "R14")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "R15")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "M2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "M3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "M4")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "M5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "H15")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "G14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F14")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "B14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "A12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "D1")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "C12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "D12")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "D11")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D10")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A11")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "P15")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "P14")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "N15")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "N14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "N13")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "M15")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "M14")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "L14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "B2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "B3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P8")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "P9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R9")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R10")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "N11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "P11")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "R11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562IGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H562IGTx"
			(at 25.4 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562ig.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562IGTx_0_1")
		(symbol "STM32H562IGTx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "31")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "38")
			)
			(pin bidirectional line
				(at -43.18 91.44 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "30")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "43")
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH3")
				(number "44")
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH4")
				(number "45")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH5")
				(number "46")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH6")
				(number "84")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH7")
				(number "85")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH8")
				(number "86")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH9")
				(number "87")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH10")
				(number "88")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH11")
				(number "89")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH12")
				(number "90")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 15.24 0)
				(length 5.08)
				(name "PG0")
				(number "66")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG1")
				(number "67")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -27.94 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF10")
				(number "28")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF12")
				(number "60")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF13")
				(number "63")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF14")
				(number "64")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "81")
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "171")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "83")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "82")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "37")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "39")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "149")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "125")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "40")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "41")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "42")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "47")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "50")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "51")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "52")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "53")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "124")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "137")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "56")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "57")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "58")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "161")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "162")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "79")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "32")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "33")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "34")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "35")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "54")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "55")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "68")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "69")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "73")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "74")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "75")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "76")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "77")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562IIKx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H562IIKx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H562"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562IIKx_0_1")
		(symbol "STM32H562IIKx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "D6")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "P1")
			)
			(pin input line
				(at -43.18 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "N1")
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "E14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "D14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "C14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C13")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "D4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "C4")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "D2")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "D3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "E3")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "E4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "G1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "H1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "F4")
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "G4")
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH4")
				(number "H4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH5")
				(number "J4")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH6")
				(number "M11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH7")
				(number "N12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH10")
				(number "L13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH11")
				(number "L12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH12")
				(number "K12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH13")
				(number "E12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH14")
				(number "E13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 17.78 0)
				(length 5.08)
				(name "PH15")
				(number "D13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG0")
				(number "N7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG1")
				(number "M7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG2")
				(number "L15")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG3")
				(number "K15")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG4")
				(number "K14")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG5")
				(number "K13")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG6")
				(number "J15")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG7")
				(number "J14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG8")
				(number "H14")
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG9")
				(number "C10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG10")
				(number "B10")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG11")
				(number "B9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG13")
				(number "A8")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG14")
				(number "A7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -25.4 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF1")
				(number "H3")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF3")
				(number "J2")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF4")
				(number "J3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF5")
				(number "K3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF6")
				(number "K2")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF7")
				(number "K1")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF8")
				(number "L3")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF9")
				(number "L2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF10")
				(number "L1")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF12")
				(number "P6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF13")
				(number "N6")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -68.58 0)
				(length 5.08)
				(name "PF15")
				(number "P7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "C6")
			)
			(pin power_out line
				(at -43.18 -76.2 0)
				(length 5.08)
				(name "VCAP")
				(number "M10")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C9")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F3")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F13")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M1")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "K4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N8")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N9")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N10")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "R1")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C8")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "H13")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "N3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "N2")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "P2")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "R2")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "N4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "P4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P3")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R3")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "D15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B15")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "A15")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A14")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "R4")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "M6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "A10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A9")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "B5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "A5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "B4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "R12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "R13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "P12")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "P13")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "R14")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "R15")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "M2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "M3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "M4")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "M5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "H15")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "G14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F14")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "B14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "A12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "D1")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "C12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "D12")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "D11")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D10")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A11")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "P15")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "P14")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "N15")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "N14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "N13")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "M15")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "M14")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "L14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "B2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "B3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P8")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "P9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R9")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R10")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "N11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "P11")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "R11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562IITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H562IITx"
			(at 25.4 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H562"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562IITx_0_1")
		(symbol "STM32H562IITx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "31")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "38")
			)
			(pin bidirectional line
				(at -43.18 91.44 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "30")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "43")
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH3")
				(number "44")
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH4")
				(number "45")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH5")
				(number "46")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH6")
				(number "84")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH7")
				(number "85")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH8")
				(number "86")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH9")
				(number "87")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH10")
				(number "88")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH11")
				(number "89")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH12")
				(number "90")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 15.24 0)
				(length 5.08)
				(name "PG0")
				(number "66")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG1")
				(number "67")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -27.94 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF10")
				(number "28")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF12")
				(number "60")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF13")
				(number "63")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF14")
				(number "64")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "81")
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "171")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "83")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "82")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "37")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "39")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "149")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "125")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "40")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "41")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "42")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "47")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "50")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "51")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "52")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "53")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "124")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "137")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "56")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "57")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "58")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "161")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "162")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "79")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "32")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "33")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "34")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "35")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "54")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "55")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "68")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "69")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "73")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "74")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "75")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "76")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "77")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562RGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H562RGTx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562RGTx_0_1")
		(symbol "STM32H562RGTx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562RGVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32H562RGVx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 53 GPIO, VFQFPN68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562RGVx_0_1")
		(symbol "STM32H562RGVx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "62")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PE0")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD11")
				(number "38")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD12")
				(number "39")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC6")
				(number "40")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC7")
				(number "41")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC8")
				(number "42")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC9")
				(number "43")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC10")
				(number "54")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC11")
				(number "55")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC12")
				(number "56")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "31")
			)
			(pin power_out line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "VCAP")
				(number "66")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "67")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "44")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "45")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "46")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "47")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "48")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "49")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "52")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "53")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "57")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "58")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "63")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "64")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562RITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H562RITx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562ri.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H562"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562RITx_0_1")
		(symbol "STM32H562RITx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562RIVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32H562RIVx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562ri.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 53 GPIO, VFQFPN68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H562"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562RIVx_0_1")
		(symbol "STM32H562RIVx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "62")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PE0")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD11")
				(number "38")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD12")
				(number "39")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC6")
				(number "40")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC7")
				(number "41")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC8")
				(number "42")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC9")
				(number "43")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC10")
				(number "54")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC11")
				(number "55")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC12")
				(number "56")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "31")
			)
			(pin power_out line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "VCAP")
				(number "66")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "67")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "44")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "45")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "46")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "47")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "48")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "49")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "52")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "53")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "57")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "58")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "63")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "64")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562VGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 67.31 0)
		)
		(property "Value" "STM32H562VGTx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562VGTx_0_1")
		(symbol "STM32H562VGTx_1_1"
			(pin input line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin power_out line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "48")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562VITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 67.31 0)
		)
		(property "Value" "STM32H562VITx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562vi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H562"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562VITx_0_1")
		(symbol "STM32H562VITx_1_1"
			(pin input line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin power_out line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "48")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562ZGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 90.17 0)
		)
		(property "Value" "STM32H562ZGTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562ZGTx_0_1")
		(symbol "STM32H562ZGTx_1_1"
			(pin input line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "70")
			)
			(pin power_out line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "133")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "134")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H562ZITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 90.17 0)
		)
		(property "Value" "STM32H562ZITx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h562zi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H562"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H562ZITx_0_1")
		(symbol "STM32H562ZITx_1_1"
			(pin input line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "70")
			)
			(pin power_out line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "133")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "134")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563AGIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H563AGIx"
			(at 20.32 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-169_7x7mm_Layout13x13_P0.5mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ag.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 136 GPIO, UFBGA169"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563AGIx_0_1")
		(symbol "STM32H563AGIx_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "H4")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "B5")
			)
			(pin input line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "L2")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -40.64 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "B13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "B12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "A13")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "C4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "A2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "E3")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI11")
				(number "F4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "H2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PH2")
				(number "K3")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH3")
				(number "N2")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH4")
				(number "N1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH5")
				(number "M3")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH6")
				(number "K10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH7")
				(number "L10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH8")
				(number "M10")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH10")
				(number "M11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH11")
				(number "N12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH12")
				(number "N13")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH13")
				(number "D12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH14")
				(number "D10")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH15")
				(number "D11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG0")
				(number "L7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PG1")
				(number "K7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PG2")
				(number "J12")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PG3")
				(number "G9")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG4")
				(number "J13")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG5")
				(number "G10")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG6")
				(number "G11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG7")
				(number "G8")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG8")
				(number "F11")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG9")
				(number "F7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG10")
				(number "A8")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG11")
				(number "E7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG12")
				(number "C8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG13")
				(number "D7")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG14")
				(number "C7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PG15")
				(number "B6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF0")
				(number "F3")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF1")
				(number "E1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PF2")
				(number "F2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PF3")
				(number "F5")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF4")
				(number "F1")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF5")
				(number "F6")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF6")
				(number "G4")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF7")
				(number "G3")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF8")
				(number "G5")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF9")
				(number "H3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF10")
				(number "G6")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF12")
				(number "N6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF13")
				(number "H7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF14")
				(number "M6")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PF15")
				(number "J7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "B4")
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "N10")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C13")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "L13")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B10")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "K2")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N7")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N11")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "L1")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "A7")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "D13")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "J4")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "J5")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "L3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "N3")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "L4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "M5")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "F13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "E13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A12")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "B11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "L5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "K6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "E6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A6")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "C6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "E5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "K11")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "L11")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "M13")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "J10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "J1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "H5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "G12")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "G13")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "C10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "A11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "B9")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E4")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "B1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "C1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "D9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "E9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "C9")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "A9")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "F8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "D8")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "E8")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "B8")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "J11")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "K12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "K13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "H9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "C5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "D5")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "D4")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "D3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "N8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "G7")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "L8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "H8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "M8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "L9")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "J8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "N9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563AIIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H563AIIx"
			(at 20.32 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-169_7x7mm_Layout13x13_P0.5mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ai.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 136 GPIO, UFBGA169"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563AIIx_0_1")
		(symbol "STM32H563AIIx_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "H4")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "B5")
			)
			(pin input line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "L2")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -40.64 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "B13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "B12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "A13")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "C4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "A2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "E3")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI11")
				(number "F4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "H2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PH2")
				(number "K3")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH3")
				(number "N2")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH4")
				(number "N1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH5")
				(number "M3")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH6")
				(number "K10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH7")
				(number "L10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH8")
				(number "M10")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH10")
				(number "M11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH11")
				(number "N12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH12")
				(number "N13")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH13")
				(number "D12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH14")
				(number "D10")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH15")
				(number "D11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG0")
				(number "L7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PG1")
				(number "K7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PG2")
				(number "J12")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PG3")
				(number "G9")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG4")
				(number "J13")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG5")
				(number "G10")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG6")
				(number "G11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG7")
				(number "G8")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG8")
				(number "F11")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG9")
				(number "F7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG10")
				(number "A8")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG11")
				(number "E7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG12")
				(number "C8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG13")
				(number "D7")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG14")
				(number "C7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PG15")
				(number "B6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF0")
				(number "F3")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF1")
				(number "E1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PF2")
				(number "F2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PF3")
				(number "F5")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF4")
				(number "F1")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF5")
				(number "F6")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF6")
				(number "G4")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF7")
				(number "G3")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF8")
				(number "G5")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF9")
				(number "H3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF10")
				(number "G6")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF12")
				(number "N6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF13")
				(number "H7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF14")
				(number "M6")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PF15")
				(number "J7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "B4")
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "N10")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C13")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "L13")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B10")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "K2")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N7")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N11")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "L1")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "A7")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "D13")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "J4")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "J5")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "L3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "N3")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "L4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "M5")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "F13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "E13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A12")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "B11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "L5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "K6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "E6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A6")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "C6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "E5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "K11")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "L11")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "M13")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "J10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "J1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "H5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "G12")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "G13")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "C10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "A11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "B9")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E4")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "B1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "C1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "D9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "E9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "C9")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "A9")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "F8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "D8")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "E8")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "B8")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "J11")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "K12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "K13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "H9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "C5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "D5")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "D4")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "D3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "N8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "G7")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "L8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "H8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "M8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "L9")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "J8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "N9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563AIIxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H563AIIxQ"
			(at 20.32 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-169_7x7mm_Layout13x13_P0.5mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ai.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 134 GPIO, UFBGA169"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563AIIxQ_0_1")
		(symbol "STM32H563AIIxQ_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "H3")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "B5")
			)
			(pin power_in line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "N9")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF+")
				(number "M2")
			)
			(pin input line
				(at -40.64 91.44 0)
				(length 5.08)
				(name "VREF-")
				(number "L2")
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI0")
				(number "B12")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI1")
				(number "C11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI2")
				(number "D10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI3")
				(number "A12")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI4")
				(number "C4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI5")
				(number "B3")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI6")
				(number "A2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI7")
				(number "A1")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PI8")
				(number "E4")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PH1")
				(number "J1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH2")
				(number "J4")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH3")
				(number "N2")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH4")
				(number "N1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH5")
				(number "L4")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH6")
				(number "N13")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH7")
				(number "L11")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH10")
				(number "K10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH11")
				(number "L13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH12")
				(number "L12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH13")
				(number "C12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PH14")
				(number "D11")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PH15")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PG0")
				(number "M6")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PG1")
				(number "K7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG2")
				(number "H13")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG3")
				(number "G9")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG4")
				(number "G11")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG5")
				(number "F8")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG6")
				(number "G12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG7")
				(number "F9")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG8")
				(number "G13")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG9")
				(number "E7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG10")
				(number "C7")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG15")
				(number "B6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF1")
				(number "F3")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF2")
				(number "F4")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PF3")
				(number "G6")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PF4")
				(number "G5")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF5")
				(number "G3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF6")
				(number "G7")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF7")
				(number "F1")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF8")
				(number "G4")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF9")
				(number "G2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF10")
				(number "H4")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF12")
				(number "K6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF13")
				(number "H7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF14")
				(number "L6")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF15")
				(number "J7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "VCAP")
				(number "A4")
			)
			(pin power_out line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "N11")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A11")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "B1")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D13")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B11")
			)
			(pin power_in line
				(at -2.54 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B4")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E12")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J12")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M11")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M3")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "L1")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N3")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "M10")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N7")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N12")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "A6")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "N10")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "E13")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "K3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "H5")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "L3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "K4")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "M4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "J5")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "N4")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "F13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "D12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "C10")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "B10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "N5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "H6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "N6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "F6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "E6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "C6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "F5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "E5")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "L10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "K11")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "J10")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "H10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "J2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "J3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "K1")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "L5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "M5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "E9")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F12")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "A10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "A9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "D9")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "E8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "A7")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "F7")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "B7")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "J11")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "H9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "K13")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "H11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "G8")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "H12")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "D5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "C5")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "C3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "D4")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "D3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "L7")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "J8")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "N8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "M8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "M9")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "K8")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "J9")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "L9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563IGKx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H563IGKx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ig.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563IGKx_0_1")
		(symbol "STM32H563IGKx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "D6")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "P1")
			)
			(pin input line
				(at -43.18 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "N1")
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "E14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "D14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "C14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C13")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "D4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "C4")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "D2")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "D3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "E3")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "E4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "G1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "H1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "F4")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "G4")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH4")
				(number "H4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH5")
				(number "J4")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH6")
				(number "M11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH7")
				(number "N12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH10")
				(number "L13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH11")
				(number "L12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH12")
				(number "K12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH13")
				(number "E12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH14")
				(number "E13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 17.78 0)
				(length 5.08)
				(name "PH15")
				(number "D13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG0")
				(number "N7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG1")
				(number "M7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG2")
				(number "L15")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG3")
				(number "K15")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG4")
				(number "K14")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG5")
				(number "K13")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG6")
				(number "J15")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG7")
				(number "J14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG8")
				(number "H14")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG9")
				(number "C10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG10")
				(number "B10")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG11")
				(number "B9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG13")
				(number "A8")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG14")
				(number "A7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -25.4 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF1")
				(number "H3")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF3")
				(number "J2")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF4")
				(number "J3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF5")
				(number "K3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF6")
				(number "K2")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF7")
				(number "K1")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF8")
				(number "L3")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF9")
				(number "L2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF10")
				(number "L1")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF12")
				(number "P6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF13")
				(number "N6")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -68.58 0)
				(length 5.08)
				(name "PF15")
				(number "P7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "C6")
			)
			(pin power_out line
				(at -43.18 -76.2 0)
				(length 5.08)
				(name "VCAP")
				(number "M10")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C9")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F3")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F13")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M1")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "K4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N8")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N9")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N10")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "R1")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C8")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "H13")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "N3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "N2")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "P2")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "R2")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "N4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "P4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P3")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R3")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "D15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B15")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "A15")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A14")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "R4")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "M6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "A10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A9")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "B5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "A5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "B4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "R12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "R13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "P12")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "P13")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "R14")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "R15")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "M2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "M3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "M4")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "M5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "H15")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "G14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F14")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "B14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "A12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "D1")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "C12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "D12")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "D11")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D10")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A11")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "P15")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "P14")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "N15")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "N14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "N13")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "M15")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "M14")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "L14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "B2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "B3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P8")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "P9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R9")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R10")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "N11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "P11")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "R11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563IGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H563IGTx"
			(at 25.4 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ig.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563IGTx_0_1")
		(symbol "STM32H563IGTx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "31")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "38")
			)
			(pin bidirectional line
				(at -43.18 91.44 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "30")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "43")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH3")
				(number "44")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH4")
				(number "45")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH5")
				(number "46")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH6")
				(number "84")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH7")
				(number "85")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH8")
				(number "86")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH9")
				(number "87")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH10")
				(number "88")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH11")
				(number "89")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH12")
				(number "90")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 15.24 0)
				(length 5.08)
				(name "PG0")
				(number "66")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG1")
				(number "67")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -27.94 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF10")
				(number "28")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF12")
				(number "60")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF13")
				(number "63")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF14")
				(number "64")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "81")
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "171")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "83")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "82")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "37")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "39")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "149")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "125")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "40")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "41")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "42")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "47")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "50")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "51")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "52")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "53")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "124")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "137")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "56")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "57")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "58")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "161")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "162")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "79")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "32")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "33")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "34")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "35")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "54")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "55")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "68")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "69")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "73")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "74")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "75")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "76")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "77")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563IIKx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H563IIKx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563IIKx_0_1")
		(symbol "STM32H563IIKx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "D6")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "P1")
			)
			(pin input line
				(at -43.18 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "N1")
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "E14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "D14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "C14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C13")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "D4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "C4")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "D2")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "D3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "E3")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "E4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "G1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "H1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "F4")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "G4")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH4")
				(number "H4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH5")
				(number "J4")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH6")
				(number "M11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH7")
				(number "N12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH10")
				(number "L13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH11")
				(number "L12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH12")
				(number "K12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH13")
				(number "E12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH14")
				(number "E13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 17.78 0)
				(length 5.08)
				(name "PH15")
				(number "D13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG0")
				(number "N7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG1")
				(number "M7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG2")
				(number "L15")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG3")
				(number "K15")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG4")
				(number "K14")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG5")
				(number "K13")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG6")
				(number "J15")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG7")
				(number "J14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG8")
				(number "H14")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG9")
				(number "C10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG10")
				(number "B10")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG11")
				(number "B9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG13")
				(number "A8")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG14")
				(number "A7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -25.4 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF1")
				(number "H3")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF3")
				(number "J2")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF4")
				(number "J3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF5")
				(number "K3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF6")
				(number "K2")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF7")
				(number "K1")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF8")
				(number "L3")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF9")
				(number "L2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF10")
				(number "L1")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF12")
				(number "P6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF13")
				(number "N6")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -68.58 0)
				(length 5.08)
				(name "PF15")
				(number "P7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "C6")
			)
			(pin power_out line
				(at -43.18 -76.2 0)
				(length 5.08)
				(name "VCAP")
				(number "M10")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C9")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F3")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F13")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M1")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "K4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N8")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N9")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N10")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "R1")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C8")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "H13")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "N3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "N2")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "P2")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "R2")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "N4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "P4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P3")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R3")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "D15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B15")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "A15")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A14")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "R4")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "M6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "A10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A9")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "B5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "A5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "B4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "R12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "R13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "P12")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "P13")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "R14")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "R15")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "M2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "M3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "M4")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "M5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "H15")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "G14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F14")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "B14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "A12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "D1")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "C12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "D12")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "D11")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D10")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A11")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "P15")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "P14")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "N15")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "N14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "N13")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "M15")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "M14")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "L14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "B2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "B3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P8")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "P9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R9")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R10")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "N11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "P11")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "R11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563IIKxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H563IIKxQ"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 139 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563IIKxQ_0_1")
		(symbol "STM32H563IIKxQ_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "K3")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "A5")
			)
			(pin power_in line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "R12")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF+")
				(number "N1")
			)
			(pin input line
				(at -40.64 91.44 0)
				(length 5.08)
				(name "VREF-")
				(number "N2")
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "A15")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "B14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "A14")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "B3")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "A2")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "C4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "A1")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "E2")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "E1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "F4")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "F3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "J1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "J2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "R2")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "P3")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH4")
				(number "R1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH5")
				(number "P1")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH6")
				(number "P13")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH7")
				(number "P14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH8")
				(number "N13")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH9")
				(number "M12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH10")
				(number "N14")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH11")
				(number "P15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PH12")
				(number "M13")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PH13")
				(number "B15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PH14")
				(number "D13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PH15")
				(number "C14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG0")
				(number "R8")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG1")
				(number "P8")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG2")
				(number "K15")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG3")
				(number "H14")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG4")
				(number "J15")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG5")
				(number "H15")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG6")
				(number "J14")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG7")
				(number "H13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG8")
				(number "G15")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG9")
				(number "B9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG10")
				(number "A9")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PG11")
				(number "C9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PG13")
				(number "C8")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PG14")
				(number "A8")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PG15")
				(number "A7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF0")
				(number "F2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF1")
				(number "F1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF2")
				(number "G3")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF3")
				(number "G2")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF4")
				(number "G1")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF5")
				(number "H3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF6")
				(number "H1")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF7")
				(number "K2")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF8")
				(number "H2")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF9")
				(number "J3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF10")
				(number "J4")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PF12")
				(number "N7")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "PF13")
				(number "P7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "PF15")
				(number "N8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "A3")
			)
			(pin power_out line
				(at -40.64 -76.2 0)
				(length 5.08)
				(name "VCAP")
				(number "R14")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D5")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D8")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D10")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "E12")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H4")
			)
			(pin power_in line
				(at -2.54 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "C1")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D11")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D14")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G4")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K1")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M4")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M2")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "L4")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "P12")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M6")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M8")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M11")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "D7")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "R13")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "F12")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "P2")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "L3")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "M3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "N5")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "M5")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "R3")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P5")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R4")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E14")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "D15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "C15")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E13")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "B13")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "C13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "N6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "P6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "B7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "C7")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "C6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "B5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "M10")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "N12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "R15")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "N15")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "M14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "L1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "L2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "K4")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "N3")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N4")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P4")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "G14")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "F14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F13")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "D12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "C11")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "D2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "A13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "C10")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "A12")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "B11")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "A11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B10")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A10")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "M15")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "L13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "K12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "L14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "K14")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "L15")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "K13")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "J13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "C5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "B4")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "D4")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "C3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R9")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P9")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "N9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R10")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R11")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "P11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "N10")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "N11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563IITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H563IITx"
			(at 25.4 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563IITx_0_1")
		(symbol "STM32H563IITx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "31")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "38")
			)
			(pin bidirectional line
				(at -43.18 91.44 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "30")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "43")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH3")
				(number "44")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH4")
				(number "45")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH5")
				(number "46")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH6")
				(number "84")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH7")
				(number "85")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH8")
				(number "86")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH9")
				(number "87")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH10")
				(number "88")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH11")
				(number "89")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH12")
				(number "90")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 15.24 0)
				(length 5.08)
				(name "PG0")
				(number "66")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG1")
				(number "67")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -27.94 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF10")
				(number "28")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF12")
				(number "60")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF13")
				(number "63")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF14")
				(number "64")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "81")
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "171")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "83")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "82")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "37")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "39")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "149")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "125")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "40")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "41")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "42")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "47")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "50")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "51")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "52")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "53")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "124")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "137")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "56")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "57")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "58")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "161")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "162")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "79")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "32")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "33")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "34")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "35")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "54")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "55")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "68")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "69")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "73")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "74")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "75")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "76")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "77")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563IITxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -40.64 113.03 0)
		)
		(property "Value" "STM32H563IITxQ"
			(at 25.4 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -40.64 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 136 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563IITxQ_0_1")
		(symbol "STM32H563IITxQ_1_1"
			(pin input line
				(at -45.72 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "30")
			)
			(pin input line
				(at -45.72 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin power_in line
				(at -45.72 96.52 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "78")
			)
			(pin input line
				(at -45.72 93.98 0)
				(length 5.08)
				(name "VREF+")
				(number "37")
			)
			(pin bidirectional line
				(at -45.72 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "28")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "29")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "42")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "43")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 45.72 0)
				(length 5.08)
				(name "PH6")
				(number "84")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 43.18 0)
				(length 5.08)
				(name "PH7")
				(number "85")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "86")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "87")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 35.56 0)
				(length 5.08)
				(name "PH11")
				(number "88")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 33.02 0)
				(length 5.08)
				(name "PH12")
				(number "89")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 30.48 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 27.94 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 25.4 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 20.32 0)
				(length 5.08)
				(name "PG0")
				(number "63")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 17.78 0)
				(length 5.08)
				(name "PG1")
				(number "64")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 7.62 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 0 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -5.08 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -7.62 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -22.86 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -25.4 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -27.94 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -30.48 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -33.02 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -35.56 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -38.1 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -40.64 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -43.18 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -45.72 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -48.26 0)
				(length 5.08)
				(name "PF11")
				(number "56")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -50.8 0)
				(length 5.08)
				(name "PF12")
				(number "57")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -53.34 0)
				(length 5.08)
				(name "PF13")
				(number "60")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -55.88 0)
				(length 5.08)
				(name "PF14")
				(number "61")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -58.42 0)
				(length 5.08)
				(name "PF15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -45.72 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "81")
			)
			(pin power_out line
				(at -45.72 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "171")
			)
			(pin power_in line
				(at -22.86 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "59")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "69")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "83")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at -2.54 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "58")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "68")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "82")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "90")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "36")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "80")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "38")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "149")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "79")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "125")
			)
			(pin bidirectional line
				(at 45.72 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "39")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "40")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "41")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "44")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "47")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "48")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "49")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "50")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "124")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "137")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "53")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "54")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "55")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "161")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "162")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "76")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "77")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "31")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "32")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "33")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "34")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "51")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "52")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "65")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "66")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "67")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "70")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "71")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "72")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "73")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "74")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "75")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563MIYxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 54.61 0)
		)
		(property "Value" "STM32H563MIYxQ"
			(at 15.24 54.61 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-80_3.5x3.27mm_Layout10x16_P0.35mm_Stagger_Offcenter"
			(at -27.94 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563mi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 57 GPIO, WLCSP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.5x3.27mm*Layout10x16*P0.35mm*Stagger*Offcenter*"
			(at 0 0 0)
		)
		(symbol "STM32H563MIYxQ_0_1")
		(symbol "STM32H563MIYxQ_1_1"
			(pin input line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "NRST")
				(number "F8")
			)
			(pin input line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "BOOT0")
				(number "D8")
			)
			(pin power_in line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "T4")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PH0")
				(number "K10")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PH1")
				(number "J9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PE7")
				(number "T6")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PE8")
				(number "N5")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PE9")
				(number "R5")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PE10")
				(number "M4")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PD0")
				(number "A3")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B4")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PD2")
				(number "A5")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PD14")
				(number "K2")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PD15")
				(number "J1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PC0")
				(number "H8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PC1")
				(number "G7")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PC2")
				(number "M10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PC3")
				(number "L9")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PC4")
				(number "M6")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PC5")
				(number "N7")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PC6")
				(number "J3")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PC7")
				(number "K4")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PC8")
				(number "J5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PC9")
				(number "F2")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PC10")
				(number "C3")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PC11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PC12")
				(number "F6")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PC13")
				(number "C9")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PC14")
				(number "D10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PC15")
				(number "F10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "VCAP")
				(number "A9")
			)
			(pin power_out line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "T2")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 5.08)
				(name "VBAT")
				(number "B10")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 5.08)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P2")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P8")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "H10")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 5.08)
				(name "VSSA")
				(number "N9")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "R1")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "N3")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "T8")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 5.08)
				(name "VDDA")
				(number "P10")
			)
			(pin power_in line
				(at 10.16 58.42 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "R3")
			)
			(pin power_in line
				(at 12.7 58.42 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B2")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA0")
				(number "K8")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA1")
				(number "J7")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "PA2")
				(number "M8")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PA3")
				(number "T10")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PA4")
				(number "R9")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PA5")
				(number "L7")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PA6")
				(number "H6")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PA7")
				(number "K6")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PA8")
				(number "G3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PA9")
				(number "H4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PA10")
				(number "G5")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PA11")
				(number "E1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PA12")
				(number "C1")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "F4")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "E3")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "D4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB0")
				(number "R7")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB1")
				(number "P6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PB2")
				(number "L5")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "C5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "B6")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PB6")
				(number "E7")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PB7")
				(number "C7")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PB8")
				(number "E9")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PB10")
				(number "P4")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PB12")
				(number "L3")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PB13")
				(number "M2")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PB14")
				(number "N1")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PB15")
				(number "L1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563RGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H563RGTx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563RGTx_0_1")
		(symbol "STM32H563RGTx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563RGVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32H563RGVx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563rg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 53 GPIO, VFQFPN68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563RGVx_0_1")
		(symbol "STM32H563RGVx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "62")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PE0")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD11")
				(number "38")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD12")
				(number "39")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC6")
				(number "40")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC7")
				(number "41")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC8")
				(number "42")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC9")
				(number "43")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC10")
				(number "54")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC11")
				(number "55")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC12")
				(number "56")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "31")
			)
			(pin power_out line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "VCAP")
				(number "66")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "67")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "44")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "45")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "46")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "47")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "48")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "49")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "52")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "53")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "57")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "58")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "63")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "64")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563RITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H563RITx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ri.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563RITx_0_1")
		(symbol "STM32H563RITx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563RIVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32H563RIVx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563ri.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 53 GPIO, VFQFPN68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563RIVx_0_1")
		(symbol "STM32H563RIVx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "62")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PE0")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD11")
				(number "38")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD12")
				(number "39")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC6")
				(number "40")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC7")
				(number "41")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC8")
				(number "42")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC9")
				(number "43")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC10")
				(number "54")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC11")
				(number "55")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC12")
				(number "56")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "31")
			)
			(pin power_out line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "VCAP")
				(number "66")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "67")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "44")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "45")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "46")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "47")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "48")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "49")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "52")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "53")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "57")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "58")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "63")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "64")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563VGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 67.31 0)
		)
		(property "Value" "STM32H563VGTx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563vg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563VGTx_0_1")
		(symbol "STM32H563VGTx_1_1"
			(pin input line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin power_out line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "48")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563VITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 67.31 0)
		)
		(property "Value" "STM32H563VITx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563vi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563VITx_0_1")
		(symbol "STM32H563VITx_1_1"
			(pin input line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin power_out line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "48")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563VITxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 64.77 0)
		)
		(property "Value" "STM32H563VITxQ"
			(at 12.7 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -27.94 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563vi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 78 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563VITxQ_0_1")
		(symbol "STM32H563VITxQ_1_1"
			(pin input line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin power_in line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "46")
			)
			(pin input line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "VREF+")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "35")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "36")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "37")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "38")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "39")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "40")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "41")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PE14")
				(number "42")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "43")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "49")
			)
			(pin power_out line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -10.16 68.58 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 68.58 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "47")
			)
			(pin power_in line
				(at 10.16 68.58 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA0")
				(number "22")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA1")
				(number "23")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA2")
				(number "24")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA4")
				(number "28")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA5")
				(number "29")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "PA6")
				(number "30")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PA7")
				(number "31")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PB10")
				(number "44")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PB11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563ZGTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 90.17 0)
		)
		(property "Value" "STM32H563ZGTx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563zg.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 1024KB flash, 640KB RAM, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H5x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563ZGTx_0_1")
		(symbol "STM32H563ZGTx_1_1"
			(pin input line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "70")
			)
			(pin power_out line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "133")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "134")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563ZITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 90.17 0)
		)
		(property "Value" "STM32H563ZITx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563zi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563ZITx_0_1")
		(symbol "STM32H563ZITx_1_1"
			(pin input line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "70")
			)
			(pin power_out line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "133")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "134")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H563ZITxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 87.63 0)
		)
		(property "Value" "STM32H563ZITxQ"
			(at 20.32 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -83.82 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h563zi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 110 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H563ZITxQ_0_1")
		(symbol "STM32H563ZITxQ_1_1"
			(pin input line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "BOOT0")
				(number "137")
			)
			(pin power_in line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "68")
			)
			(pin input line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "VREF+")
				(number "31")
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "53")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "54")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "126")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "127")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "128")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "131")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "46")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "47")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "140")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "141")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "55")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "56")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "60")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "61")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "62")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "63")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "64")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "71")
			)
			(pin power_out line
				(at -40.64 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "59")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "129")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at -2.54 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "58")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "72")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 0 -88.9 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -88.9 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "70")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "130")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "32")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 15.24 91.44 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "69")
			)
			(pin power_in line
				(at 17.78 91.44 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "33")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "34")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "35")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "36")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "39")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "40")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "41")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "42")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "43")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "44")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "45")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "132")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "133")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "135")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "136")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "138")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "139")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "66")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573AIIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H573AIIx"
			(at 20.32 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-169_7x7mm_Layout13x13_P0.5mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573ai.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 136 GPIO, UFBGA169"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573AIIx_0_1")
		(symbol "STM32H573AIIx_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "H4")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "B5")
			)
			(pin input line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "L2")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -40.64 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "B13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "B12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "A13")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "C4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "A2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "E3")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI11")
				(number "F4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "H2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PH2")
				(number "K3")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH3")
				(number "N2")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH4")
				(number "N1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH5")
				(number "M3")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH6")
				(number "K10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH7")
				(number "L10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH8")
				(number "M10")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH10")
				(number "M11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH11")
				(number "N12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH12")
				(number "N13")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH13")
				(number "D12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH14")
				(number "D10")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH15")
				(number "D11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG0")
				(number "L7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PG1")
				(number "K7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PG2")
				(number "J12")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PG3")
				(number "G9")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG4")
				(number "J13")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG5")
				(number "G10")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG6")
				(number "G11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG7")
				(number "G8")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG8")
				(number "F11")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG9")
				(number "F7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG10")
				(number "A8")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG11")
				(number "E7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG12")
				(number "C8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG13")
				(number "D7")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG14")
				(number "C7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PG15")
				(number "B6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF0")
				(number "F3")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF1")
				(number "E1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PF2")
				(number "F2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PF3")
				(number "F5")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF4")
				(number "F1")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF5")
				(number "F6")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF6")
				(number "G4")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF7")
				(number "G3")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF8")
				(number "G5")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF9")
				(number "H3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF10")
				(number "G6")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF12")
				(number "N6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF13")
				(number "H7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF14")
				(number "M6")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PF15")
				(number "J7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "B4")
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "N10")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "E2")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A10")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C13")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "L13")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B10")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "B3")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "C12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "K2")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N7")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N11")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "L1")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "A7")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "D13")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "J4")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "J5")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "L3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "N3")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "L4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "M5")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "F13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "E13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A12")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "B11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "L5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "K6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "E6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A6")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "C6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "E5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "M9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "K11")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "L11")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "M13")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "J10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "J1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "H5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "F9")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "F10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "G12")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "G13")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "C10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "A11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "B9")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E4")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "B1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "C1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "D9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "E9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "C9")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "A9")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "F8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "D8")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "E8")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "B8")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "J9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "J11")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "H10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "K12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "K13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "H9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "C5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "D5")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "D4")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "D3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "N8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "G7")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "L8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "H8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "M8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "K8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "L9")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "J8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "N9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573AIIxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H573AIIxQ"
			(at 20.32 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-169_7x7mm_Layout13x13_P0.5mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573ai.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 134 GPIO, UFBGA169"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout13x13*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573AIIxQ_0_1")
		(symbol "STM32H573AIIxQ_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "H3")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "B5")
			)
			(pin power_in line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "N9")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF+")
				(number "M2")
			)
			(pin input line
				(at -40.64 91.44 0)
				(length 5.08)
				(name "VREF-")
				(number "L2")
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI0")
				(number "B12")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI1")
				(number "C11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI2")
				(number "D10")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI3")
				(number "A12")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI4")
				(number "C4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI5")
				(number "B3")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI6")
				(number "A2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI7")
				(number "A1")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PI8")
				(number "E4")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH0")
				(number "H1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PH1")
				(number "J1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH2")
				(number "J4")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH3")
				(number "N2")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH4")
				(number "N1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH5")
				(number "L4")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH6")
				(number "N13")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH7")
				(number "L11")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH10")
				(number "K10")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH11")
				(number "L13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH12")
				(number "L12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH13")
				(number "C12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PH14")
				(number "D11")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PH15")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PG0")
				(number "M6")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PG1")
				(number "K7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG2")
				(number "H13")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG3")
				(number "G9")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG4")
				(number "G11")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG5")
				(number "F8")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG6")
				(number "G12")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG7")
				(number "F9")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG8")
				(number "G13")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG9")
				(number "E7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG10")
				(number "C7")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG15")
				(number "B6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF1")
				(number "F3")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF2")
				(number "F4")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PF3")
				(number "G6")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PF4")
				(number "G5")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF5")
				(number "G3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF6")
				(number "G7")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF7")
				(number "F1")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF8")
				(number "G4")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF9")
				(number "G2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF10")
				(number "H4")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF11")
				(number "J6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF12")
				(number "K6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF13")
				(number "H7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF14")
				(number "L6")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF15")
				(number "J7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "VCAP")
				(number "A4")
			)
			(pin power_out line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "N11")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A3")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "A11")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "B1")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D13")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B11")
			)
			(pin power_in line
				(at -2.54 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B4")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E12")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J12")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M11")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M3")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "L1")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N3")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "M10")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N7")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N12")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "A6")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "N10")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "E13")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "K3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "H5")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "L3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "K4")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "M4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "J5")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "N4")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "K5")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "E10")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "F13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "D12")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "C10")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "B10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "N5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "H6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "N6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "F6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "E6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "C6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "D6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "F5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "E5")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "L10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "K11")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "J10")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "H10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "J2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "J3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "K1")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "L5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "M5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "F10")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "F11")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "E9")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F12")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "A10")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "A9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "D9")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "E8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D8")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "A7")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "F7")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "B7")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "J11")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "H9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "K13")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "H8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "H11")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "G8")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "H12")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "G10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "D5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "C5")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "C3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "D4")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "D3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "L7")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "J8")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "N8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "M8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "M9")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "K8")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "J9")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "L9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573IIKx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H573IIKx"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 140 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573IIKx_0_1")
		(symbol "STM32H573IIKx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "J1")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "D6")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "P1")
			)
			(pin input line
				(at -43.18 93.98 0)
				(length 5.08)
				(name "VREF-")
				(number "N1")
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "E14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "D14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "C14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "C13")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "D4")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "C4")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "C3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "D2")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "D3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "E3")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "E4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "G1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "H1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "F4")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "G4")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH4")
				(number "H4")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH5")
				(number "J4")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH6")
				(number "M11")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH7")
				(number "N12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH8")
				(number "M12")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH9")
				(number "M13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH10")
				(number "L13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH11")
				(number "L12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH12")
				(number "K12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH13")
				(number "E12")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH14")
				(number "E13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 17.78 0)
				(length 5.08)
				(name "PH15")
				(number "D13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG0")
				(number "N7")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG1")
				(number "M7")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG2")
				(number "L15")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG3")
				(number "K15")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG4")
				(number "K14")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG5")
				(number "K13")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG6")
				(number "J15")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG7")
				(number "J14")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG8")
				(number "H14")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG9")
				(number "C10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG10")
				(number "B10")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG11")
				(number "B9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG13")
				(number "A8")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG14")
				(number "A7")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -25.4 0)
				(length 5.08)
				(name "PG15")
				(number "B7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF0")
				(number "E2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF1")
				(number "H3")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF2")
				(number "H2")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF3")
				(number "J2")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF4")
				(number "J3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF5")
				(number "K3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF6")
				(number "K2")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF7")
				(number "K1")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF8")
				(number "L3")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF9")
				(number "L2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF10")
				(number "L1")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF12")
				(number "P6")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF13")
				(number "N6")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -68.58 0)
				(length 5.08)
				(name "PF15")
				(number "P7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "C6")
			)
			(pin power_out line
				(at -43.18 -76.2 0)
				(length 5.08)
				(name "VCAP")
				(number "M10")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "C1")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C5")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C7")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "C9")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F3")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "F13")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "G13")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G2")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L4")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M8")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J13")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M1")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "K4")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N8")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N9")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "N10")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "R1")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "C8")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "H13")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "N3")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "N2")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "P2")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "R2")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "N4")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "P4")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P3")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R3")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "D15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "C15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "B15")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "A15")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "A14")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "A13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "R4")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "M6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "A10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "A9")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "B5")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "A5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "B4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "R12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "R13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "P12")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "P13")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "R14")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "R15")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "M2")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "M3")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "M4")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "M5")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N5")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P5")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "H15")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G15")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "G14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F14")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "B14")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "B13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "A12")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "D1")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "E1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "C12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "D12")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "D11")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "D10")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "C11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B11")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A11")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "P15")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "P14")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "N15")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "N14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "N13")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "M15")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "M14")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "L14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "A4")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "A2")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "B2")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "B3")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R8")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P8")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "P9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R9")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R10")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "N11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "P11")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "R11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573IIKxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 113.03 0)
		)
		(property "Value" "STM32H573IIKxQ"
			(at 22.86 113.03 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-201_10x10mm_Layout15x15_P0.65mm"
			(at -35.56 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 139 GPIO, UFBGA176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*10x10mm*Layout15x15*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573IIKxQ_0_1")
		(symbol "STM32H573IIKxQ_1_1"
			(pin input line
				(at -40.64 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "K3")
			)
			(pin input line
				(at -40.64 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "A5")
			)
			(pin power_in line
				(at -40.64 96.52 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "R12")
			)
			(pin input line
				(at -40.64 93.98 0)
				(length 5.08)
				(name "VREF+")
				(number "N1")
			)
			(pin input line
				(at -40.64 91.44 0)
				(length 5.08)
				(name "VREF-")
				(number "N2")
			)
			(pin bidirectional line
				(at -40.64 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "A15")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "B14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "A14")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "B3")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "A2")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "C4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "A1")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "E2")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "E1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "F4")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "F3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "J1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "J2")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "R2")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "P3")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PH4")
				(number "R1")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PH5")
				(number "P1")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PH6")
				(number "P13")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PH7")
				(number "P14")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PH8")
				(number "N13")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PH9")
				(number "M12")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PH10")
				(number "N14")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PH11")
				(number "P15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PH12")
				(number "M13")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PH13")
				(number "B15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PH14")
				(number "D13")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PH15")
				(number "C14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PG0")
				(number "R8")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PG1")
				(number "P8")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PG2")
				(number "K15")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PG3")
				(number "H14")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PG4")
				(number "J15")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PG5")
				(number "H15")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PG6")
				(number "J14")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PG7")
				(number "H13")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PG8")
				(number "G15")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PG9")
				(number "B9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PG10")
				(number "A9")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PG11")
				(number "C9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PG12")
				(number "B8")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PG13")
				(number "C8")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PG14")
				(number "A8")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PG15")
				(number "A7")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PF0")
				(number "F2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PF1")
				(number "F1")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PF2")
				(number "G3")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PF3")
				(number "G2")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PF4")
				(number "G1")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PF5")
				(number "H3")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PF6")
				(number "H1")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PF7")
				(number "K2")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PF8")
				(number "H2")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PF9")
				(number "J3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PF10")
				(number "J4")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PF11")
				(number "R6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PF12")
				(number "N7")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "PF13")
				(number "P7")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "PF14")
				(number "R7")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "PF15")
				(number "N8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "A3")
			)
			(pin power_out line
				(at -40.64 -76.2 0)
				(length 5.08)
				(name "VCAP")
				(number "R14")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D5")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D8")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "D10")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "E12")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "H4")
			)
			(pin power_in line
				(at -2.54 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "C1")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D11")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D14")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G12")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G4")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H12")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K1")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K6")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K9")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M4")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M7")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M9")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "J12")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "M2")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "L4")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "P12")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M6")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M8")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "M11")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "D7")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "R13")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "F12")
			)
			(pin bidirectional line
				(at 40.64 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "P2")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "L3")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "M3")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "N5")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "M5")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "R3")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "P5")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "R4")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "F15")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "E15")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "E14")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "D15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "C15")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "E13")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "B13")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "C13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "R5")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "N6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "P6")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "B7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "C7")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "B6")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "C6")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "B5")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "M10")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "N12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "R15")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "N15")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "M14")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "L1")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "L2")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "K4")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "N3")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "N4")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "P4")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "G14")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "G13")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC8")
				(number "F14")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "F13")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "D12")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "C11")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "E3")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "D2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "B12")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "A13")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "C10")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "A12")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "B11")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "A11")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "B10")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "A10")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "M15")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "L13")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "K12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "L14")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "K14")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "L15")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "K13")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "J13")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "C5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "B4")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "D4")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "B2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "C3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "D3")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "R9")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "P9")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "N9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "R10")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "P10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "R11")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "P11")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "N10")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "N11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573IITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -38.1 113.03 0)
		)
		(property "Value" "STM32H573IITx"
			(at 25.4 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -38.1 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 140 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573IITx_0_1")
		(symbol "STM32H573IITx_1_1"
			(pin input line
				(at -43.18 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "31")
			)
			(pin input line
				(at -43.18 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin input line
				(at -43.18 96.52 0)
				(length 5.08)
				(name "VREF+")
				(number "38")
			)
			(pin bidirectional line
				(at -43.18 91.44 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 88.9 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 86.36 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 83.82 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 81.28 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 78.74 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 76.2 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 71.12 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 66.04 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "29")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "30")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "43")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 50.8 0)
				(length 5.08)
				(name "PH3")
				(number "44")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 5.08)
				(name "PH4")
				(number "45")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 5.08)
				(name "PH5")
				(number "46")
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "SPI6_RDY" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 5.08)
				(name "PH6")
				(number "84")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 5.08)
				(name "PH7")
				(number "85")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 5.08)
				(name "PH8")
				(number "86")
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 5.08)
				(name "PH9")
				(number "87")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 33.02 0)
				(length 5.08)
				(name "PH10")
				(number "88")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 30.48 0)
				(length 5.08)
				(name "PH11")
				(number "89")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 5.08)
				(name "PH12")
				(number "90")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 15.24 0)
				(length 5.08)
				(name "PG0")
				(number "66")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 5.08)
				(name "PG1")
				(number "67")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -17.78 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -20.32 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -27.94 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -30.48 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -33.02 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -35.56 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -38.1 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -40.64 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -43.18 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -45.72 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 5.08)
				(name "PF10")
				(number "28")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 5.08)
				(name "PF11")
				(number "59")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 5.08)
				(name "PF12")
				(number "60")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 5.08)
				(name "PF13")
				(number "63")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 5.08)
				(name "PF14")
				(number "64")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 5.08)
				(name "PF15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -43.18 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "81")
			)
			(pin power_out line
				(at -43.18 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "171")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "83")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "82")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "37")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "39")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "149")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "125")
			)
			(pin bidirectional line
				(at 43.18 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "40")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "41")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "42")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "47")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "50")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "51")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "52")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "53")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "124")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "137")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "56")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "57")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "58")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "161")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "162")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "79")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "32")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "33")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "34")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "35")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "54")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "55")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "68")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "69")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "70")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "73")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "74")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "75")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "76")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "77")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 43.18 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "78")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573IITxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -40.64 113.03 0)
		)
		(property "Value" "STM32H573IITxQ"
			(at 25.4 113.03 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at -40.64 -109.22 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573ii.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 136 GPIO, LQFP176"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573IITxQ_0_1")
		(symbol "STM32H573IITxQ_1_1"
			(pin input line
				(at -45.72 106.68 0)
				(length 5.08)
				(name "NRST")
				(number "30")
			)
			(pin input line
				(at -45.72 101.6 0)
				(length 5.08)
				(name "BOOT0")
				(number "166")
			)
			(pin power_in line
				(at -45.72 96.52 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "78")
			)
			(pin input line
				(at -45.72 93.98 0)
				(length 5.08)
				(name "VREF+")
				(number "37")
			)
			(pin bidirectional line
				(at -45.72 88.9 0)
				(length 5.08)
				(name "PI0")
				(number "131")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 86.36 0)
				(length 5.08)
				(name "PI1")
				(number "132")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 83.82 0)
				(length 5.08)
				(name "PI2")
				(number "133")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 81.28 0)
				(length 5.08)
				(name "PI3")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 78.74 0)
				(length 5.08)
				(name "PI4")
				(number "173")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 76.2 0)
				(length 5.08)
				(name "PI5")
				(number "174")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 73.66 0)
				(length 5.08)
				(name "PI6")
				(number "175")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 71.12 0)
				(length 5.08)
				(name "PI7")
				(number "176")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 68.58 0)
				(length 5.08)
				(name "PI8")
				(number "7")
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 66.04 0)
				(length 5.08)
				(name "PI9")
				(number "11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 63.5 0)
				(length 5.08)
				(name "PI10")
				(number "12")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 60.96 0)
				(length 5.08)
				(name "PI11")
				(number "13")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 55.88 0)
				(length 5.08)
				(name "PH0")
				(number "28")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 53.34 0)
				(length 5.08)
				(name "PH1")
				(number "29")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 50.8 0)
				(length 5.08)
				(name "PH2")
				(number "42")
				(alternate "ETH_CRS" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 48.26 0)
				(length 5.08)
				(name "PH3")
				(number "43")
				(alternate "ETH_COL" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 45.72 0)
				(length 5.08)
				(name "PH6")
				(number "84")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 43.18 0)
				(length 5.08)
				(name "PH7")
				(number "85")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "86")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "87")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SPI5_RDY" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 35.56 0)
				(length 5.08)
				(name "PH11")
				(number "88")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 33.02 0)
				(length 5.08)
				(name "PH12")
				(number "89")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 30.48 0)
				(length 5.08)
				(name "PH13")
				(number "128")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 27.94 0)
				(length 5.08)
				(name "PH14")
				(number "129")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 25.4 0)
				(length 5.08)
				(name "PH15")
				(number "130")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 20.32 0)
				(length 5.08)
				(name "PG0")
				(number "63")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 17.78 0)
				(length 5.08)
				(name "PG1")
				(number "64")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 5.08)
				(name "PG2")
				(number "106")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 5.08)
				(name "PG3")
				(number "107")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 5.08)
				(name "PG4")
				(number "108")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 7.62 0)
				(length 5.08)
				(name "PG5")
				(number "109")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 5.08)
				(name "PG6")
				(number "110")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 5.08)
				(name "PG7")
				(number "111")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 0 0)
				(length 5.08)
				(name "PG8")
				(number "112")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 5.08)
				(name "PG9")
				(number "152")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -5.08 0)
				(length 5.08)
				(name "PG10")
				(number "153")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -7.62 0)
				(length 5.08)
				(name "PG11")
				(number "154")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 5.08)
				(name "PG12")
				(number "155")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 5.08)
				(name "PG13")
				(number "156")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 5.08)
				(name "PG14")
				(number "157")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 5.08)
				(name "PG15")
				(number "160")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -22.86 0)
				(length 5.08)
				(name "PF0")
				(number "16")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -25.4 0)
				(length 5.08)
				(name "PF1")
				(number "17")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -27.94 0)
				(length 5.08)
				(name "PF2")
				(number "18")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -30.48 0)
				(length 5.08)
				(name "PF3")
				(number "19")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -33.02 0)
				(length 5.08)
				(name "PF4")
				(number "20")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -35.56 0)
				(length 5.08)
				(name "PF5")
				(number "21")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -38.1 0)
				(length 5.08)
				(name "PF6")
				(number "24")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -40.64 0)
				(length 5.08)
				(name "PF7")
				(number "25")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -43.18 0)
				(length 5.08)
				(name "PF8")
				(number "26")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -45.72 0)
				(length 5.08)
				(name "PF9")
				(number "27")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -48.26 0)
				(length 5.08)
				(name "PF11")
				(number "56")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -50.8 0)
				(length 5.08)
				(name "PF12")
				(number "57")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -53.34 0)
				(length 5.08)
				(name "PF13")
				(number "60")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -55.88 0)
				(length 5.08)
				(name "PF14")
				(number "61")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -45.72 -58.42 0)
				(length 5.08)
				(name "PF15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin power_out line
				(at -45.72 -63.5 0)
				(length 5.08)
				(name "VCAP")
				(number "81")
			)
			(pin power_out line
				(at -45.72 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "171")
			)
			(pin power_in line
				(at -22.86 116.84 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -20.32 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -17.78 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -15.24 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at -12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at -10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "59")
			)
			(pin power_in line
				(at -7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "69")
			)
			(pin power_in line
				(at -5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "83")
			)
			(pin power_in line
				(at -2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "91")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "102")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "113")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "126")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "135")
			)
			(pin power_in line
				(at -2.54 -114.3 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "148")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "158")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "58")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "68")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "82")
			)
			(pin passive line
				(at -2.54 -114.3 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "90")
			)
			(pin power_in line
				(at 0 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "103")
			)
			(pin power_in line
				(at 0 -114.3 90)
				(length 5.08)
				(name "VSSA")
				(number "36")
			)
			(pin power_in line
				(at 2.54 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "114")
			)
			(pin power_in line
				(at 2.54 -114.3 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "80")
			)
			(pin power_in line
				(at 5.08 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "127")
			)
			(pin power_in line
				(at 7.62 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "136")
			)
			(pin power_in line
				(at 10.16 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "159")
			)
			(pin power_in line
				(at 12.7 116.84 270)
				(length 5.08)
				(name "VDD")
				(number "172")
			)
			(pin power_in line
				(at 15.24 116.84 270)
				(length 5.08)
				(name "VDDA")
				(number "38")
			)
			(pin power_in line
				(at 17.78 116.84 270)
				(length 5.08)
				(name "VDDIO2")
				(number "149")
			)
			(pin power_in line
				(at 20.32 116.84 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "79")
			)
			(pin power_in line
				(at 22.86 116.84 270)
				(length 5.08)
				(name "VDDUSB")
				(number "125")
			)
			(pin bidirectional line
				(at 45.72 106.68 180)
				(length 5.08)
				(name "PA0")
				(number "39")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 104.14 180)
				(length 5.08)
				(name "PA1")
				(number "40")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 101.6 180)
				(length 5.08)
				(name "PA2")
				(number "41")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 99.06 180)
				(length 5.08)
				(name "PA3")
				(number "44")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 96.52 180)
				(length 5.08)
				(name "PA4")
				(number "47")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 93.98 180)
				(length 5.08)
				(name "PA5")
				(number "48")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 91.44 180)
				(length 5.08)
				(name "PA6")
				(number "49")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 88.9 180)
				(length 5.08)
				(name "PA7")
				(number "50")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 86.36 180)
				(length 5.08)
				(name "PA8")
				(number "119")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 83.82 180)
				(length 5.08)
				(name "PA9")
				(number "120")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 81.28 180)
				(length 5.08)
				(name "PA10")
				(number "121")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 78.74 180)
				(length 5.08)
				(name "PA11")
				(number "122")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 76.2 180)
				(length 5.08)
				(name "PA12")
				(number "123")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 73.66 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "124")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 71.12 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "137")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 68.58 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "138")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 63.5 180)
				(length 5.08)
				(name "PB0")
				(number "53")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 60.96 180)
				(length 5.08)
				(name "PB1")
				(number "54")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 58.42 180)
				(length 5.08)
				(name "PB2")
				(number "55")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 55.88 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "161")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 53.34 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "162")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 50.8 180)
				(length 5.08)
				(name "PB5")
				(number "163")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 48.26 180)
				(length 5.08)
				(name "PB6")
				(number "164")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 45.72 180)
				(length 5.08)
				(name "PB7")
				(number "165")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 43.18 180)
				(length 5.08)
				(name "PB8")
				(number "167")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 40.64 180)
				(length 5.08)
				(name "PB9")
				(number "168")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 38.1 180)
				(length 5.08)
				(name "PB10")
				(number "76")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 35.56 180)
				(length 5.08)
				(name "PB11")
				(number "77")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 33.02 180)
				(length 5.08)
				(name "PB12")
				(number "92")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 5.08)
				(name "PB13")
				(number "93")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 5.08)
				(name "PB14")
				(number "94")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 5.08)
				(name "PB15")
				(number "95")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 5.08)
				(name "PC0")
				(number "31")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 5.08)
				(name "PC1")
				(number "32")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 5.08)
				(name "PC2")
				(number "33")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 5.08)
				(name "PC3")
				(number "34")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 5.08)
				(name "PC4")
				(number "51")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 5.08)
				(name "PC5")
				(number "52")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 5.08)
				(name "PC6")
				(number "115")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 5.08)
				(name "PC7")
				(number "116")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 5.08)
				(name "PC8")
				(number "117")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 5.08)
				(name "PC9")
				(number "118")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 5.08)
				(name "PC10")
				(number "139")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 5.08)
				(name "PC11")
				(number "140")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -10.16 180)
				(length 5.08)
				(name "PC12")
				(number "141")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 5.08)
				(name "PC13")
				(number "8")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -15.24 180)
				(length 5.08)
				(name "PC14")
				(number "9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 5.08)
				(name "PC15")
				(number "10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 5.08)
				(name "PD0")
				(number "142")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 5.08)
				(name "PD1")
				(number "143")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 5.08)
				(name "PD2")
				(number "144")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 5.08)
				(name "PD3")
				(number "145")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -33.02 180)
				(length 5.08)
				(name "PD4")
				(number "146")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -35.56 180)
				(length 5.08)
				(name "PD5")
				(number "147")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -38.1 180)
				(length 5.08)
				(name "PD6")
				(number "150")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -40.64 180)
				(length 5.08)
				(name "PD7")
				(number "151")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -43.18 180)
				(length 5.08)
				(name "PD8")
				(number "96")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -45.72 180)
				(length 5.08)
				(name "PD9")
				(number "97")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -48.26 180)
				(length 5.08)
				(name "PD10")
				(number "98")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -50.8 180)
				(length 5.08)
				(name "PD11")
				(number "99")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -53.34 180)
				(length 5.08)
				(name "PD12")
				(number "100")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -55.88 180)
				(length 5.08)
				(name "PD13")
				(number "101")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -58.42 180)
				(length 5.08)
				(name "PD14")
				(number "104")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -60.96 180)
				(length 5.08)
				(name "PD15")
				(number "105")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -66.04 180)
				(length 5.08)
				(name "PE0")
				(number "169")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -68.58 180)
				(length 5.08)
				(name "PE1")
				(number "170")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -71.12 180)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -73.66 180)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -76.2 180)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -78.74 180)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -81.28 180)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -83.82 180)
				(length 5.08)
				(name "PE7")
				(number "65")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -86.36 180)
				(length 5.08)
				(name "PE8")
				(number "66")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -88.9 180)
				(length 5.08)
				(name "PE9")
				(number "67")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -91.44 180)
				(length 5.08)
				(name "PE10")
				(number "70")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -93.98 180)
				(length 5.08)
				(name "PE11")
				(number "71")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -96.52 180)
				(length 5.08)
				(name "PE12")
				(number "72")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -99.06 180)
				(length 5.08)
				(name "PE13")
				(number "73")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -101.6 180)
				(length 5.08)
				(name "PE14")
				(number "74")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 45.72 -104.14 180)
				(length 5.08)
				(name "PE15")
				(number "75")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573MIYxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 54.61 0)
		)
		(property "Value" "STM32H573MIYxQ"
			(at 15.24 54.61 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-80_3.5x3.27mm_Layout10x16_P0.35mm_Stagger_Offcenter"
			(at -27.94 -53.34 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573mi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 57 GPIO, WLCSP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*3.5x3.27mm*Layout10x16*P0.35mm*Stagger*Offcenter*"
			(at 0 0 0)
		)
		(symbol "STM32H573MIYxQ_0_1")
		(symbol "STM32H573MIYxQ_1_1"
			(pin input line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "NRST")
				(number "F8")
			)
			(pin input line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "BOOT0")
				(number "D8")
			)
			(pin power_in line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "T4")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PH0")
				(number "K10")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PH1")
				(number "J9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PE7")
				(number "T6")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PE8")
				(number "N5")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PE9")
				(number "R5")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PE10")
				(number "M4")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PD0")
				(number "A3")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B4")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PD2")
				(number "A5")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PD14")
				(number "K2")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PD15")
				(number "J1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PC0")
				(number "H8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PC1")
				(number "G7")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PC2")
				(number "M10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PC3")
				(number "L9")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PC4")
				(number "M6")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PC5")
				(number "N7")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PC6")
				(number "J3")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PC7")
				(number "K4")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PC8")
				(number "J5")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PC9")
				(number "F2")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PC10")
				(number "C3")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PC11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PC12")
				(number "F6")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PC13")
				(number "C9")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PC14")
				(number "D10")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PC15")
				(number "F10")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "VCAP")
				(number "A9")
			)
			(pin power_out line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "T2")
			)
			(pin power_in line
				(at -10.16 58.42 270)
				(length 5.08)
				(name "VBAT")
				(number "B10")
			)
			(pin power_in line
				(at -7.62 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "G1")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 5.08)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G9")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P2")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "P8")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "H10")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 5.08)
				(name "VSSA")
				(number "N9")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "R1")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "N3")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "T8")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 5.08)
				(name "VDDA")
				(number "P10")
			)
			(pin power_in line
				(at 10.16 58.42 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "R3")
			)
			(pin power_in line
				(at 12.7 58.42 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B2")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA0")
				(number "K8")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA1")
				(number "J7")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "PA2")
				(number "M8")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PA3")
				(number "T10")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PA4")
				(number "R9")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PA5")
				(number "L7")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PA6")
				(number "H6")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PA7")
				(number "K6")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PA8")
				(number "G3")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PA9")
				(number "H4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PA10")
				(number "G5")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PA11")
				(number "E1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PA12")
				(number "C1")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "F4")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "E3")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "D4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB0")
				(number "R7")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB1")
				(number "P6")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PB2")
				(number "L5")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "C5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "B6")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PB6")
				(number "E7")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PB7")
				(number "C7")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PB8")
				(number "E9")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PB10")
				(number "P4")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PB12")
				(number "L3")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PB13")
				(number "M2")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PB14")
				(number "N1")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PB15")
				(number "L1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573RITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "STM32H573RITx"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -22.86 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573ri.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 49 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573RITx_0_1")
		(symbol "STM32H573RITx_1_1"
			(pin input line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "VCAP")
				(number "30")
			)
			(pin power_out line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "VCAP")
				(number "62")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "56")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573RIVx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 46.99 0)
		)
		(property "Value" "STM32H573RIVx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP6.4x6.4mm"
			(at -22.86 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573ri.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 53 GPIO, VFQFPN68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573RIVx_0_1")
		(symbol "STM32H573RIVx_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "62")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PE0")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PD11")
				(number "38")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PD12")
				(number "39")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PC6")
				(number "40")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC7")
				(number "41")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC8")
				(number "42")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC9")
				(number "43")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC10")
				(number "54")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC11")
				(number "55")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC12")
				(number "56")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_out line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "VCAP")
				(number "31")
			)
			(pin power_out line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "VCAP")
				(number "66")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "67")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "68")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "44")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "45")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "46")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "47")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "48")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA13(JTMS")
				(number "49")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "PA14(JTCK")
				(number "52")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PA15(JTDI)")
				(number "53")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB3(JTDO")
				(number "57")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB4(NJTRST)")
				(number "58")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "59")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "60")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "61")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "63")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "64")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "34")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "35")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "36")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "37")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573VITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 67.31 0)
		)
		(property "Value" "STM32H573VITx"
			(at 12.7 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -25.4 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573vi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 80 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573VITx_0_1")
		(symbol "STM32H573VITx_1_1"
			(pin input line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin power_out line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VCAP")
				(number "48")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573VITxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 64.77 0)
		)
		(property "Value" "STM32H573VITxQ"
			(at 12.7 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -27.94 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573vi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 78 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573VITxQ_0_1")
		(symbol "STM32H573VITxQ_1_1"
			(pin input line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin power_in line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "46")
			)
			(pin input line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "VREF+")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "35")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "36")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "37")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "38")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "39")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "40")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "41")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PE14")
				(number "42")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "43")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin power_out line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "VCAP")
				(number "49")
			)
			(pin power_out line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "VCAP")
				(number "98")
			)
			(pin power_in line
				(at -10.16 68.58 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "50")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 68.58 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "47")
			)
			(pin power_in line
				(at 10.16 68.58 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA0")
				(number "22")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA1")
				(number "23")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA2")
				(number "24")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA4")
				(number "28")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA5")
				(number "29")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "PA6")
				(number "30")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PA7")
				(number "31")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "89")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "90")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PB10")
				(number "44")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PB11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573ZITx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 90.17 0)
		)
		(property "Value" "STM32H573ZITx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -86.36 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573zi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 112 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573ZITx_0_1")
		(symbol "STM32H573ZITx_1_1"
			(pin input line
				(at -40.64 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -40.64 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin bidirectional line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 66.04 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "VCAP")
				(number "70")
			)
			(pin power_out line
				(at -40.64 -68.58 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "31")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "133")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "134")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_INP4" bidirectional line)
				(alternate "ADC2_INP4" bidirectional line)
				(alternate "ETH_RXD0" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S1_MCK" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_INN4" bidirectional line)
				(alternate "ADC1_INP8" bidirectional line)
				(alternate "ADC2_INN4" bidirectional line)
				(alternate "ADC2_INP8" bidirectional line)
				(alternate "ETH_RXD1" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -81.28 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32H573ZITxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 87.63 0)
		)
		(property "Value" "STM32H573ZITxQ"
			(at 20.32 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -35.56 -83.82 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32h573zi.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 2048KB flash, 640KB RAM, 250 MHz, 1.62-3.6V, 110 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32H5 STM32H563/H573"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32H573ZITxQ_0_1")
		(symbol "STM32H573ZITxQ_1_1"
			(pin input line
				(at -40.64 81.28 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -40.64 76.2 0)
				(length 5.08)
				(name "BOOT0")
				(number "137")
			)
			(pin power_in line
				(at -40.64 71.12 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "68")
			)
			(pin input line
				(at -40.64 68.58 0)
				(length 5.08)
				(name "VREF+")
				(number "31")
			)
			(pin bidirectional line
				(at -40.64 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "53")
				(alternate "FMC_A10" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "54")
				(alternate "FMC_A11" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "FMC_BA0" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "FMC_BA1" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FMC_SDCLK" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FMC_NE3" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "126")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
				(alternate "USART6_DE" bidirectional line)
				(alternate "USART6_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "127")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "FMC_A24" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "USART10_CTS" bidirectional line)
				(alternate "USART10_NSS" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "128")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "USART10_DE" bidirectional line)
				(alternate "USART10_RTS" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 5.08)
				(name "PG15")
				(number "131")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_SDNCAS" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
				(alternate "USART6_CTS" bidirectional line)
				(alternate "USART6_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM5_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "LPTIM5_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI5_NSS" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "LPTIM5_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI5_SCK" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "LPTIM5_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI5_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LPTIM5_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PSSI_D15" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 5.08)
				(name "PF11")
				(number "46")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC1_INP2" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_SDNRAS" bidirectional line)
				(alternate "LPTIM6_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI5_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 5.08)
				(name "PF12")
				(number "47")
				(alternate "ADC1_INN2" bidirectional line)
				(alternate "ADC1_INP6" bidirectional line)
				(alternate "FMC_A6" bidirectional line)
				(alternate "LPTIM6_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "ADC2_INP2" bidirectional line)
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM6_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "ADC2_INN2" bidirectional line)
				(alternate "ADC2_INP6" bidirectional line)
				(alternate "FMC_A8" bidirectional line)
				(alternate "LPTIM6_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 5.08)
				(name "PE0")
				(number "140")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "UART8_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 5.08)
				(name "PE1")
				(number "141")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "UART8_TX" bidirectional line)
				(alternate "USART10_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "USART10_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DCMI_D4" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 5.08)
				(name "PE7")
				(number "55")
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART12_DE" bidirectional line)
				(alternate "UART12_RTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 5.08)
				(name "PE8")
				(number "56")
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -50.8 0)
				(length 5.08)
				(name "PE9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "UART12_RX" bidirectional line)
				(alternate "UART7_DE" bidirectional line)
				(alternate "UART7_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -53.34 0)
				(length 5.08)
				(name "PE10")
				(number "60")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "UART12_TX" bidirectional line)
				(alternate "UART7_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -55.88 0)
				(length 5.08)
				(name "PE11")
				(number "61")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI4_NSS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -58.42 0)
				(length 5.08)
				(name "PE12")
				(number "62")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI4_SCK" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -60.96 0)
				(length 5.08)
				(name "PE13")
				(number "63")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI4_MISO" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -63.5 0)
				(length 5.08)
				(name "PE14")
				(number "64")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI4_MOSI" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -40.64 -66.04 0)
				(length 5.08)
				(name "PE15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART10_CK" bidirectional line)
			)
			(pin power_out line
				(at -40.64 -71.12 0)
				(length 5.08)
				(name "VCAP")
				(number "71")
			)
			(pin power_out line
				(at -40.64 -73.66 0)
				(length 5.08)
				(name "VCAP")
				(number "142")
			)
			(pin power_in line
				(at -17.78 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "59")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "129")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at -2.54 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "58")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "72")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin power_in line
				(at 0 -88.9 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -88.9 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "70")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "130")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "32")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDIO2")
				(number "121")
			)
			(pin power_in line
				(at 15.24 91.44 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "69")
			)
			(pin power_in line
				(at 17.78 91.44 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 40.64 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "33")
				(alternate "ADC1_INN1" bidirectional line)
				(alternate "ADC1_INP0" bidirectional line)
				(alternate "ADC2_INN1" bidirectional line)
				(alternate "ADC2_INP0" bidirectional line)
				(alternate "ETH_CRS" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI3_RDY" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "34")
				(alternate "ADC1_INP1" bidirectional line)
				(alternate "ADC2_INP1" bidirectional line)
				(alternate "ETH_REF_CLK" bidirectional line)
				(alternate "ETH_RX_CLK" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "35")
				(alternate "ADC1_INP14" bidirectional line)
				(alternate "ADC2_INP14" bidirectional line)
				(alternate "ETH_MDIO" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "36")
				(alternate "ADC1_INP15" bidirectional line)
				(alternate "ADC2_INP15" bidirectional line)
				(alternate "ETH_COL" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "39")
				(alternate "ADC1_INP18" bidirectional line)
				(alternate "ADC2_INP18" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "DCMI_HSYNC" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "PSSI_DE" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "40")
				(alternate "ADC1_INN18" bidirectional line)
				(alternate "ADC1_INP19" bidirectional line)
				(alternate "ADC2_INN18" bidirectional line)
				(alternate "ADC2_INP19" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "PSSI_D14" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "41")
				(alternate "ADC1_INP3" bidirectional line)
				(alternate "ADC2_INP3" bidirectional line)
				(alternate "DCMI_PIXCLK" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_PDCK" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM13_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART11_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "42")
				(alternate "ADC1_INN3" bidirectional line)
				(alternate "ADC1_INP7" bidirectional line)
				(alternate "ADC2_INN3" bidirectional line)
				(alternate "ADC2_INP7" bidirectional line)
				(alternate "ETH_CRS_DV" bidirectional line)
				(alternate "ETH_RX_DV" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM14_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
				(alternate "USART11_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_1" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USB_SOF" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D0" bidirectional line)
				(alternate "ETH_TX_ER" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "UCPD1_DB1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 48.26 180)
				(length 5.08)
				(name "PA13(JTMS")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 45.72 180)
				(length 5.08)
				(name "PA14(JTCK")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 43.18 180)
				(length 5.08)
				(name "PA15(JTDI)")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2S1_WS" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SPI6_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "43")
				(alternate "ADC1_INN5" bidirectional line)
				(alternate "ADC1_INP9" bidirectional line)
				(alternate "ADC2_INN5" bidirectional line)
				(alternate "ADC2_INP9" bidirectional line)
				(alternate "ETH_RXD2" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART11_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "44")
				(alternate "ADC1_INP5" bidirectional line)
				(alternate "ADC2_INP5" bidirectional line)
				(alternate "ETH_RXD3" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "45")
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM5_ETR" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "SPI1_RDY" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 5.08)
				(name "PB3(JTDO")
				(number "132")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S1_CK" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM6_ETR" bidirectional line)
				(alternate "SDMMC2_D2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "UART12_CTS" bidirectional line)
				(alternate "UART7_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 5.08)
				(name "PB4(NJTRST)")
				(number "133")
				(alternate "DCMI_D7" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2S1_SDI" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC2_D3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SPI6_MISO" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "UART7_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "134")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "ETH_PPS_OUT" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_SDCKE1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_MOSI" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "135")
				(alternate "CEC" bidirectional line)
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "FMC_SDNE1" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "136")
				(alternate "DCMI_VSYNC" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "PSSI_RDY" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "138")
				(alternate "DCMI_D6" bidirectional line)
				(alternate "ETH_TXD3" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "PSSI_D6" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "SDMMC2_D4" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "139")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D7" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "PSSI_D7" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SDMMC2_CKIN" bidirectional line)
				(alternate "SDMMC2_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "66")
				(alternate "ETH_RX_ER" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "ETH_TX_EN" bidirectional line)
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "SPI4_RDY" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "FDCAN2_TX" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SDMMC2_D0" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM12_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DCMI_D2" bidirectional line)
				(alternate "ETH_TXD1" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SDMMC2_D1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM12_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART11_CTS" bidirectional line)
				(alternate "USART11_NSS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_INP10" bidirectional line)
				(alternate "ADC2_INP10" bidirectional line)
				(alternate "FMC_A25" bidirectional line)
				(alternate "FMC_SDNWE" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_INN10" bidirectional line)
				(alternate "ADC1_INP11" bidirectional line)
				(alternate "ADC2_INN10" bidirectional line)
				(alternate "ADC2_INP11" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "ETH_MDC" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "PWR_WKUP6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART11_DE" bidirectional line)
				(alternate "USART11_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_INN11" bidirectional line)
				(alternate "ADC1_INP12" bidirectional line)
				(alternate "ADC2_INN11" bidirectional line)
				(alternate "ADC2_INP12" bidirectional line)
				(alternate "ETH_TXD2" bidirectional line)
				(alternate "FMC_SDNE0" bidirectional line)
				(alternate "I2S2_SDI" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PWR_CSLEEP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_INN12" bidirectional line)
				(alternate "ADC1_INP13" bidirectional line)
				(alternate "ADC2_INN12" bidirectional line)
				(alternate "ADC2_INP13" bidirectional line)
				(alternate "ETH_TX_CLK" bidirectional line)
				(alternate "FMC_SDCKE0" bidirectional line)
				(alternate "I2S2_SDO" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PWR_CSTOP" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DCMI_D0" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "PSSI_D0" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "SDMMC2_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "USART6_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DCMI_D1" bidirectional line)
				(alternate "DEBUG_TRGIO" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D1" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "SDMMC2_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "USART6_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "DCMI_D2" bidirectional line)
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "PSSI_D2" bidirectional line)
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART6_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "AUDIOCLK" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DCMI_D3" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "PSSI_D3" bidirectional line)
				(alternate "RCC_MCO_2" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DB2" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -22.86 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DCMI_D8" bidirectional line)
				(alternate "ETH_TXD0" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D8" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "DCMI_D4" bidirectional line)
				(alternate "I2S3_SDI" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PSSI_D4" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DCMI_D9" bidirectional line)
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "PSSI_D9" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "SPI6_SCK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "TIM8_CH4N" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UART9_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -45.72 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DCMI_D11" bidirectional line)
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "LPTIM4_ETR" bidirectional line)
				(alternate "PSSI_D11" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DCMI_D5" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "PSSI_D5" bidirectional line)
				(alternate "PWR_WKUP8" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_RDY" bidirectional line)
				(alternate "TIM1_CH4N" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DCMI_D10" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "I2S3_SDO" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "PSSI_D10" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SDMMC2_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "I2S1_SDO" bidirectional line)
				(alternate "LPTIM4_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SDMMC2_CMD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN2_RX" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -68.58 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -71.12 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "DCMI_D12" bidirectional line)
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "I3C1_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "PSSI_D12" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -73.66 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "DCMI_D13" bidirectional line)
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "I3C1_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPTIM4_IN1" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "PSSI_D13" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "UART9_DE" bidirectional line)
				(alternate "UART9_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -76.2 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "UART8_CTS" bidirectional line)
				(alternate "UART9_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 40.64 -78.74 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "UART8_DE" bidirectional line)
				(alternate "UART8_RTS" bidirectional line)
				(alternate "UART9_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
)
