(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32L010C6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L010C6Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l010c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.8-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L010C6Tx_0_1")
		(symbol "STM32L010C6Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "1")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L010F4Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L010F4Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l010f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.8-3.6V, 16 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32L010F4Px_0_1")
		(symbol "STM32L010F4Px_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB9")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "18")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L010K4Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L010K4Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l010k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.8-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L010K4Tx_0_1")
		(symbol "STM32L010K4Tx_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB9")
				(number "31")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L010K8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L010K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l010k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.8-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L010K8Tx_0_1")
		(symbol "STM32L010K8Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L010R8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L010R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l010r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L010R8Tx_0_1")
		(symbol "STM32L010R8Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM21_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L010RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L010RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l010rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x0 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L010RBTx_0_1")
		(symbol "STM32L010RBTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM22_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM21_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "RTC_REFIN" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L011D_3-4_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "STM32L011D_3-4_Px"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -7.62 -12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011d3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8-16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 11 GPIO, TSSOP14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32L011D_3-4_Px_0_1")
		(symbol "STM32L011D_3-4_Px_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB9")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "8")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA9")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA10")
				(number "12")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA13")
				(number "13")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA14")
				(number "14")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L011E_3-4_Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L011E_3-4_Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die457"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011e3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8-16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 21 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die457*"
			(at 0 0 0)
		)
		(symbol "STM32L011E_3-4_Yx_0_1")
		(symbol "STM32L011E_3-4_Yx_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "B5")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "E2")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB1")
				(number "D2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "B2")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB9")
				(number "A5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "E1")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "C4")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "B4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "D4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "B3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "D3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "C3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "C1")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA9")
				(number "B1")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "A2")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L011F_3-4_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L011F_3-4_Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011f3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8-16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 16 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32L011F_3-4_Px_0_1")
		(symbol "STM32L011F_3-4_Px_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB9")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "18")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L011F_3-4_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "STM32L011F_3-4_Ux"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at -10.16 -15.24 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011f3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8-16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 16 GPIO, UFQFPN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L011F_3-4_Ux_0_1")
		(symbol "STM32L011F_3-4_Ux_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "NRST")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB1")
				(number "11")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "18")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB9")
				(number "20")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDDA")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "8")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "9")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "10")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "14")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "15")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "16")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "17")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L011G_3-4_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32L011G_3-4_Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011g3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8-16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 24 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L011G_3-4_Ux_0_1")
		(symbol "STM32L011G_3-4_Ux_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "25")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB9")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L011K_3-4_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L011K_3-4_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011k3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8-16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L011K_3-4_Tx_0_1")
		(symbol "STM32L011K_3-4_Tx_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB9")
				(number "31")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L011K_3-4_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L011K_3-4_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011k3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8-16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 28 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L011K_3-4_Ux_0_1")
		(symbol "STM32L011K_3-4_Ux_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "31")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L021D4Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "STM32L021D4Px"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -7.62 -12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l021d4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 11 GPIO, TSSOP14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32L021D4Px_0_1")
		(symbol "STM32L021D4Px_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PB9")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "8")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "PA9")
				(number "11")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PA10")
				(number "12")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "PA13")
				(number "13")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "PA14")
				(number "14")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L021F4Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L021F4Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l021f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 16 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32L021F4Px_0_1")
		(symbol "STM32L021F4Px_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB9")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "18")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L021F4Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "STM32L021F4Ux"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at -10.16 -15.24 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l021f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 16 GPIO, UFQFPN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L021F4Ux_0_1")
		(symbol "STM32L021F4Ux_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "NRST")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB1")
				(number "11")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB6")
				(number "18")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB9")
				(number "20")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDDA")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA0")
				(number "5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA1")
				(number "6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "8")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "9")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "10")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "14")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "15")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "16")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "17")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L021G4Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32L021G4Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l021g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 24 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L021G4Ux_0_1")
		(symbol "STM32L021G4Ux_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "25")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB9")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L021K4Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L021K4Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l021k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L021K4Tx_0_1")
		(symbol "STM32L021K4Tx_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB9")
				(number "31")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L021K4Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L021K4Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l021k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 28 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L021K4Ux_0_1")
		(symbol "STM32L021K4Ux_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "31")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L031C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L031C_4-6_Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L031C_4-6_Tx_0_1")
		(symbol "STM32L031C_4-6_Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "1")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L031C_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L031C_4-6_Ux"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L031C_4-6_Ux_0_1")
		(symbol "STM32L031C_4-6_Ux_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "1")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L031E_4-6_Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L031E_4-6_Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die425"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031e4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 20 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die425*"
			(at 0 0 0)
		)
		(symbol "STM32L031E_4-6_Yx_0_1")
		(symbol "STM32L031E_4-6_Yx_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "B5")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB0")
				(number "E2")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB1")
				(number "D2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "B2")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSSA")
				(number "E1")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "C4")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "B4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "D4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "B3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "D3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "C3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "C1")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA9")
				(number "B1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "A2")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L031F_4-6_Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L031F_4-6_Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32L031F_4-6_Px_0_1")
		(symbol "STM32L031F_4-6_Px_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "18")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L031G6UxS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32L031G6UxS"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L031G6UxS_0_1")
		(symbol "STM32L031G6UxS_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "25")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L031G_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L031G_4-6_Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -12.7 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 21 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L031G_4-6_Ux_0_1")
		(symbol "STM32L031G_4-6_Ux_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "25")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "28")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L031K_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L031K_4-6_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L031K_4-6_Tx_0_1")
		(symbol "STM32L031K_4-6_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L031K_4-6_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L031K_4-6_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L031K_4-6_Ux_0_1")
		(symbol "STM32L031K_4-6_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L041C6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L041C6Ux"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L041C6Ux_0_1")
		(symbol "STM32L041C6Ux_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "1")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L041C_4-6_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L041C_4-6_Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16-32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L041C_4-6_Tx_0_1")
		(symbol "STM32L041C_4-6_Tx_1_1"
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "1")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L041E6Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L041E6Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die425"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041e6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 20 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die425*"
			(at 0 0 0)
		)
		(symbol "STM32L041E6Yx_0_1")
		(symbol "STM32L041E6Yx_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "B5")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "C5")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB0")
				(number "E2")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB1")
				(number "D2")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "B2")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "D1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSSA")
				(number "E1")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "C4")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "B4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "D4")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "E4")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "B3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "D3")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "C3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA8")
				(number "C1")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA9")
				(number "B1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA10")
				(number "C2")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "A2")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L041F6Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L041F6Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32L041F6Px_0_1")
		(symbol "STM32L041F6Px_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "14")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "17")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "18")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "19")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "20")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L041G6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L041G6Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -12.7 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 21 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L041G6Ux_0_1")
		(symbol "STM32L041G6Ux_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "25")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "28")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L041G6UxS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32L041G6UxS"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L041G6UxS_0_1")
		(symbol "STM32L041G6UxS_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "24")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "25")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA13")
				(number "21")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA14")
				(number "22")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA15")
				(number "23")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L041K6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L041K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L041K6Tx_0_1")
		(symbol "STM32L041K6Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L041K6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L041K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L041K6Ux_0_1")
		(symbol "STM32L041K6Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_CK_IN" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L051C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L051C_6-8_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L051C_6-8_Tx_0_1")
		(symbol "STM32L051C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L051C_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L051C_6-8_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L051C_6-8_Ux_0_1")
		(symbol "STM32L051C_6-8_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L051K_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L051K_6-8_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L051K_6-8_Tx_0_1")
		(symbol "STM32L051K_6-8_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L051K_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L051K_6-8_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L051K_6-8_Ux_0_1")
		(symbol "STM32L051K_6-8_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L051R_6-8_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L051R_6-8_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L051R_6-8_Hx_0_1")
		(symbol "STM32L051R_6-8_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM22_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "TIM21_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L051R_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L051R_6-8_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L051R_6-8_Tx_0_1")
		(symbol "STM32L051R_6-8_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM22_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "TIM21_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L051T_6-8_Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "STM32L051T_6-8_Yx"
			(at 5.08 31.75 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die417"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051t6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die417*"
			(at 0 0 0)
		)
		(symbol "STM32L051T_6-8_Yx_0_1")
		(symbol "STM32L051T_6-8_Yx_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "NRST")
				(number "C6")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "BOOT0")
				(number "C5")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VREF+")
				(number "E6")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "A6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "B6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "D3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "C3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "F2")
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "D2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "A5")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "F1")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDA")
				(number "D5")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "D4")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "E4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA8")
				(number "E1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L052C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L052C_6-8_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L052C_6-8_Tx_0_1")
		(symbol "STM32L052C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L052C_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L052C_6-8_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L052C_6-8_Ux_0_1")
		(symbol "STM32L052C_6-8_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L052K_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L052K_6-8_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L052K_6-8_Tx_0_1")
		(symbol "STM32L052K_6-8_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L052K_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L052K_6-8_Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L052K_6-8_Ux_0_1")
		(symbol "STM32L052K_6-8_Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L052R_6-8_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L052R_6-8_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L052R_6-8_Hx_0_1")
		(symbol "STM32L052R_6-8_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L052R_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L052R_6-8_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L052R_6-8_Tx_0_1")
		(symbol "STM32L052R_6-8_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L052T8Fx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "STM32L052T8Fx"
			(at 5.08 31.75 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die417"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die417*"
			(at 0 0 0)
		)
		(symbol "STM32L052T8Fx_0_1")
		(symbol "STM32L052T8Fx_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "NRST")
				(number "C6")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "BOOT0")
				(number "C5")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VREF+")
				(number "E6")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "A6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "B6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "D3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "C3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "F2")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "D2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "A5")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "F1")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDA")
				(number "D5")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "D4")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "E4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA8")
				(number "E1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L052T_6-8_Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "STM32L052T_6-8_Yx"
			(at 5.08 31.75 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die417"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052t6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die417*"
			(at 0 0 0)
		)
		(symbol "STM32L052T_6-8_Yx_0_1")
		(symbol "STM32L052T_6-8_Yx_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "NRST")
				(number "C6")
			)
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "BOOT0")
				(number "C5")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VREF+")
				(number "E6")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "A6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "B6")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "D3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "C3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "F2")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "E2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "D2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "A5")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "F1")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDA")
				(number "D5")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "D4")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "E5")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "E4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "E3")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "F3")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA8")
				(number "E1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA11")
				(number "C2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A1")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L053C_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L053C_6-8_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L053C_6-8_Tx_0_1")
		(symbol "STM32L053C_6-8_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L053C_6-8_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L053C_6-8_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L053C_6-8_Ux_0_1")
		(symbol "STM32L053C_6-8_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L053R_6-8_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L053R_6-8_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L053R_6-8_Hx_0_1")
		(symbol "STM32L053R_6-8_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L053R_6-8_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L053R_6-8_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32-64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L053R_6-8_Tx_0_1")
		(symbol "STM32L053R_6-8_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "48")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L062C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L062C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l062c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L062C8Ux_0_1")
		(symbol "STM32L062C8Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L062K8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L062K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l062k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L062K8Tx_0_1")
		(symbol "STM32L062K8Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L062K8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L062K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l062k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L062K8Ux_0_1")
		(symbol "STM32L062K8Ux_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB2")
				(number "16")
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB8")
				(number "32")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L063C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L063C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l063c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L063C8Tx_0_1")
		(symbol "STM32L063C8Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L063C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L063C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l063c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L063C8Ux_0_1")
		(symbol "STM32L063C8Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L063R8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L063R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l063r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L063R8Tx_0_1")
		(symbol "STM32L063R8Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "48")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L071C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071C8Tx_0_1")
		(symbol "STM32L071C8Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L071C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071C8Ux_0_1")
		(symbol "STM32L071C8Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071C_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L071C_B-Z_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071C_B-Z_Tx_0_1")
		(symbol "STM32L071C_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071C_B-Z_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L071C_B-Z_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071C_B-Z_Ux_0_1")
		(symbol "STM32L071C_B-Z_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071C_B-Z_Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071C_B-Z_Yx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
		(symbol "STM32L071C_B-Z_Yx_0_1")
		(symbol "STM32L071C_B-Z_Yx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "E6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "D6")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "C5")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C4")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "E7")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "C6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "C7")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "G4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "D3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "E3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "A6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "G1")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B6")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "F7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F6")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G6")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071K8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L071K8Ux"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071K8Ux_0_1")
		(symbol "STM32L071K8Ux_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "4")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VDDIO2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071K_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L071K_B-Z_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071K_B-Z_Tx_0_1")
		(symbol "STM32L071K_B-Z_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071K_B-Z_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L071K_B-Z_Ux"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071K_B-Z_Ux_0_1")
		(symbol "STM32L071K_B-Z_Ux_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "4")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VDDIO2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071R_B-Z_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071R_B-Z_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071R_B-Z_Hx_0_1")
		(symbol "STM32L071R_B-Z_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071R_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071R_B-Z_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071R_B-Z_Tx_0_1")
		(symbol "STM32L071R_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO2")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071V8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L071V8Ix"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071V8Ix_0_1")
		(symbol "STM32L071V8Ix_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "F2")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "G11")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071V8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L071V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071V8Tx_0_1")
		(symbol "STM32L071V8Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071V_B-Z_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L071V_B-Z_Ix"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071V_B-Z_Ix_0_1")
		(symbol "STM32L071V_B-Z_Ix_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "F2")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "G11")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L071V_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L071V_B-Z_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L071V_B-Z_Tx_0_1")
		(symbol "STM32L071V_B-Z_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDIO2")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072CZEx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072CZEx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, EWLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
		(symbol "STM32L072CZEx_0_1")
		(symbol "STM32L072CZEx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "E6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "D6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "C5")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C4")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "E7")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "C6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "C7")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "G4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "D3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "E3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "A6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "G1")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B6")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "F7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F6")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G6")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072C_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L072C_B-Z_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072C_B-Z_Tx_0_1")
		(symbol "STM32L072C_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072C_B-Z_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L072C_B-Z_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072C_B-Z_Ux_0_1")
		(symbol "STM32L072C_B-Z_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072C_B-Z_Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072C_B-Z_Yx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
		(symbol "STM32L072C_B-Z_Yx_0_1")
		(symbol "STM32L072C_B-Z_Yx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "E6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "D6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "C5")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C4")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "E7")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "C6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "C7")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "G4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "D3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "E3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "A6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "G1")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B6")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "F7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F6")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G6")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072K_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L072K_B-Z_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072K_B-Z_Tx_0_1")
		(symbol "STM32L072K_B-Z_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072K_B-Z_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L072K_B-Z_Ux"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072K_B-Z_Ux_0_1")
		(symbol "STM32L072K_B-Z_Ux_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "4")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VDD_USB")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072R_B-Z_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072R_B-Z_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072R_B-Z_Hx_0_1")
		(symbol "STM32L072R_B-Z_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072R_B-Z_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072R_B-Z_Ix"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072R_B-Z_Ix_0_1")
		(symbol "STM32L072R_B-Z_Ix_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072R_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072R_B-Z_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072R_B-Z_Tx_0_1")
		(symbol "STM32L072R_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072V8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L072V8Ix"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072V8Ix_0_1")
		(symbol "STM32L072V8Ix_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "G11")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072V8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L072V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072V8Tx_0_1")
		(symbol "STM32L072V8Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072V_B-Z_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L072V_B-Z_Ix"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072V_B-Z_Ix_0_1")
		(symbol "STM32L072V_B-Z_Ix_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "G11")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L072V_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L072V_B-Z_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L072V_B-Z_Tx_0_1")
		(symbol "STM32L072V_B-Z_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073CZYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L073CZYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
		(symbol "STM32L073CZYx_0_1")
		(symbol "STM32L073CZYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "E6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "D6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "C5")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C4")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "E7")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "C6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "C7")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "G4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "D3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "E3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "A6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "G1")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "F7")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F6")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G6")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073C_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L073C_B-Z_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073C_B-Z_Tx_0_1")
		(symbol "STM32L073C_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073C_B-Z_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L073C_B-Z_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073C_B-Z_Ux_0_1")
		(symbol "STM32L073C_B-Z_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073RZIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L073RZIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073RZIx_0_1")
		(symbol "STM32L073RZIx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073R_B-Z_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L073R_B-Z_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073R_B-Z_Hx_0_1")
		(symbol "STM32L073R_B-Z_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073R_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L073R_B-Z_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073R_B-Z_Tx_0_1")
		(symbol "STM32L073R_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "48")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073V8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L073V8Ix"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073V8Ix_0_1")
		(symbol "STM32L073V8Ix_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "G11")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073V8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L073V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073V8Tx_0_1")
		(symbol "STM32L073V8Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "75")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073V_B-Z_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L073V_B-Z_Ix"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073V_B-Z_Ix_0_1")
		(symbol "STM32L073V_B-Z_Ix_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "G11")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L073V_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L073V_B-Z_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L073V_B-Z_Tx_0_1")
		(symbol "STM32L073V_B-Z_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "75")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L081CZUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L081CZUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l081cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L081CZUx_0_1")
		(symbol "STM32L081CZUx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L081C_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L081C_B-Z_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l081cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L081C_B-Z_Tx_0_1")
		(symbol "STM32L081C_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDIO2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L081KZTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L081KZTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l081kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L081KZTx_0_1")
		(symbol "STM32L081KZTx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L081KZUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L081KZUx"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l081kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L081KZUx_0_1")
		(symbol "STM32L081KZUx_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "4")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VDDIO2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L082CZUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L082CZUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l082cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L082CZUx_0_1")
		(symbol "STM32L082CZUx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L082CZYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L082CZYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l082cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
		(symbol "STM32L082CZYx_0_1")
		(symbol "STM32L082CZYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "D5")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A5")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "E6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "D6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "C5")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "C4")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "E7")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "C6")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "C7")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB0")
				(number "G4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "D3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "E3")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "A3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "B3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB8")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB9")
				(number "A6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB12")
				(number "G1")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PB14")
				(number "F1")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PB15")
				(number "E1")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A7")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B6")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "F7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E5")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F6")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "G6")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "F4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "E2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "D2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B1")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L082K_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L082K_B-Z_Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l082kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "STM32L082K_B-Z_Tx_0_1")
		(symbol "STM32L082K_B-Z_Tx_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "NRST")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "BOOT0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L082K_B-Z_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L082K_B-Z_Ux"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l082kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L082K_B-Z_Ux_0_1")
		(symbol "STM32L082K_B-Z_Ux_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "NRST")
				(number "3")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "BOOT0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PC14")
				(number "1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC15")
				(number "2")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "26")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "28")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSA")
				(number "4")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VDD_USB")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PA14")
				(number "25")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L083CZUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L083CZUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L083CZUx_0_1")
		(symbol "STM32L083CZUx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L083C_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L083C_B-Z_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L083C_B-Z_Tx_0_1")
		(symbol "STM32L083C_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD_USB")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L083R_B-Z_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L083R_B-Z_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L083R_B-Z_Hx_0_1")
		(symbol "STM32L083R_B-Z_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L083R_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L083R_B-Z_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L083R_B-Z_Tx_0_1")
		(symbol "STM32L083R_B-Z_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD_USB")
				(number "48")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L083V8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L083V8Ix"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L083V8Ix_0_1")
		(symbol "STM32L083V8Ix_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "G11")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L083V8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L083V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L083V8Tx_0_1")
		(symbol "STM32L083V8Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "75")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L083V_B-Z_Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L083V_B-Z_Ix"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L083V_B-Z_Ix_0_1")
		(symbol "STM32L083V_B-Z_Ix_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "F2")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "G2")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "G11")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L083V_B-Z_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L083V_B-Z_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128-192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L083V_B-Z_Tx_0_1")
		(symbol "STM32L083V_B-Z_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH9")
				(number "10")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PH10")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_VLCD1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD_USB")
				(number "75")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "SYS_SWDIO" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SYS_SWCLK" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LCD_VLCD3" bidirectional line)
				(alternate "SYS_VREF_OUT_PB0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SYS_VREF_OUT_PB1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
				(alternate "USART5_CK" bidirectional line)
				(alternate "USART5_DE" bidirectional line)
				(alternate "USART5_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LCD_VLCD2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM21_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM21_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM22_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM22_CH2" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM22_ETR" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM21_ETR" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
				(alternate "USART5_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L011D3Px"
		(extends "STM32L011D_3-4_Px")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "STM32L011D3Px"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -7.62 -12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011d3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 11 GPIO, TSSOP14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011D4Px"
		(extends "STM32L011D_3-4_Px")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "STM32L011D4Px"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -7.62 -12.7 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011d4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 11 GPIO, TSSOP14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011E3Yx"
		(extends "STM32L011E_3-4_Yx")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L011E3Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die457"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011e3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 21 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die457*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011E4Yx"
		(extends "STM32L011E_3-4_Yx")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L011E4Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die457"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011e4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 21 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die457*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011F3Px"
		(extends "STM32L011F_3-4_Px")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L011F3Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011f3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 16 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011F3Ux"
		(extends "STM32L011F_3-4_Ux")
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "STM32L011F3Ux"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at -10.16 -15.24 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011f3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 16 GPIO, UFQFPN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011F4Px"
		(extends "STM32L011F_3-4_Px")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L011F4Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 16 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011F4Ux"
		(extends "STM32L011F_3-4_Ux")
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "STM32L011F4Ux"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:ST_UFQFPN-20_3x3mm_P0.5mm"
			(at -10.16 -15.24 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 16 GPIO, UFQFPN20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFQFPN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011G3Ux"
		(extends "STM32L011G_3-4_Ux")
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32L011G3Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011g3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 24 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011G4Ux"
		(extends "STM32L011G_3-4_Ux")
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32L011G4Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 24 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011K3Tx"
		(extends "STM32L011K_3-4_Tx")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L011K3Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011k3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011K3Ux"
		(extends "STM32L011K_3-4_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L011K3Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011k3.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 8KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 28 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011K4Tx"
		(extends "STM32L011K_3-4_Tx")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L011K4Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 26 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L011K4Ux"
		(extends "STM32L011K_3-4_Ux")
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32L011K4Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l011k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 2KB RAM, 32 MHz, 1.65-3.6V, 28 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031C4Tx"
		(extends "STM32L031C_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L031C4Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031C4Ux"
		(extends "STM32L031C_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L031C4Ux"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031C6Tx"
		(extends "STM32L031C_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L031C6Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031C6Ux"
		(extends "STM32L031C_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L031C6Ux"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031E4Yx"
		(extends "STM32L031E_4-6_Yx")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L031E4Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die425"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031e4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 20 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die425*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031E6Yx"
		(extends "STM32L031E_4-6_Yx")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L031E6Yx"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-25_Die425"
			(at -10.16 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031e6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 20 GPIO, WLCSP25"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die425*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031F4Px"
		(extends "STM32L031F_4-6_Px")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L031F4Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031F6Px"
		(extends "STM32L031F_4-6_Px")
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "STM32L031F6Px"
			(at 5.08 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -10.16 -17.78 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 15 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031G4Ux"
		(extends "STM32L031G_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L031G4Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -12.7 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031g4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 21 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031G6Ux"
		(extends "STM32L031G_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L031G6Ux"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at -12.7 -20.32 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 21 GPIO, UFQFPN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031K4Tx"
		(extends "STM32L031K_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L031K4Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031K4Ux"
		(extends "STM32L031K_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L031K4Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031K6Tx"
		(extends "STM32L031K_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L031K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L031K6Ux"
		(extends "STM32L031K_4-6_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L031K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L041C4Tx"
		(extends "STM32L041C_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L041C4Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041c4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L041C6Tx"
		(extends "STM32L041C_4-6_Tx")
		(property "Reference" "U"
			(at -12.7 41.91 0)
		)
		(property "Value" "STM32L041C6Tx"
			(at 7.62 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l041c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051C6Tx"
		(extends "STM32L051C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L051C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051C6Ux"
		(extends "STM32L051C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L051C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051C8Tx"
		(extends "STM32L051C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L051C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051C8Ux"
		(extends "STM32L051C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L051C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051K6Tx"
		(extends "STM32L051K_6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L051K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051K6Ux"
		(extends "STM32L051K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L051K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051K8Tx"
		(extends "STM32L051K_6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L051K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051K8Ux"
		(extends "STM32L051K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L051K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051R6Hx"
		(extends "STM32L051R_6-8_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L051R6Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051R6Tx"
		(extends "STM32L051R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L051R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051R8Hx"
		(extends "STM32L051R_6-8_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L051R8Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051R8Tx"
		(extends "STM32L051R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L051R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051T6Yx"
		(extends "STM32L051T_6-8_Yx")
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "STM32L051T6Yx"
			(at 5.08 31.75 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die417"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051t6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die417*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L051T8Yx"
		(extends "STM32L051T_6-8_Yx")
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "STM32L051T8Yx"
			(at 5.08 31.75 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die417"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l051t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die417*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052C6Tx"
		(extends "STM32L052C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L052C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052C6Ux"
		(extends "STM32L052C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L052C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052C8Tx"
		(extends "STM32L052C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L052C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052C8Ux"
		(extends "STM32L052C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L052C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052K6Tx"
		(extends "STM32L052K_6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L052K6Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052K6Ux"
		(extends "STM32L052K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L052K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052K8Tx"
		(extends "STM32L052K_6-8_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L052K8Tx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052K8Ux"
		(extends "STM32L052K_6-8_Ux")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L052K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052R6Hx"
		(extends "STM32L052R_6-8_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L052R6Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052R6Tx"
		(extends "STM32L052R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L052R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052R8Hx"
		(extends "STM32L052R_6-8_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L052R8Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052R8Tx"
		(extends "STM32L052R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L052R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052T6Yx"
		(extends "STM32L052T_6-8_Yx")
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "STM32L052T6Yx"
			(at 5.08 31.75 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die417"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052t6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die417*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L052T8Yx"
		(extends "STM32L052T_6-8_Yx")
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "STM32L052T8Yx"
			(at 5.08 31.75 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-36_Die417"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l052t8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 29 GPIO, WLCSP36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die417*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L053C6Tx"
		(extends "STM32L053C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L053C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L053C6Ux"
		(extends "STM32L053C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L053C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L053C8Tx"
		(extends "STM32L053C_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L053C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L053C8Ux"
		(extends "STM32L053C_6-8_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L053C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L053R6Hx"
		(extends "STM32L053R_6-8_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L053R6Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L053R6Tx"
		(extends "STM32L053R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L053R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L053R8Hx"
		(extends "STM32L053R_6-8_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L053R8Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L053R8Tx"
		(extends "STM32L053R_6-8_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L053R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l053r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071CBTx"
		(extends "STM32L071C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L071CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071CBUx"
		(extends "STM32L071C_B-Z_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L071CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071CBYx"
		(extends "STM32L071C_B-Z_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071CBYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071CZTx"
		(extends "STM32L071C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L071CZTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071CZUx"
		(extends "STM32L071C_B-Z_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L071CZUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071CZYx"
		(extends "STM32L071C_B-Z_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071CZYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071KBTx"
		(extends "STM32L071K_B-Z_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L071KBTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071KBUx"
		(extends "STM32L071K_B-Z_Ux")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L071KBUx"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071KZTx"
		(extends "STM32L071K_B-Z_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L071KZTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071KZUx"
		(extends "STM32L071K_B-Z_Ux")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L071KZUx"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071RBHx"
		(extends "STM32L071R_B-Z_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071RBTx"
		(extends "STM32L071R_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071RZHx"
		(extends "STM32L071R_B-Z_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071RZHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071RZTx"
		(extends "STM32L071R_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L071RZTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071VBIx"
		(extends "STM32L071V_B-Z_Ix")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L071VBIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071VBTx"
		(extends "STM32L071V_B-Z_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L071VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071VZIx"
		(extends "STM32L071V_B-Z_Ix")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L071VZIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071vz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L071VZTx"
		(extends "STM32L071V_B-Z_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L071VZTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l071vz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072CBTx"
		(extends "STM32L072C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L072CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072CBUx"
		(extends "STM32L072C_B-Z_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L072CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072CBYx"
		(extends "STM32L072C_B-Z_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072CBYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072CZTx"
		(extends "STM32L072C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L072CZTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072CZUx"
		(extends "STM32L072C_B-Z_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L072CZUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072CZYx"
		(extends "STM32L072C_B-Z_Yx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072CZYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-49_Die447"
			(at -15.24 -43.18 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 40 GPIO, WLCSP49"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die447*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072KBTx"
		(extends "STM32L072K_B-Z_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L072KBTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072KBUx"
		(extends "STM32L072K_B-Z_Ux")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L072KBUx"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072KZTx"
		(extends "STM32L072K_B-Z_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L072KZTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072KZUx"
		(extends "STM32L072K_B-Z_Ux")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L072KZUx"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072RBHx"
		(extends "STM32L072R_B-Z_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072RBIx"
		(extends "STM32L072R_B-Z_Ix")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072RBIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072RBTx"
		(extends "STM32L072R_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072RZHx"
		(extends "STM32L072R_B-Z_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072RZHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072RZIx"
		(extends "STM32L072R_B-Z_Ix")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072RZIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072RZTx"
		(extends "STM32L072R_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L072RZTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072VBIx"
		(extends "STM32L072V_B-Z_Ix")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L072VBIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072VBTx"
		(extends "STM32L072V_B-Z_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L072VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072VZIx"
		(extends "STM32L072V_B-Z_Ix")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L072VZIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072vz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L072VZTx"
		(extends "STM32L072V_B-Z_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L072VZTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l072vz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073CBTx"
		(extends "STM32L073C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L073CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073CBUx"
		(extends "STM32L073C_B-Z_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L073CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073CZTx"
		(extends "STM32L073C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L073CZTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073CZUx"
		(extends "STM32L073C_B-Z_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L073CZUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073RBHx"
		(extends "STM32L073R_B-Z_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L073RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073RBTx"
		(extends "STM32L073R_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L073RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073RZHx"
		(extends "STM32L073R_B-Z_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L073RZHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073RZTx"
		(extends "STM32L073R_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L073RZTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073VBIx"
		(extends "STM32L073V_B-Z_Ix")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L073VBIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073VBTx"
		(extends "STM32L073V_B-Z_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L073VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073VZIx"
		(extends "STM32L073V_B-Z_Ix")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L073VZIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073vz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L073VZTx"
		(extends "STM32L073V_B-Z_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L073VZTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l073vz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L081CBTx"
		(extends "STM32L081C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L081CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l081cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L081CZTx"
		(extends "STM32L081C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L081CZTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l081cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L082KBTx"
		(extends "STM32L082K_B-Z_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L082KBTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l082kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L082KBUx"
		(extends "STM32L082K_B-Z_Ux")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L082KBUx"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l082kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L082KZTx"
		(extends "STM32L082K_B-Z_Tx")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "STM32L082KZTx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l082kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 25 GPIO, LQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L082KZUx"
		(extends "STM32L082K_B-Z_Ux")
		(property "Reference" "U"
			(at -12.7 24.13 0)
		)
		(property "Value" "STM32L082KZUx"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -12.7 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l082kz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 23 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083CBTx"
		(extends "STM32L083C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L083CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083CZTx"
		(extends "STM32L083C_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L083CZTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083cz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083RBHx"
		(extends "STM32L083R_B-Z_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L083RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083RBTx"
		(extends "STM32L083R_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L083RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083RZHx"
		(extends "STM32L083R_B-Z_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L083RZHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083RZTx"
		(extends "STM32L083R_B-Z_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L083RZTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083rz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083VBIx"
		(extends "STM32L083V_B-Z_Ix")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L083VBIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083VBTx"
		(extends "STM32L083V_B-Z_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L083VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083VZIx"
		(extends "STM32L083V_B-Z_Ix")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L083VZIx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083vz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L083VZTx"
		(extends "STM32L083V_B-Z_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L083VZTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l083vz.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 192KB flash, 20KB RAM, 32 MHz, 1.65-3.6V, 84 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32L0 STM32L0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
