(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32L100C6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L100C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 4KB RAM, 32 MHz, 1.8-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L100C6Ux_0_1")
		(symbol "STM32L100C6Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L100C6UxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L100C6UxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 4KB RAM, 32 MHz, 1.8-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L100C6UxA_0_1")
		(symbol "STM32L100C6UxA_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L100RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L100RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 16KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L100RCTx_0_1")
		(symbol "STM32L100RCTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L100R_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L100R_8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 8-10KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L100R_8-B_Tx_0_1")
		(symbol "STM32L100R_8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L100R_8-B_TxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L100R_8-B_TxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100r8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 8-16KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L100R_8-B_TxA_0_1")
		(symbol "STM32L100R_8-B_TxA_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151CCTx_0_1")
		(symbol "STM32L151CCTx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151CCUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151CCUx_0_1")
		(symbol "STM32L151CCUx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151C_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C_6-8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151C_6-8-B_Tx_0_1")
		(symbol "STM32L151C_6-8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151C_6-8-B_TxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C_6-8-B_TxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 16-32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151C_6-8-B_TxA_0_1")
		(symbol "STM32L151C_6-8-B_TxA_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151C_6-8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C_6-8-B_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151C_6-8-B_Ux_0_1")
		(symbol "STM32L151C_6-8-B_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151C_6-8-B_UxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C_6-8-B_UxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 16-32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151C_6-8-B_UxA_0_1")
		(symbol "STM32L151C_6-8-B_UxA_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151QCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32L151QCHx"
			(at 12.7 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151qc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 112 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151QCHx_0_1")
		(symbol "STM32L151QCHx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "M3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M4")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OPAMP3_VINM")
				(number "K1")
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG0")
				(number "H9")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG1")
				(number "G9")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG3")
				(number "F9")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG4")
				(number "F10")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG5")
				(number "E9")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "D9")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "C7")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "C6")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "D6")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "D5")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "E4")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "F3")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "F4")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "G3")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "G4")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "H4")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "J6")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF11")
				(number "K6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF12")
				(number "J7")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF13")
				(number "K7")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF14")
				(number "J8")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF15")
				(number "J9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151QDHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32L151QDHx"
			(at 12.7 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151qd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 112 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151QDHx_0_1")
		(symbol "STM32L151QDHx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "M3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M4")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OPAMP3_VINM")
				(number "K1")
				(alternate "OPAMP3_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG0")
				(number "H9")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "FSMC_A10" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG1")
				(number "G9")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "FSMC_A11" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "FSMC_A12" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG3")
				(number "F9")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "FSMC_A13" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG4")
				(number "F10")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "FSMC_A14" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG5")
				(number "E9")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "D9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "C7")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "C6")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "D6")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "D5")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "E4")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "F3")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "F4")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "G3")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "G4")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "H4")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "J6")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF11")
				(number "K6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF12")
				(number "J7")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "FSMC_A6" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF13")
				(number "K7")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "FSMC_A7" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF14")
				(number "J8")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "FSMC_A8" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF15")
				(number "J9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151QEHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 90.17 0)
		)
		(property "Value" "STM32L151QEHx"
			(at 12.7 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -22.86 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 111 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151QEHx_0_1")
		(symbol "STM32L151QEHx_1_1"
			(pin input line
				(at -27.94 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -27.94 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -27.94 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -27.94 68.58 0)
				(length 5.08)
				(name "AOP1_INN")
				(number "M3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin input line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "AOP2_INN")
				(number "M4")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PG0")
				(number "H9")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PG1")
				(number "G9")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PG3")
				(number "F9")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PG4")
				(number "F10")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PG5")
				(number "E9")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "D9")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "C7")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "C6")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PF0")
				(number "D6")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PF1")
				(number "D5")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PF3")
				(number "E4")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PF4")
				(number "F3")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PF5")
				(number "F4")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PF6")
				(number "G3")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PF7")
				(number "G4")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PF8")
				(number "H4")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PF9")
				(number "J6")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PF11")
				(number "K6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PF12")
				(number "J7")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PF13")
				(number "K7")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PF14")
				(number "J8")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PF15")
				(number "J9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin no_connect line
				(at -22.86 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "K1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 27.94 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151RCTx_0_1")
		(symbol "STM32L151RCTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151RCTxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RCTxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rc-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151RCTxA_0_1")
		(symbol "STM32L151RCTxA_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151RCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RCYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die427"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die427*"
			(at 0 0 0)
		)
		(symbol "STM32L151RCYx_0_1")
		(symbol "STM32L151RCYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "C7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "D8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "F7")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H6")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E3")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C4")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "C8")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "B8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B7")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "E7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "G8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "C6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "G4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E4")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D4")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "H4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F4")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H3")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F2")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151RDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RDTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151RDTx_0_1")
		(symbol "STM32L151RDTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151RDYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RDYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die436"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die436*"
			(at 0 0 0)
		)
		(symbol "STM32L151RDYx_0_1")
		(symbol "STM32L151RDYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "C7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "D8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "F7")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H6")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E3")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C4")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "C8")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "B8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B7")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "E7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "G8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "C6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "G4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E4")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D4")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "H4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F4")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H3")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F2")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151RETx_0_1")
		(symbol "STM32L151RETx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151R_6-8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R_6-8-B_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151R_6-8-B_Hx_0_1")
		(symbol "STM32L151R_6-8-B_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151R_6-8-B_HxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R_6-8-B_HxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 16-32KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151R_6-8-B_HxA_0_1")
		(symbol "STM32L151R_6-8-B_HxA_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151R_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R_6-8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151R_6-8-B_Tx_0_1")
		(symbol "STM32L151R_6-8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151R_6-8-B_TxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R_6-8-B_TxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 16-32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151R_6-8-B_TxA_0_1")
		(symbol "STM32L151R_6-8-B_TxA_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151UCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151UCYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-63_Die427"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151uc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, WLCSP63"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die427*"
			(at 0 0 0)
		)
		(symbol "STM32L151UCYx_0_1")
		(symbol "STM32L151UCYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "F6")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "F7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "A4")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E6")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "E5")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "G7")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "G6")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "F4")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "J4")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "D1")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "E2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "A3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "B4")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "D5")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "D7")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "D6")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B7")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J1")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F5")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "C7")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E4")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G5")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H6")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "J7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J6")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "H4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E3")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D2")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "D3")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C3")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "J3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "H3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G3")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "D4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "J2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F3")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151VCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151VCHx_0_1")
		(symbol "STM32L151VCHx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151VCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151VCTx_0_1")
		(symbol "STM32L151VCTx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151VCTxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VCTxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vc-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151VCTxA_0_1")
		(symbol "STM32L151VCTxA_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151VDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VDTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151VDTx_0_1")
		(symbol "STM32L151VDTx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151VDTxX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VDTxX"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vd-x.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151VDTxX_0_1")
		(symbol "STM32L151VDTxX_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151VDYxX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32L151VDYxX"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-104_Die437"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vd-x.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, WLCSP104"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die437*"
			(at 0 0 0)
		)
		(symbol "STM32L151VDYxX_0_1")
		(symbol "STM32L151VDYxX_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 2.54)
				(name "NRST")
				(number "F7")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 2.54)
				(name "BOOT0")
				(number "A7")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "G7")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 2.54)
				(name "VREF-")
				(number "H8")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 2.54)
				(name "PH0")
				(number "F8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "PH1")
				(number "F9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "PH2")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PE0")
				(number "B7")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PE1")
				(number "A8")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PE2")
				(number "D6")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PE3")
				(number "D7")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PE4")
				(number "C8")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PE5")
				(number "B9")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PE6")
				(number "E6")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PE7")
				(number "L6")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PE8")
				(number "M5")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PE9")
				(number "M4")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PE10")
				(number "J5")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PE11")
				(number "L5")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PE12")
				(number "M3")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PE13")
				(number "K5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE14")
				(number "L4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PE15")
				(number "K4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "A2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "D4")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "C3")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "C4")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "A3")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "B3")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "B4")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "A4")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PD8")
				(number "H4")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PD9")
				(number "J2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PD10")
				(number "K1")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PD11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PD12")
				(number "H3")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "PD13")
				(number "H2")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 2.54)
				(name "PD14")
				(number "J1")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 2.54)
				(name "PD15")
				(number "G3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "B8")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "C1")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "K3")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 2.54)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "L2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "L8")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 2.54)
				(name "VSSA")
				(number "J9")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "M9")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 2.54)
				(name "VDDA")
				(number "G6")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 2.54)
				(name "VLCD")
				(number "E7")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 2.54)
				(name "PA0")
				(number "K9")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 2.54)
				(name "PA1")
				(number "L9")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 2.54)
				(name "PA2")
				(number "J8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 2.54)
				(name "PA3")
				(number "H7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 2.54)
				(name "PA4")
				(number "J7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 2.54)
				(name "PA5")
				(number "M8")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 2.54)
				(name "PA6")
				(number "H6")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 2.54)
				(name "PA7")
				(number "K7")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PA8")
				(number "F3")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA9")
				(number "F1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA10")
				(number "F2")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA11")
				(number "E1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA12")
				(number "E2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA13")
				(number "E3")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "K6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "M6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB9")
				(number "C6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB10")
				(number "M2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB11")
				(number "L3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB12")
				(number "J4")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB13")
				(number "J3")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB14")
				(number "L1")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB15")
				(number "K2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PC0")
				(number "F6")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PC1")
				(number "H9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PC2")
				(number "G9")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PC3")
				(number "G8")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PC4")
				(number "L7")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PC5")
				(number "M7")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PC6")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PC7")
				(number "G1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "PC8")
				(number "G2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 2.54)
				(name "PC9")
				(number "F4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 2.54)
				(name "PC10")
				(number "E4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 2.54)
				(name "PC11")
				(number "C2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 2.54)
				(name "PC13")
				(number "C9")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 2.54)
				(name "PC14")
				(number "D8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151VETx_0_1")
		(symbol "STM32L151VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151VEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32L151VEYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-104_Die437"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, WLCSP104"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die437*"
			(at 0 0 0)
		)
		(symbol "STM32L151VEYx_0_1")
		(symbol "STM32L151VEYx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 2.54)
				(name "NRST")
				(number "F7")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 2.54)
				(name "BOOT0")
				(number "A7")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "G7")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 2.54)
				(name "VREF-")
				(number "H8")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 2.54)
				(name "PH0")
				(number "F8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "PH1")
				(number "F9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "PH2")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PE0")
				(number "B7")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PE1")
				(number "A8")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PE2")
				(number "D6")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PE3")
				(number "D7")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PE4")
				(number "C8")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PE5")
				(number "B9")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PE6")
				(number "E6")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PE7")
				(number "L6")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PE8")
				(number "M5")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PE9")
				(number "M4")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PE10")
				(number "J5")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PE11")
				(number "L5")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PE12")
				(number "M3")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PE13")
				(number "K5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE14")
				(number "L4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PE15")
				(number "K4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "A2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "D4")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "C3")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "C4")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "A3")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "B3")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "B4")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "A4")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PD8")
				(number "H4")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PD9")
				(number "J2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PD10")
				(number "K1")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PD11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PD12")
				(number "H3")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "PD13")
				(number "H2")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 2.54)
				(name "PD14")
				(number "J1")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 2.54)
				(name "PD15")
				(number "G3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "B8")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "C1")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "K3")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 2.54)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "L2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "L8")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 2.54)
				(name "VSSA")
				(number "J9")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "M9")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 2.54)
				(name "VDDA")
				(number "G6")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 2.54)
				(name "VLCD")
				(number "E7")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 2.54)
				(name "PA0")
				(number "K9")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 2.54)
				(name "PA1")
				(number "L9")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 2.54)
				(name "PA2")
				(number "J8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 2.54)
				(name "PA3")
				(number "H7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 2.54)
				(name "PA4")
				(number "J7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 2.54)
				(name "PA5")
				(number "M8")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 2.54)
				(name "PA6")
				(number "H6")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 2.54)
				(name "PA7")
				(number "K7")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PA8")
				(number "F3")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA9")
				(number "F1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA10")
				(number "F2")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA11")
				(number "E1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA12")
				(number "E2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA13")
				(number "E3")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "K6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "M6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB9")
				(number "C6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB10")
				(number "M2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB11")
				(number "L3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB12")
				(number "J4")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB13")
				(number "J3")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB14")
				(number "L1")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB15")
				(number "K2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PC0")
				(number "F6")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PC1")
				(number "H9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PC2")
				(number "G9")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PC3")
				(number "G8")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PC4")
				(number "L7")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PC5")
				(number "M7")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PC6")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PC7")
				(number "G1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "PC8")
				(number "G2")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 2.54)
				(name "PC9")
				(number "F4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 2.54)
				(name "PC10")
				(number "E4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 2.54)
				(name "PC11")
				(number "C2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 2.54)
				(name "PC13")
				(number "C9")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 2.54)
				(name "PC14")
				(number "D8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151V_8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151V_8-B_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151V_8-B_Hx_0_1")
		(symbol "STM32L151V_8-B_Hx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151V_8-B_HxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151V_8-B_HxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151v8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151V_8-B_HxA_0_1")
		(symbol "STM32L151V_8-B_HxA_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151V_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151V_8-B_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151V_8-B_Tx_0_1")
		(symbol "STM32L151V_8-B_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151V_8-B_TxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151V_8-B_TxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151v8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151V_8-B_TxA_0_1")
		(symbol "STM32L151V_8-B_TxA_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151ZCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L151ZCTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151ZCTx_0_1")
		(symbol "STM32L151ZCTx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151ZDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L151ZDTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151ZDTx_0_1")
		(symbol "STM32L151ZDTx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "FSMC_A10" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "FSMC_A11" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "FSMC_A12" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "FSMC_A13" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "FSMC_A14" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "FSMC_A6" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "FSMC_A7" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "FSMC_A8" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L151ZETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L151ZETx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L151ZETx_0_1")
		(symbol "STM32L151ZETx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152CCTx_0_1")
		(symbol "STM32L152CCTx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152CCUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152CCUx_0_1")
		(symbol "STM32L152CCUx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152C_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C_6-8-B_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152C_6-8-B_Tx_0_1")
		(symbol "STM32L152C_6-8-B_Tx_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152C_6-8-B_TxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C_6-8-B_TxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 16-32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152C_6-8-B_TxA_0_1")
		(symbol "STM32L152C_6-8-B_TxA_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152C_6-8-B_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C_6-8-B_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152C_6-8-B_Ux_0_1")
		(symbol "STM32L152C_6-8-B_Ux_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152C_6-8-B_UxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C_6-8-B_UxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 16-32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152C_6-8-B_UxA_0_1")
		(symbol "STM32L152C_6-8-B_UxA_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "BOOT0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152QCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32L152QCHx"
			(at 12.7 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152qc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 112 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152QCHx_0_1")
		(symbol "STM32L152QCHx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "M3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M4")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OPAMP3_VINM")
				(number "K1")
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG0")
				(number "H9")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG1")
				(number "G9")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG3")
				(number "F9")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG4")
				(number "F10")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG5")
				(number "E9")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "D9")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "C7")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "C6")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "D6")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "D5")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "E4")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "F3")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "F4")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "G3")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "G4")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "H4")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "J6")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF11")
				(number "K6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF12")
				(number "J7")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF13")
				(number "K7")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF14")
				(number "J8")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF15")
				(number "J9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152QDHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32L152QDHx"
			(at 12.7 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152qd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 112 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152QDHx_0_1")
		(symbol "STM32L152QDHx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "M3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M4")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OPAMP3_VINM")
				(number "K1")
				(alternate "OPAMP3_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG0")
				(number "H9")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "FSMC_A10" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG1")
				(number "G9")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "FSMC_A11" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "FSMC_A12" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG3")
				(number "F9")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "FSMC_A13" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG4")
				(number "F10")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "FSMC_A14" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG5")
				(number "E9")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "D9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "C7")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "C6")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "D6")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "D5")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "E4")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "F3")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "F4")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "G3")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "G4")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "H4")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "J6")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF11")
				(number "K6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF12")
				(number "J7")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "FSMC_A6" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF13")
				(number "K7")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "FSMC_A7" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF14")
				(number "J8")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "FSMC_A8" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF15")
				(number "J9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152QEHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 90.17 0)
		)
		(property "Value" "STM32L152QEHx"
			(at 12.7 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -22.86 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 111 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152QEHx_0_1")
		(symbol "STM32L152QEHx_1_1"
			(pin input line
				(at -27.94 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -27.94 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -27.94 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -27.94 68.58 0)
				(length 5.08)
				(name "AOP1_INN")
				(number "M3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin input line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "AOP2_INN")
				(number "M4")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PG0")
				(number "H9")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PG1")
				(number "G9")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PG3")
				(number "F9")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PG4")
				(number "F10")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PG5")
				(number "E9")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PG9")
				(number "D9")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "C7")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "C6")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PF0")
				(number "D6")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PF1")
				(number "D5")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PF3")
				(number "E4")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PF4")
				(number "F3")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PF5")
				(number "F4")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PF6")
				(number "G3")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PF7")
				(number "G4")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PF8")
				(number "H4")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PF9")
				(number "J6")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PF11")
				(number "K6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PF12")
				(number "J7")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PF13")
				(number "K7")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PF14")
				(number "J8")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PF15")
				(number "J9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin no_connect line
				(at -22.86 -88.9 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "K1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 27.94 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152RCTx_0_1")
		(symbol "STM32L152RCTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152RCTxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RCTxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152rc-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152RCTxA_0_1")
		(symbol "STM32L152RCTxA_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152RDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RDTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152RDTx_0_1")
		(symbol "STM32L152RDTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152RDYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RDYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die436"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die436*"
			(at 0 0 0)
		)
		(symbol "STM32L152RDYx_0_1")
		(symbol "STM32L152RDYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "C7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "D8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "F7")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H6")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E3")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C4")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "C8")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "B8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B7")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "E7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "G8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "C6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "G4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E4")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D4")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "H4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F4")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H3")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F2")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152RETx_0_1")
		(symbol "STM32L152RETx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152R_6-8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R_6-8-B_Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152R_6-8-B_Hx_0_1")
		(symbol "STM32L152R_6-8-B_Hx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152R_6-8-B_HxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R_6-8-B_HxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 16-32KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152R_6-8-B_HxA_0_1")
		(symbol "STM32L152R_6-8-B_HxA_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E1")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "B4")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "VREF+")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "D1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152R_6-8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R_6-8-B_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152R_6-8-B_Tx_0_1")
		(symbol "STM32L152R_6-8-B_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152R_6-8-B_TxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R_6-8-B_TxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32-128KB flash, 16-32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152R_6-8-B_TxA_0_1")
		(symbol "STM32L152R_6-8-B_TxA_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152UCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152UCYx"
			(at 7.62 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-63_Die427"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152uc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, WLCSP63"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die427*"
			(at 0 0 0)
		)
		(symbol "STM32L152UCYx_0_1")
		(symbol "STM32L152UCYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "E7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "F6")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "F7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "A4")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E6")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "E5")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "G7")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "G6")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "F4")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "J4")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "F1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "D1")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "E2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "B3")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "A3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "B4")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "D5")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "D7")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "D6")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "B7")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J1")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F5")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "C7")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "E4")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "G5")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H6")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "J7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "J6")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "H4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E3")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D2")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "B1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "D3")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "C3")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "J3")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "H3")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G3")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "D4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B6")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "C6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "J2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F3")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152VCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152VCHx_0_1")
		(symbol "STM32L152VCHx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152VCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152VCTx_0_1")
		(symbol "STM32L152VCTx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152VCTxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VCTxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vc-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152VCTxA_0_1")
		(symbol "STM32L152VCTxA_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152VDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VDTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152VDTx_0_1")
		(symbol "STM32L152VDTx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152VDTxX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VDTxX"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vd-x.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152VDTxX_0_1")
		(symbol "STM32L152VDTxX_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152VETx_0_1")
		(symbol "STM32L152VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152VEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32L152VEYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-104_Die437"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, WLCSP104"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die437*"
			(at 0 0 0)
		)
		(symbol "STM32L152VEYx_0_1")
		(symbol "STM32L152VEYx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 2.54)
				(name "NRST")
				(number "F7")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 2.54)
				(name "BOOT0")
				(number "A7")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "G7")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 2.54)
				(name "VREF-")
				(number "H8")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 2.54)
				(name "PH0")
				(number "F8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "PH1")
				(number "F9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "PH2")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PE0")
				(number "B7")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PE1")
				(number "A8")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PE2")
				(number "D6")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PE3")
				(number "D7")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PE4")
				(number "C8")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PE5")
				(number "B9")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PE6")
				(number "E6")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PE7")
				(number "L6")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PE8")
				(number "M5")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PE9")
				(number "M4")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PE10")
				(number "J5")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PE11")
				(number "L5")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PE12")
				(number "M3")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PE13")
				(number "K5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE14")
				(number "L4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PE15")
				(number "K4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "A2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "D4")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "C3")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "C4")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "A3")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "B3")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "B4")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "A4")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PD8")
				(number "H4")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PD9")
				(number "J2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PD10")
				(number "K1")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PD11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PD12")
				(number "H3")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "PD13")
				(number "H2")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 2.54)
				(name "PD14")
				(number "J1")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 2.54)
				(name "PD15")
				(number "G3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "B8")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "C1")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "K3")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 2.54)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "L2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "L8")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 2.54)
				(name "VSSA")
				(number "J9")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "M9")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 2.54)
				(name "VDDA")
				(number "G6")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 2.54)
				(name "VLCD")
				(number "E7")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 2.54)
				(name "PA0")
				(number "K9")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 2.54)
				(name "PA1")
				(number "L9")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 2.54)
				(name "PA2")
				(number "J8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 2.54)
				(name "PA3")
				(number "H7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 2.54)
				(name "PA4")
				(number "J7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 2.54)
				(name "PA5")
				(number "M8")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 2.54)
				(name "PA6")
				(number "H6")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 2.54)
				(name "PA7")
				(number "K7")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PA8")
				(number "F3")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA9")
				(number "F1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA10")
				(number "F2")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA11")
				(number "E1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA12")
				(number "E2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA13")
				(number "E3")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "K6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "M6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB9")
				(number "C6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB10")
				(number "M2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB11")
				(number "L3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB12")
				(number "J4")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB13")
				(number "J3")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB14")
				(number "L1")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB15")
				(number "K2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PC0")
				(number "F6")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PC1")
				(number "H9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PC2")
				(number "G9")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PC3")
				(number "G8")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PC4")
				(number "L7")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PC5")
				(number "M7")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PC6")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PC7")
				(number "G1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "PC8")
				(number "G2")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 2.54)
				(name "PC9")
				(number "F4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 2.54)
				(name "PC10")
				(number "E4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 2.54)
				(name "PC11")
				(number "C2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 2.54)
				(name "PC13")
				(number "C9")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 2.54)
				(name "PC14")
				(number "D8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152V_8-B_Hx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152V_8-B_Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152V_8-B_Hx_0_1")
		(symbol "STM32L152V_8-B_Hx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152V_8-B_HxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152V_8-B_HxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152v8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152V_8-B_HxA_0_1")
		(symbol "STM32L152V_8-B_HxA_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152V_8-B_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152V_8-B_Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 10-16KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152V_8-B_Tx_0_1")
		(symbol "STM32L152V_8-B_Tx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152V_8-B_TxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152V_8-B_TxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152v8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64-128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152V_8-B_TxA_0_1")
		(symbol "STM32L152V_8-B_TxA_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152ZCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L152ZCTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152ZCTx_0_1")
		(symbol "STM32L152ZCTx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152ZDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L152ZDTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152ZDTx_0_1")
		(symbol "STM32L152ZDTx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "FSMC_A10" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "FSMC_A11" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "FSMC_A12" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "FSMC_A13" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "FSMC_A14" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "FSMC_A6" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "FSMC_A7" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "FSMC_A8" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L152ZETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L152ZETx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L152ZETx_0_1")
		(symbol "STM32L152ZETx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162QCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32L162QCHx"
			(at 12.7 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162qc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 112 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162QCHx_0_1")
		(symbol "STM32L162QCHx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "M3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M4")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OPAMP3_VINM")
				(number "K1")
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG0")
				(number "H9")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG1")
				(number "G9")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG3")
				(number "F9")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG4")
				(number "F10")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG5")
				(number "E9")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "D9")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "C7")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "C6")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "D6")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "D5")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "E4")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "F3")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "F4")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "G3")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "G4")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "H4")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "J6")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF11")
				(number "K6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF12")
				(number "J7")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF13")
				(number "K7")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF14")
				(number "J8")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF15")
				(number "J9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162QDHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32L162QDHx"
			(at 12.7 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162qd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 112 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162QDHx_0_1")
		(symbol "STM32L162QDHx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -33.02 68.58 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "M3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M4")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin input line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "OPAMP3_VINM")
				(number "K1")
				(alternate "OPAMP3_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG0")
				(number "H9")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "FSMC_A10" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG1")
				(number "G9")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "FSMC_A11" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "FSMC_A12" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG3")
				(number "F9")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "FSMC_A13" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG4")
				(number "F10")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "FSMC_A14" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG5")
				(number "E9")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "D9")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "D8")
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "D7")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "C7")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "C6")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "D6")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "D5")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "D4")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "E4")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "F3")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "F4")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "G3")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF7")
				(number "G4")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "H4")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "J6")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF11")
				(number "K6")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF12")
				(number "J7")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "FSMC_A6" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF13")
				(number "K7")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "FSMC_A7" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF14")
				(number "J8")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "FSMC_A8" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF15")
				(number "J9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "J4")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "J5")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L162RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162RCTx_0_1")
		(symbol "STM32L162RCTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162RCTxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L162RCTxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162rc-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162RCTxA_0_1")
		(symbol "STM32L162RCTxA_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162RDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L162RDTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162RDTx_0_1")
		(symbol "STM32L162RDTx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162RDYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L162RDYx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-64_Die436"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162rd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, WLCSP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die436*"
			(at 0 0 0)
		)
		(symbol "STM32L162RDYx_0_1")
		(symbol "STM32L162RDYx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "C7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "D8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "D7")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "E8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "D6")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "F7")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "H6")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "H5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E3")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "D1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "B3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "C4")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "C8")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "B8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "B7")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "A8")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "A7")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B1")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "E7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "G8")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "C6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "F6")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "E6")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "H8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "E5")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "G4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "E4")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "D2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "D3")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "D4")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "B2")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "C3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "H4")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "F4")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "H3")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "B6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G3")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "F3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G1")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F2")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L162RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162RETx_0_1")
		(symbol "STM32L162RETx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "BOOT0")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VLCD")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162VCHx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L162VCHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162VCHx_0_1")
		(symbol "STM32L162VCHx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "H2")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "A4")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "L1")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "C11")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "C3")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "A2")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "B2")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "A1")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B1")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "C2")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "D2")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "M7")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "L7")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "M8")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "L8")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "M9")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "L9")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "M10")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "M11")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "M12")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "C8")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "B8")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "B7")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "A6")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "B6")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "A5")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "K9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "K8")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "J12")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "J10")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "H12")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "H11")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "H10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "C4")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G11")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "G12")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "D3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F11")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F12")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "J1")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "M1")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "E2")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "L2")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "M2")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "K3")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "L3")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "M3")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "K4")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "L4")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "M4")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "D11")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "C12")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "B12")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "A12")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "A11")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "A10")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "A9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "M5")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "M6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "L6")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "A7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "B5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "A3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "B3")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "L10")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "L11")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L12")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "K12")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "K10")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "H1")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "J2")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "J3")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "K2")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "K5")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "L5")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "E12")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "E11")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "E10")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "D12")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "C10")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "C1")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "D1")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "E1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162VCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L162VCTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162VCTx_0_1")
		(symbol "STM32L162VCTx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162VCTxA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L162VCTxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162vc-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162VCTxA_0_1")
		(symbol "STM32L162VCTxA_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162VDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L162VDTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162vd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162VDTx_0_1")
		(symbol "STM32L162VDTx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162VDYxX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32L162VDYxX"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-104_Die437"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162vd-x.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, WLCSP104"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die437*"
			(at 0 0 0)
		)
		(symbol "STM32L162VDYxX_0_1")
		(symbol "STM32L162VDYxX_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 2.54)
				(name "NRST")
				(number "F7")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 2.54)
				(name "BOOT0")
				(number "A7")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "G7")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 2.54)
				(name "VREF-")
				(number "H8")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 2.54)
				(name "PH0")
				(number "F8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "PH1")
				(number "F9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "PH2")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PE0")
				(number "B7")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PE1")
				(number "A8")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PE2")
				(number "D6")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PE3")
				(number "D7")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PE4")
				(number "C8")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PE5")
				(number "B9")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PE6")
				(number "E6")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PE7")
				(number "L6")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PE8")
				(number "M5")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PE9")
				(number "M4")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PE10")
				(number "J5")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PE11")
				(number "L5")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PE12")
				(number "M3")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PE13")
				(number "K5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE14")
				(number "L4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PE15")
				(number "K4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "A2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "D4")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "C3")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "C4")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "A3")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "B3")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "B4")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "A4")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PD8")
				(number "H4")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PD9")
				(number "J2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PD10")
				(number "K1")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PD11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PD12")
				(number "H3")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "PD13")
				(number "H2")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 2.54)
				(name "PD14")
				(number "J1")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 2.54)
				(name "PD15")
				(number "G3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "B8")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "C1")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "K3")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 2.54)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "L2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "L8")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 2.54)
				(name "VSSA")
				(number "J9")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "M9")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 2.54)
				(name "VDDA")
				(number "G6")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 2.54)
				(name "VLCD")
				(number "E7")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 2.54)
				(name "PA0")
				(number "K9")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 2.54)
				(name "PA1")
				(number "L9")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 2.54)
				(name "PA2")
				(number "J8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 2.54)
				(name "PA3")
				(number "H7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 2.54)
				(name "PA4")
				(number "J7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 2.54)
				(name "PA5")
				(number "M8")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 2.54)
				(name "PA6")
				(number "H6")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 2.54)
				(name "PA7")
				(number "K7")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PA8")
				(number "F3")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA9")
				(number "F1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA10")
				(number "F2")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA11")
				(number "E1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA12")
				(number "E2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA13")
				(number "E3")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "K6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "M6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB9")
				(number "C6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB10")
				(number "M2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB11")
				(number "L3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB12")
				(number "J4")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB13")
				(number "J3")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB14")
				(number "L1")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB15")
				(number "K2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PC0")
				(number "F6")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PC1")
				(number "H9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PC2")
				(number "G9")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PC3")
				(number "G8")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PC4")
				(number "L7")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PC5")
				(number "M7")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PC6")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PC7")
				(number "G1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "PC8")
				(number "G2")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 2.54)
				(name "PC9")
				(number "F4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 2.54)
				(name "PC10")
				(number "E4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 2.54)
				(name "PC11")
				(number "C2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 2.54)
				(name "PC13")
				(number "C9")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 2.54)
				(name "PC14")
				(number "D8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L162VETx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162VETx_0_1")
		(symbol "STM32L162VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "BOOT0")
				(number "94")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PH2")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162VEYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 69.85 0)
		)
		(property "Value" "STM32L162VEYx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-104_Die437"
			(at -20.32 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, WLCSP104"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*Die437*"
			(at 0 0 0)
		)
		(symbol "STM32L162VEYx_0_1")
		(symbol "STM32L162VEYx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 2.54)
				(name "NRST")
				(number "F7")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 2.54)
				(name "BOOT0")
				(number "A7")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "G7")
			)
			(pin input line
				(at -22.86 50.8 0)
				(length 2.54)
				(name "VREF-")
				(number "H8")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 2.54)
				(name "PH0")
				(number "F8")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "PH1")
				(number "F9")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 2.54)
				(name "PH2")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PE0")
				(number "B7")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PE1")
				(number "A8")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PE2")
				(number "D6")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PE3")
				(number "D7")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PE4")
				(number "C8")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PE5")
				(number "B9")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PE6")
				(number "E6")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PE7")
				(number "L6")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PE8")
				(number "M5")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PE9")
				(number "M4")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PE10")
				(number "J5")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PE11")
				(number "L5")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PE12")
				(number "M3")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PE13")
				(number "K5")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PE14")
				(number "L4")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PE15")
				(number "K4")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "A2")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "D4")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "C3")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "C4")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "A3")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "B3")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "B4")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "A4")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PD8")
				(number "H4")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PD9")
				(number "J2")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PD10")
				(number "K1")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PD11")
				(number "G4")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "PD12")
				(number "H3")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "PD13")
				(number "H2")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 2.54)
				(name "PD14")
				(number "J1")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 2.54)
				(name "PD15")
				(number "G3")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "B8")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "C1")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "E9")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "K3")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 2.54)
				(name "VSS")
				(number "A1")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "C7")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "K8")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "L2")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "M1")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "L8")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 2.54)
				(name "VSSA")
				(number "J9")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 2.54)
				(name "VDD")
				(number "M9")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 2.54)
				(name "VDDA")
				(number "G6")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 2.54)
				(name "VLCD")
				(number "E7")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 2.54)
				(name "PA0")
				(number "K9")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 2.54)
				(name "PA1")
				(number "L9")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 2.54)
				(name "PA2")
				(number "J8")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 2.54)
				(name "PA3")
				(number "H7")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 2.54)
				(name "PA4")
				(number "J7")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 2.54)
				(name "PA5")
				(number "M8")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 2.54)
				(name "PA6")
				(number "H6")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 2.54)
				(name "PA7")
				(number "K7")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PA8")
				(number "F3")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA9")
				(number "F1")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA10")
				(number "F2")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA11")
				(number "E1")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA12")
				(number "E2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA13")
				(number "E3")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA15")
				(number "B1")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "K6")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "M6")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "C5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PB8")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB9")
				(number "C6")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB10")
				(number "M2")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB11")
				(number "L3")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB12")
				(number "J4")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB13")
				(number "J3")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB14")
				(number "L1")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB15")
				(number "K2")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PC0")
				(number "F6")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PC1")
				(number "H9")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PC2")
				(number "G9")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PC3")
				(number "G8")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PC4")
				(number "L7")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PC5")
				(number "M7")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PC6")
				(number "H1")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PC7")
				(number "G1")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "PC8")
				(number "G2")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 2.54)
				(name "PC9")
				(number "F4")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 2.54)
				(name "PC10")
				(number "E4")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 2.54)
				(name "PC11")
				(number "C2")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 2.54)
				(name "PC12")
				(number "B2")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 2.54)
				(name "PC13")
				(number "C9")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 2.54)
				(name "PC14")
				(number "D8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 2.54)
				(name "PC15")
				(number "D9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162ZCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L162ZCTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 256KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162ZCTx_0_1")
		(symbol "STM32L162ZCTx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162ZDTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L162ZDTx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162zd.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 384KB flash, 48KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162ZDTx_0_1")
		(symbol "STM32L162ZDTx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
				(alternate "FSMC_A22" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "FSMC_A10" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "FSMC_A11" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "FSMC_A12" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "FSMC_A13" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "FSMC_A14" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FSMC_A15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_NE2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FSMC_NE3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FSMC_NE4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FSMC_A24" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FSMC_A25" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FSMC_A0" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FSMC_A1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FSMC_A2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FSMC_A3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FSMC_A4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FSMC_A5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "FSMC_A6" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "FSMC_A7" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "FSMC_A8" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "FSMC_A9" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FSMC_NBL0" bidirectional line)
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FSMC_NBL1" bidirectional line)
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "FSMC_A23" bidirectional line)
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "FSMC_A19" bidirectional line)
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "FSMC_A20" bidirectional line)
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "FSMC_A21" bidirectional line)
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D4" bidirectional line)
				(alternate "FSMC_DA4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D5" bidirectional line)
				(alternate "FSMC_DA5" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D6" bidirectional line)
				(alternate "FSMC_DA6" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "FSMC_D7" bidirectional line)
				(alternate "FSMC_DA7" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_D8" bidirectional line)
				(alternate "FSMC_DA8" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FSMC_D9" bidirectional line)
				(alternate "FSMC_DA9" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FSMC_D10" bidirectional line)
				(alternate "FSMC_DA10" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FSMC_D11" bidirectional line)
				(alternate "FSMC_DA11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D12" bidirectional line)
				(alternate "FSMC_DA12" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "FSMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "SDIO_D4" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "SDIO_D5" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "OPAMP3_VINP" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "OPAMP3_VINM" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "OPAMP3_VOUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "SDIO_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "SDIO_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "SDIO_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "SDIO_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SDIO_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SDIO_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SDIO_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FSMC_D2" bidirectional line)
				(alternate "FSMC_DA2" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FSMC_D3" bidirectional line)
				(alternate "FSMC_DA3" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "SDIO_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "FSMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "FSMC_NOE" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FSMC_NWE" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "FSMC_NWAIT" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "FSMC_NE1" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FSMC_D13" bidirectional line)
				(alternate "FSMC_DA13" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "FSMC_D14" bidirectional line)
				(alternate "FSMC_DA14" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FSMC_D15" bidirectional line)
				(alternate "FSMC_DA15" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "FSMC_A16" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FSMC_A17" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FSMC_A18" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FSMC_D0" bidirectional line)
				(alternate "FSMC_DA0" bidirectional line)
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "FSMC_D1" bidirectional line)
				(alternate "FSMC_DA1" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L162ZETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L162ZETx"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l162ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 512KB flash, 80KB RAM, 32 MHz, 1.65-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L162"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L162ZETx_0_1")
		(symbol "STM32L162ZETx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "BOOT0")
				(number "138")
			)
			(pin input line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
			)
			(pin input line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PH2")
				(number "106")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "ADC_IN8b" bidirectional line)
				(alternate "TS_G2_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "ADC_IN9b" bidirectional line)
				(alternate "TS_G2_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "ADC_IN10b" bidirectional line)
				(alternate "TS_G7_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "ADC_IN11b" bidirectional line)
				(alternate "TS_G7_IO6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "ADC_IN12b" bidirectional line)
				(alternate "TS_G7_IO7" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC_EXTI9" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "125")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC_EXTI11" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "127")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "128")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "129")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC_EXTI15" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "ADC_IN27" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
				(alternate "TS_G11_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "ADC_IN28" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TS_G11_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "ADC_IN29" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TS_G11_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "ADC_IN30" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TS_G11_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "ADC_IN31" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TS_G11_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "ADC_IN1b" bidirectional line)
				(alternate "TS_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "ADC_IN2b" bidirectional line)
				(alternate "TS_G3_IO5" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "ADC_IN3b" bidirectional line)
				(alternate "TS_G9_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "ADC_IN6b" bidirectional line)
				(alternate "TS_G9_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN7b" bidirectional line)
				(alternate "TS_G2_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "SYS_TRACECK" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "SYS_TRACED0" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "SYS_TRACED1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "SYS_TRACED2" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "RTC_TAMP3" bidirectional line)
				(alternate "SYS_TRACED3" bidirectional line)
				(alternate "SYS_WKUP3" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "ADC_IN22" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "ADC_IN23" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "ADC_IN24" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "ADC_IN25" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "95")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "131")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VLCD")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC_IN0" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "RTC_TAMP2" bidirectional line)
				(alternate "SYS_WKUP1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G1_IO1" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC_IN1" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G1_IO2" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC_IN2" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G1_IO3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC_IN3" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G1_IO4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC_IN4" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT1" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC_OUT2" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC_IN6" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G2_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G2_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G4_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G4_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "LCD_COM2" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G4_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "SYS_JTMS-SWDIO" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "SYS_JTCK-SWCLK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "I2S3_WS" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "SYS_JTDI" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC_IN8" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TS_G3_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC_IN9" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "SYS_V_REF_OUT" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TS_G3_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "ADC_IN0b" bidirectional line)
				(alternate "TS_G3_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "SYS_JTDO-TRACESWO" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "SYS_JTRST" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TS_G6_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TS_G6_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TS_G6_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "SYS_PVD_IN" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TS_G6_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "ADC_IN18" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "I2S2_WS" bidirectional line)
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM10_CH1" bidirectional line)
				(alternate "TS_G7_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "ADC_IN19" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_CK" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TS_G7_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "ADC_IN20" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TS_G7_IO3" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "ADC_IN21" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "I2S2_SD" bidirectional line)
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM11_CH1" bidirectional line)
				(alternate "TS_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC_IN10" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC_IN11" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC_IN12" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC_IN13" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G9_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC_IN15" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G9_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "I2S2_MCK" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "TS_G10_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "I2S3_MCK" bidirectional line)
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "TS_G10_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "TS_G10_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "TS_G10_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "I2S3_CK" bidirectional line)
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "I2S3_SD" bidirectional line)
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "RTC_OUT_ALARM" bidirectional line)
				(alternate "RTC_OUT_CALIB" bidirectional line)
				(alternate "RTC_TAMP1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "SYS_WKUP2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "I2S2_WS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM9_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "I2S2_CK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "I2S2_SD" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "TIM9_CH2" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIMX_IC1" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIMX_IC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
				(alternate "TIMX_IC3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC_EXTI15" bidirectional line)
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
				(alternate "TIMX_IC4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L100R8Tx"
		(extends "STM32L100R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L100R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 8KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L100R8TxA"
		(extends "STM32L100R_8-B_TxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L100R8TxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100r8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 8KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L100RBTx"
		(extends "STM32L100R_8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L100RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 10KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L100RBTxA"
		(extends "STM32L100R_8-B_TxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L100RBTxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l100rb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.8-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L100 Value Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151C6Tx"
		(extends "STM32L151C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151C6TxA"
		(extends "STM32L151C_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C6TxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151C6Ux"
		(extends "STM32L151C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151C6UxA"
		(extends "STM32L151C_6-8-B_UxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C6UxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151C8Tx"
		(extends "STM32L151C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151C8TxA"
		(extends "STM32L151C_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C8TxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151C8Ux"
		(extends "STM32L151C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151C8UxA"
		(extends "STM32L151C_6-8-B_UxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151C8UxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151c8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151CBTx"
		(extends "STM32L151C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151CBTxA"
		(extends "STM32L151C_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151CBTxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151cb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151CBUx"
		(extends "STM32L151C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151CBUxA"
		(extends "STM32L151C_6-8-B_UxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L151CBUxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151cb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151R6Hx"
		(extends "STM32L151R_6-8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R6Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151R6HxA"
		(extends "STM32L151R_6-8-B_HxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R6HxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151R6Tx"
		(extends "STM32L151R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151R6TxA"
		(extends "STM32L151R_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R6TxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151R8Hx"
		(extends "STM32L151R_6-8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R8Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151R8HxA"
		(extends "STM32L151R_6-8-B_HxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R8HxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151R8Tx"
		(extends "STM32L151R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151R8TxA"
		(extends "STM32L151R_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151R8TxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151r8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151RBHx"
		(extends "STM32L151R_6-8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151RBHxA"
		(extends "STM32L151R_6-8-B_HxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RBHxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151RBTx"
		(extends "STM32L151R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151RBTxA"
		(extends "STM32L151R_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L151RBTxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151rb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151V8Hx"
		(extends "STM32L151V_8-B_Hx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151V8Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151V8HxA"
		(extends "STM32L151V_8-B_HxA")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151V8HxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151v8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151V8Tx"
		(extends "STM32L151V_8-B_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151V8TxA"
		(extends "STM32L151V_8-B_TxA")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151V8TxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151v8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151VBHx"
		(extends "STM32L151V_8-B_Hx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VBHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151VBHxA"
		(extends "STM32L151V_8-B_HxA")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VBHxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151VBTx"
		(extends "STM32L151V_8-B_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L151VBTxA"
		(extends "STM32L151V_8-B_TxA")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L151VBTxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l151vb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152C6Tx"
		(extends "STM32L152C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C6Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152C6TxA"
		(extends "STM32L152C_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C6TxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152C6Ux"
		(extends "STM32L152C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C6Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152C6UxA"
		(extends "STM32L152C_6-8-B_UxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C6UxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152C8Tx"
		(extends "STM32L152C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C8Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152C8TxA"
		(extends "STM32L152C_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C8TxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152C8Ux"
		(extends "STM32L152C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C8Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152C8UxA"
		(extends "STM32L152C_6-8-B_UxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152C8UxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152c8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152CBTx"
		(extends "STM32L152C_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152CBTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152CBTxA"
		(extends "STM32L152C_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152CBTxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152cb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152CBUx"
		(extends "STM32L152C_6-8-B_Ux")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152CBUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152CBUxA"
		(extends "STM32L152C_6-8-B_UxA")
		(property "Reference" "U"
			(at -15.24 39.37 0)
		)
		(property "Value" "STM32L152CBUxA"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -38.1 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152cb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 37 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152R6Hx"
		(extends "STM32L152R_6-8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R6Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152R6HxA"
		(extends "STM32L152R_6-8-B_HxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R6HxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152R6Tx"
		(extends "STM32L152R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152R6TxA"
		(extends "STM32L152R_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R6TxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r6-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 32KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152R8Hx"
		(extends "STM32L152R_6-8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R8Hx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152R8HxA"
		(extends "STM32L152R_6-8-B_HxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R8HxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152R8Tx"
		(extends "STM32L152R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152R8TxA"
		(extends "STM32L152R_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152R8TxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152r8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152RBHx"
		(extends "STM32L152R_6-8-B_Hx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RBHx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152RBHxA"
		(extends "STM32L152R_6-8-B_HxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RBHxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152rb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 50 GPIO, TFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152RBTx"
		(extends "STM32L152R_6-8-B_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152RBTxA"
		(extends "STM32L152R_6-8-B_TxA")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L152RBTxA"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152rb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 51 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152V8Hx"
		(extends "STM32L152V_8-B_Hx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152V8Hx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152V8HxA"
		(extends "STM32L152V_8-B_HxA")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152V8HxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152v8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152V8Tx"
		(extends "STM32L152V_8-B_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152V8Tx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152v8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 10KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152V8TxA"
		(extends "STM32L152V_8-B_TxA")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152V8TxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152v8-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152VBHx"
		(extends "STM32L152V_8-B_Hx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VBHx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152VBHxA"
		(extends "STM32L152V_8-B_HxA")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VBHxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-100_7x7mm_Layout12x12_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, UFBGA100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152VBTx"
		(extends "STM32L152V_8-B_Tx")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VBTx"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 16KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L152VBTxA"
		(extends "STM32L152V_8-B_TxA")
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L152VBTxA"
			(at 10.16 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l152vb-a.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 128KB flash, 32KB RAM, 32 MHz, 1.65-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M3 STM32L1 STM32L151/152"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
