(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32L552CETxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 36.83 0)
		)
		(property "Value" "STM32L552CETxP"
			(at 10.16 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 36 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552CETxP_0_1")
		(symbol "STM32L552CETxP_1_1"
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH3")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD12")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD12")
				(number "46")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552CEUxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 36.83 0)
		)
		(property "Value" "STM32L552CEUxP"
			(at 10.16 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 36 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552CEUxP_0_1")
		(symbol "STM32L552CEUxP_1_1"
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH3")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD12")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD12")
				(number "46")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552C_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32L552C_C-E_Tx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256-512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552C_C-E_Tx_0_1")
		(symbol "STM32L552C_C-E_Tx_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552C_C-E_Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32L552C_C-E_Ux"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256-512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552C_C-E_Ux_0_1")
		(symbol "STM32L552C_C-E_Ux_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552MEYxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 52.07 0)
		)
		(property "Value" "STM32L552MEYxP"
			(at 15.24 52.07 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-81_4.36x4.07mm_Layout9x9_P0.4mm"
			(at -22.86 -50.8 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 61 GPIO, WLCSP81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.36x4.07mm*Layout9x9*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552MEYxP_0_1")
		(symbol "STM32L552MEYxP_1_1"
			(pin input line
				(at -25.4 45.72 0)
				(length 2.54)
				(name "NRST")
				(number "E9")
			)
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "G8")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "PH0")
				(number "D9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "PH1")
				(number "D8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PH3")
				(number "D7")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PG9")
				(number "D4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PG10")
				(number "C4")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PG11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PG12")
				(number "B4")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PG13")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PG14")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PG15")
				(number "C5")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PE13")
				(number "J4")
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PE14")
				(number "H4")
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PE15")
				(number "H3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "E7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "F7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC8")
				(number "F3")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "PC9")
				(number "G3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "PC11")
				(number "C3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "PC12")
				(number "B3")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 2.54)
				(name "PC14")
				(number "C9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 2.54)
				(name "PC15")
				(number "C8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -12.7 53.34 270)
				(length 2.54)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "F9")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "J8")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B5")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 2.54)
				(name "VDD12")
				(number "A8")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 2.54)
				(name "VSSA")
				(number "G9")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 2.54)
				(name "VDD12")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 53.34 270)
				(length 2.54)
				(name "VDDA")
				(number "H9")
			)
			(pin power_in line
				(at 10.16 53.34 270)
				(length 2.54)
				(name "VDDIO2")
				(number "A5")
			)
			(pin power_in line
				(at 12.7 53.34 270)
				(length 2.54)
				(name "VDDUSB")
				(number "B1")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 2.54)
				(name "PA0")
				(number "H8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA2")
				(number "G6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA5")
				(number "H6")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA7")
				(number "J7")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA8")
				(number "F4")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA10")
				(number "E3")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA13")
				(number "D2")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA15")
				(number "E4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "J5")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "E6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "C6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "D6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "C7")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB10")
				(number "J3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB11")
				(number "J2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "G1")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552MEYxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 52.07 0)
		)
		(property "Value" "STM32L552MEYxQ"
			(at 15.24 52.07 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-81_4.36x4.07mm_Layout9x9_P0.4mm"
			(at -22.86 -48.26 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 58 GPIO, WLCSP81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.36x4.07mm*Layout9x9*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552MEYxQ_0_1")
		(symbol "STM32L552MEYxQ_1_1"
			(pin input line
				(at -25.4 45.72 0)
				(length 2.54)
				(name "NRST")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "V15SMPS")
				(number "A8")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "V15SMPS")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "H3")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "G8")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "D9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "D8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH3")
				(number "D7")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PG9")
				(number "D4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PG10")
				(number "C4")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PG11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PG12")
				(number "B4")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PG13")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PG14")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PG15")
				(number "C5")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC0")
				(number "E7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC2")
				(number "F7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC8")
				(number "F3")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC9")
				(number "G3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "PC11")
				(number "C3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "PC12")
				(number "B3")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 2.54)
				(name "PC14")
				(number "C9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 2.54)
				(name "PC15")
				(number "C8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 2.54)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "F9")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B5")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSSA")
				(number "G9")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "J8")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "J2")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 2.54)
				(name "VDDA")
				(number "H9")
			)
			(pin power_in line
				(at 7.62 53.34 270)
				(length 2.54)
				(name "VDDIO2")
				(number "A5")
			)
			(pin power_in line
				(at 10.16 53.34 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "J3")
			)
			(pin power_in line
				(at 12.7 53.34 270)
				(length 2.54)
				(name "VDDUSB")
				(number "B1")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 2.54)
				(name "PA0")
				(number "H8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA2")
				(number "G6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA5")
				(number "H6")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA7")
				(number "J7")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA8")
				(number "F4")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA10")
				(number "E3")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA13")
				(number "D2")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA15")
				(number "E4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "J5")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "E6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "C6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "D6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "C7")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB10")
				(number "J4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB11")
				(number "H4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "G1")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552QEIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32L552QEIx"
			(at 15.24 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 110 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552QEIx_0_1")
		(symbol "STM32L552QEIx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "H3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M2")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "PH3")
				(number "B5")
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "M6")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "K6")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "G11")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "G9")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "F9")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "F10")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "F12")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "C7")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "M11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "M10")
				(alternate "FMC_A24" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "M9")
				(alternate "FMC_A25" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "B4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "D2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "E1")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF5")
				(number "F2")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF11")
				(number "K5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF12")
				(number "L5")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF13")
				(number "M5")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF14")
				(number "J5")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF15")
				(number "L6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PE2")
				(number "B3")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE5")
				(number "A1")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE7")
				(number "K7")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE8")
				(number "J6")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE9")
				(number "M7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE10")
				(number "J7")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE11")
				(number "L7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE12")
				(number "J8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE13")
				(number "M8")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE14")
				(number "K8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE15")
				(number "L8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D4")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D9")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L10")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J4")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "H1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "D8")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "J2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "M1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "B12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "C10")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "C11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "C6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "D5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "C5")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K10")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "F4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "F11")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "A9")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B8")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A8")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "A7")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "D7")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "J10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "M12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J12")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H11")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552QEIxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32L552QEIxP"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -30.48 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 108 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552QEIxP_0_1")
		(symbol "STM32L552QEIxP_1_1"
			(pin input line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin input line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "H3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M2")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "PH3")
				(number "B5")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "M6")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "K6")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "G11")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "G9")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "F9")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "F10")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "F12")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "C7")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "M10")
				(alternate "FMC_A24" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "M9")
				(alternate "FMC_A25" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "D2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "E1")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "F2")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF11")
				(number "K5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF12")
				(number "L5")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF13")
				(number "M5")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF14")
				(number "J5")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF15")
				(number "L6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PE2")
				(number "B3")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PE5")
				(number "A1")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE7")
				(number "K7")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE8")
				(number "J6")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE9")
				(number "M7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE10")
				(number "J7")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE11")
				(number "L7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE12")
				(number "J8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE13")
				(number "M8")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE14")
				(number "K8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE15")
				(number "L8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D9")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J4")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L10")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "H1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD12")
				(number "B4")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD12")
				(number "M11")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "D8")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "J2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "M1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "B12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "C10")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "C11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "C6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "D5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "C5")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K10")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "F4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "F11")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "A9")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B8")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A8")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "A7")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "D7")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "J10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "M12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J12")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H11")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552Q_C-E_IxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32L552Q_C-E_IxQ"
			(at 15.24 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -30.48 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552qc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256-512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 106 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552Q_C-E_IxQ_0_1")
		(symbol "STM32L552Q_C-E_IxQ_1_1"
			(pin input line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin power_in line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "V15SMPS")
				(number "B4")
			)
			(pin power_in line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "V15SMPS")
				(number "M11")
			)
			(pin power_in line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "M10")
			)
			(pin input line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "H3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M2")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PH3")
				(number "B5")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG0")
				(number "M6")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG1")
				(number "K6")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG3")
				(number "G11")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG4")
				(number "G9")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG6")
				(number "F9")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG7")
				(number "F10")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG8")
				(number "F12")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG10")
				(number "C7")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "D2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "E1")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "F2")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF11")
				(number "K5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF12")
				(number "L5")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF13")
				(number "M5")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF14")
				(number "J5")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PF15")
				(number "L6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PE2")
				(number "B3")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PE5")
				(number "A1")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE7")
				(number "K7")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE8")
				(number "J6")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE9")
				(number "M7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE10")
				(number "J7")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE11")
				(number "L7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE12")
				(number "J8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE13")
				(number "M8")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE14")
				(number "K8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PE15")
				(number "L8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D9")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H4")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J4")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "L10")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "D8")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "M9")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "J2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "M1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "B12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "C10")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "C11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "C6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "D5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "C5")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K10")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "F4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "F11")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "A9")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B8")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A8")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "A7")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "D7")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "J10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "M12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J12")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H11")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552RETxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32L552RETxP"
			(at 12.7 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 50 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552RETxP_0_1")
		(symbol "STM32L552RETxP_1_1"
			(pin input line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PH3")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD12")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD12")
				(number "62")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "26")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "27")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "54")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "55")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "56")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "58")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "60")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "61")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "29")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552RETxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "STM32L552RETxQ"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -20.32 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 47 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552RETxQ_0_1")
		(symbol "STM32L552RETxQ_1_1"
			(pin input line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin power_in line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "V15SMPS")
				(number "32")
			)
			(pin power_in line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "V15SMPS")
				(number "63")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PH3")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "62")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "30")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "28")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "27")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552R_C-E_Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L552R_C-E_Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256-512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552R_C-E_Tx_0_1")
		(symbol "STM32L552R_C-E_Tx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L552VETx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552VETx_0_1")
		(symbol "STM32L552VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 55.88 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH3")
				(number "94")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552V_C-E_TxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 64.77 0)
		)
		(property "Value" "STM32L552V_C-E_TxQ"
			(at 12.7 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -22.86 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256-512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 79 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552V_C-E_TxQ_0_1")
		(symbol "STM32L552V_C-E_TxQ_1_1"
			(pin input line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin power_in line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "V15SMPS")
				(number "50")
			)
			(pin power_in line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "V15SMPS")
				(number "99")
			)
			(pin power_in line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "47")
			)
			(pin input line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PH3")
				(number "94")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "35")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "36")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "37")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "38")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "39")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "40")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PE13")
				(number "41")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "42")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "43")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 68.58 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "98")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 68.58 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "46")
			)
			(pin power_in line
				(at 10.16 68.58 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA0")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA1")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA2")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA4")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA5")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA6")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PA7")
				(number "31")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PB10")
				(number "44")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PB11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552ZETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L552ZETx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552ZETx_0_1")
		(symbol "STM32L552ZETx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH3")
				(number "138")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FMC_A24" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FMC_A25" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "95")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "131")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552Z_C-E_TxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 87.63 0)
		)
		(property "Value" "STM32L552Z_C-E_TxQ"
			(at 20.32 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -30.48 -83.82 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256-512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 111 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L552Z_C-E_TxQ_0_1")
		(symbol "STM32L552Z_C-E_TxQ_1_1"
			(pin input line
				(at -35.56 81.28 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin power_in line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "V15SMPS")
				(number "72")
			)
			(pin power_in line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "V15SMPS")
				(number "143")
			)
			(pin power_in line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "69")
			)
			(pin input line
				(at -35.56 68.58 0)
				(length 5.08)
				(name "VREF+")
				(number "31")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PH3")
				(number "137")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PG0")
				(number "53")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PG1")
				(number "54")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "126")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "127")
				(alternate "FMC_A24" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "128")
				(alternate "FMC_A25" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "131")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "46")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "47")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "140")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "141")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "55")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "56")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "60")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "61")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "62")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "63")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "64")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -17.78 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "59")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "129")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "142")
			)
			(pin power_in line
				(at -2.54 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "58")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 0 -88.9 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 2.54 -88.9 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "70")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "32")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDDIO2")
				(number "95")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDIO2")
				(number "130")
			)
			(pin power_in line
				(at 15.24 91.44 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "68")
			)
			(pin power_in line
				(at 17.78 91.44 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "33")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "34")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "35")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "36")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "39")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "40")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "41")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "42")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "43")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "44")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "45")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB3")
				(number "132")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB4")
				(number "133")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "134")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "136")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "138")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "139")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "66")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562CETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32L562CETx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562CETx_0_1")
		(symbol "STM32L562CETx_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562CETxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 36.83 0)
		)
		(property "Value" "STM32L562CETxP"
			(at 10.16 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -15.24 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 36 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562CETxP_0_1")
		(symbol "STM32L562CETxP_1_1"
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH3")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD12")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD12")
				(number "46")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562CEUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32L562CEUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562CEUx_0_1")
		(symbol "STM32L562CEUx_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PH3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562CEUxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 36.83 0)
		)
		(property "Value" "STM32L562CEUxP"
			(at 10.16 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -15.24 -33.02 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 36 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562CEUxP_0_1")
		(symbol "STM32L562CEUxP_1_1"
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PH3")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD12")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD12")
				(number "46")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562MEYxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 52.07 0)
		)
		(property "Value" "STM32L562MEYxP"
			(at 15.24 52.07 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-81_4.36x4.07mm_Layout9x9_P0.4mm"
			(at -22.86 -50.8 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 61 GPIO, WLCSP81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.36x4.07mm*Layout9x9*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562MEYxP_0_1")
		(symbol "STM32L562MEYxP_1_1"
			(pin input line
				(at -25.4 45.72 0)
				(length 2.54)
				(name "NRST")
				(number "E9")
			)
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "VREF+")
				(number "G8")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "PH0")
				(number "D9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "PH1")
				(number "D8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "PH3")
				(number "D7")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PG9")
				(number "D4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PG10")
				(number "C4")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "PG11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PG12")
				(number "B4")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PG13")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PG14")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PG15")
				(number "C5")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PE13")
				(number "J4")
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PE14")
				(number "H4")
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "PE15")
				(number "H3")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC0")
				(number "E7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC2")
				(number "F7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC8")
				(number "F3")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "PC9")
				(number "G3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "PC11")
				(number "C3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "PC12")
				(number "B3")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 2.54)
				(name "PC14")
				(number "C9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 2.54)
				(name "PC15")
				(number "C8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -12.7 53.34 270)
				(length 2.54)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "F9")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "J8")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B5")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 2.54)
				(name "VDD12")
				(number "A8")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 2.54)
				(name "VSSA")
				(number "G9")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 2.54)
				(name "VDD12")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 53.34 270)
				(length 2.54)
				(name "VDDA")
				(number "H9")
			)
			(pin power_in line
				(at 10.16 53.34 270)
				(length 2.54)
				(name "VDDIO2")
				(number "A5")
			)
			(pin power_in line
				(at 12.7 53.34 270)
				(length 2.54)
				(name "VDDUSB")
				(number "B1")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 2.54)
				(name "PA0")
				(number "H8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA2")
				(number "G6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA5")
				(number "H6")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA7")
				(number "J7")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA8")
				(number "F4")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA10")
				(number "E3")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA13")
				(number "D2")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA15")
				(number "E4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "J5")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "E6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "C6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "D6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "C7")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB10")
				(number "J3")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB11")
				(number "J2")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "G1")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562MEYxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 52.07 0)
		)
		(property "Value" "STM32L562MEYxQ"
			(at 15.24 52.07 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-81_4.36x4.07mm_Layout9x9_P0.4mm"
			(at -22.86 -48.26 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562me.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 58 GPIO, WLCSP81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*4.36x4.07mm*Layout9x9*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562MEYxQ_0_1")
		(symbol "STM32L562MEYxQ_1_1"
			(pin input line
				(at -25.4 45.72 0)
				(length 2.54)
				(name "NRST")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "V15SMPS")
				(number "A8")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "V15SMPS")
				(number "J1")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "H3")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "VREF+")
				(number "G8")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "PH0")
				(number "D9")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "PH1")
				(number "D8")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "PH3")
				(number "D7")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "PG9")
				(number "D4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "PG10")
				(number "C4")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "PG11")
				(number "E5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "PG12")
				(number "B4")
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "PG13")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "PG14")
				(number "D5")
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "PG15")
				(number "C5")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "PD2")
				(number "A3")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "PC0")
				(number "E7")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "PC1")
				(number "F8")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "PC2")
				(number "F7")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "PC3")
				(number "G7")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "PC4")
				(number "G4")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PC6")
				(number "E1")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PC7")
				(number "E2")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PC8")
				(number "F3")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PC9")
				(number "G3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "PC10")
				(number "A2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "PC11")
				(number "C3")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "PC12")
				(number "B3")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "PC13")
				(number "B7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 2.54)
				(name "PC14")
				(number "C9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 2.54)
				(name "PC15")
				(number "C8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 2.54)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "A9")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "F9")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "VSS")
				(number "B2")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B5")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "B8")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "E8")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "H2")
			)
			(pin passive line
				(at -2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "H1")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "VSSA")
				(number "G9")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 2.54)
				(name "VDD")
				(number "J8")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "J2")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 2.54)
				(name "VDDA")
				(number "H9")
			)
			(pin power_in line
				(at 7.62 53.34 270)
				(length 2.54)
				(name "VDDIO2")
				(number "A5")
			)
			(pin power_in line
				(at 10.16 53.34 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "J3")
			)
			(pin power_in line
				(at 12.7 53.34 270)
				(length 2.54)
				(name "VDDUSB")
				(number "B1")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 2.54)
				(name "PA0")
				(number "H8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "PA1")
				(number "F6")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "PA2")
				(number "G6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "PA3")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PA4")
				(number "H7")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "PA5")
				(number "H6")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "PA6")
				(number "G5")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "PA7")
				(number "J7")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "PA8")
				(number "F4")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "PA9")
				(number "D1")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "PA10")
				(number "E3")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PA11")
				(number "C1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "PA12")
				(number "C2")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "PA13")
				(number "D2")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "PA14")
				(number "D3")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "PA15")
				(number "E4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "J6")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "J5")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "E6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "PB6")
				(number "C6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB7")
				(number "D6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PB8")
				(number "C7")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "PB9")
				(number "A7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB10")
				(number "J4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PB11")
				(number "H4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PB12")
				(number "G2")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "F2")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "G1")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "F1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562QEIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 90.17 0)
		)
		(property "Value" "STM32L562QEIx"
			(at 15.24 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -27.94 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 110 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562QEIx_0_1")
		(symbol "STM32L562QEIx_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin input line
				(at -33.02 78.74 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 73.66 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "H3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 71.12 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M2")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 60.96 0)
				(length 5.08)
				(name "PH3")
				(number "B5")
			)
			(pin bidirectional line
				(at -33.02 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "M6")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "K6")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "G11")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "G9")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "F9")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "F10")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "F12")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "C7")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG11")
				(number "M11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "M10")
				(alternate "FMC_A24" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "M9")
				(alternate "FMC_A25" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "B4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "D2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "E1")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PF5")
				(number "F2")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF11")
				(number "K5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF12")
				(number "L5")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF13")
				(number "M5")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF14")
				(number "J5")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF15")
				(number "L6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PE2")
				(number "B3")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PE5")
				(number "A1")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PE7")
				(number "K7")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PE8")
				(number "J6")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PE9")
				(number "M7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "PE10")
				(number "J7")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE11")
				(number "L7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE12")
				(number "J8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE13")
				(number "M8")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE14")
				(number "K8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE15")
				(number "L8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D4")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D9")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L10")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J4")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "H1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "D8")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "J2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "M1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "B12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "C10")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "C11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "C6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "D5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "C5")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K10")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "F4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "F11")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "A9")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B8")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A8")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "A7")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "D7")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "J10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "M12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J12")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H11")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562QEIxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32L562QEIxP"
			(at 17.78 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -30.48 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 108 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562QEIxP_0_1")
		(symbol "STM32L562QEIxP_1_1"
			(pin input line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin input line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "H3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M2")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "PH3")
				(number "B5")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PG0")
				(number "M6")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PG1")
				(number "K6")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG3")
				(number "G11")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG4")
				(number "G9")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG6")
				(number "F9")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG7")
				(number "F10")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG8")
				(number "F12")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG10")
				(number "C7")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG13")
				(number "M10")
				(alternate "FMC_A24" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG14")
				(number "M9")
				(alternate "FMC_A25" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "D2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "E1")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "F2")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF11")
				(number "K5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF12")
				(number "L5")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF13")
				(number "M5")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF14")
				(number "J5")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF15")
				(number "L6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PE2")
				(number "B3")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PE5")
				(number "A1")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE7")
				(number "K7")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE8")
				(number "J6")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE9")
				(number "M7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE10")
				(number "J7")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE11")
				(number "L7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE12")
				(number "J8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE13")
				(number "M8")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE14")
				(number "K8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE15")
				(number "L8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D9")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J4")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H4")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L10")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "H1")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD12")
				(number "B4")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD12")
				(number "M11")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "D8")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "J2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "M1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "B12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "C10")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "C11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "C6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "D5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "C5")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K10")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "F4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "F11")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "A9")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B8")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A8")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "A7")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "D7")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "J10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "M12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J12")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H11")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562QEIxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32L562QEIxQ"
			(at 15.24 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -30.48 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 106 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562QEIxQ_0_1")
		(symbol "STM32L562QEIxQ_1_1"
			(pin input line
				(at -35.56 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "G2")
			)
			(pin power_in line
				(at -35.56 78.74 0)
				(length 5.08)
				(name "V15SMPS")
				(number "B4")
			)
			(pin power_in line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "V15SMPS")
				(number "M11")
			)
			(pin power_in line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "M10")
			)
			(pin input line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "VREF+")
				(number "J1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 5.08)
				(name "OPAMP1_VINM")
				(number "H3")
				(alternate "OPAMP1_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "OPAMP2_VINM")
				(number "M2")
				(alternate "OPAMP2_VINM" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PH0")
				(number "F1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 5.08)
				(name "PH1")
				(number "G1")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PH3")
				(number "B5")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG0")
				(number "M6")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG1")
				(number "K6")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG2")
				(number "G10")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG3")
				(number "G11")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG4")
				(number "G9")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG5")
				(number "G12")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG6")
				(number "F9")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG7")
				(number "F10")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG8")
				(number "F12")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG9")
				(number "B7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG10")
				(number "C7")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PG12")
				(number "A6")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PF0")
				(number "D2")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF1")
				(number "E2")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF2")
				(number "E1")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF3")
				(number "D3")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF4")
				(number "E3")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF5")
				(number "F2")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF11")
				(number "K5")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF12")
				(number "L5")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF13")
				(number "M5")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF14")
				(number "J5")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PF15")
				(number "L6")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PE0")
				(number "C4")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PE1")
				(number "A3")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PE2")
				(number "B3")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PE3")
				(number "A2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PE4")
				(number "B2")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "PE5")
				(number "A1")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE6")
				(number "C2")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE7")
				(number "K7")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE8")
				(number "J6")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE9")
				(number "M7")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE10")
				(number "J7")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE11")
				(number "L7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE12")
				(number "J8")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE13")
				(number "M8")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE14")
				(number "K8")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PE15")
				(number "L8")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D4")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "D9")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "F7")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "G6")
			)
			(pin power_in line
				(at -2.54 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "E4")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E9")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H4")
			)
			(pin passive line
				(at -2.54 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H9")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J4")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "H1")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "J9")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "L10")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "K1")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "D8")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "M9")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "A12")
			)
			(pin bidirectional line
				(at 35.56 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "J2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "G4")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "K2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "L1")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "L3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "M1")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "L2")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "K3")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "D12")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "D10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "D11")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "C12")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "B12")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "C10")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "C11")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "A11")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "M4")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "L4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "K4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "C6")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "B6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "D6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "A5")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "D5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "C5")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "A4")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "K9")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "L9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "L11")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "K10")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "K11")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "K12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "H2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "G3")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "F3")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "F4")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "M3")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "J3")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "F11")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "E10")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "E12")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "E11")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "B11")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "A10")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "B10")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "C3")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "C1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "D1")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "C9")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "B9")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "A9")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "C8")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "B8")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "A8")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "A7")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "D7")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "L12")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "J10")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "M12")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "J11")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "J12")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "H11")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "H10")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "H12")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562RETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L562RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562RETx_0_1")
		(symbol "STM32L562RETx_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PH3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562RETxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "STM32L562RETxP"
			(at 12.7 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -17.78 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 50 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562RETxP_0_1")
		(symbol "STM32L562RETxP_1_1"
			(pin input line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "PH3")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD12")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD12")
				(number "62")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "25")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "26")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "27")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "54")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "55")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "56")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "57")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "58")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "60")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "61")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "28")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "29")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562RETxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "STM32L562RETxQ"
			(at 10.16 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -20.32 -40.64 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 47 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562RETxQ_0_1")
		(symbol "STM32L562RETxQ_1_1"
			(pin input line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "NRST")
				(number "7")
			)
			(pin power_in line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "V15SMPS")
				(number "32")
			)
			(pin power_in line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "V15SMPS")
				(number "63")
			)
			(pin power_in line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "VLXSMPS")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PH0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PH1")
				(number "6")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PH3")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "62")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSSMPS")
				(number "30")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDSMPS")
				(number "28")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "25")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "26")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "27")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562VETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 69.85 0)
		)
		(property "Value" "STM32L562VETx"
			(at 12.7 69.85 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -17.78 -66.04 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 83 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562VETx_0_1")
		(symbol "STM32L562VETx_1_1"
			(pin input line
				(at -22.86 63.5 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin input line
				(at -22.86 58.42 0)
				(length 5.08)
				(name "VREF+")
				(number "21")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -22.86 55.88 0)
				(length 5.08)
				(name "VREF-")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PH3")
				(number "94")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PE1")
				(number "98")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PE7")
				(number "38")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PE8")
				(number "39")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PE9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PE10")
				(number "41")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PE11")
				(number "42")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PE12")
				(number "43")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PE13")
				(number "44")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PE14")
				(number "45")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PE15")
				(number "46")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "50")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -71.12 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 22.86 63.5 180)
				(length 5.08)
				(name "PA0")
				(number "23")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 5.08)
				(name "PA1")
				(number "24")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 5.08)
				(name "PA2")
				(number "25")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 5.08)
				(name "PA3")
				(number "26")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 5.08)
				(name "PA4")
				(number "29")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 5.08)
				(name "PA5")
				(number "30")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PA6")
				(number "31")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PA7")
				(number "32")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PB0")
				(number "35")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PB1")
				(number "36")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PB2")
				(number "37")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PB10")
				(number "47")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PB11")
				(number "48")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PB12")
				(number "51")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PC4")
				(number "33")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PC5")
				(number "34")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562VETxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 64.77 0)
		)
		(property "Value" "STM32L562VETxQ"
			(at 12.7 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -22.86 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 79 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562VETxQ_0_1")
		(symbol "STM32L562VETxQ_1_1"
			(pin input line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "NRST")
				(number "14")
			)
			(pin power_in line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "V15SMPS")
				(number "50")
			)
			(pin power_in line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "V15SMPS")
				(number "99")
			)
			(pin power_in line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "47")
			)
			(pin input line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "VREF+")
				(number "20")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PH0")
				(number "12")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PH1")
				(number "13")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PH3")
				(number "94")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PE0")
				(number "97")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PE7")
				(number "35")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PE8")
				(number "36")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PE9")
				(number "37")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PE10")
				(number "38")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PE11")
				(number "39")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PE12")
				(number "40")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PE13")
				(number "41")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PE14")
				(number "42")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PE15")
				(number "43")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PD0")
				(number "81")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PD1")
				(number "82")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PD2")
				(number "83")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PD3")
				(number "84")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PD4")
				(number "85")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PD5")
				(number "86")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PD6")
				(number "87")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PD7")
				(number "88")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PD8")
				(number "55")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PD9")
				(number "56")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PD10")
				(number "57")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PD11")
				(number "58")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "PD12")
				(number "59")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PD13")
				(number "60")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 5.08)
				(name "PD14")
				(number "61")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 5.08)
				(name "PD15")
				(number "62")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin power_in line
				(at -10.16 68.58 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "98")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 5.08)
				(name "VSSA")
				(number "19")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 5.08)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "48")
			)
			(pin power_in line
				(at 5.08 68.58 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 7.62 68.58 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "46")
			)
			(pin power_in line
				(at 10.16 68.58 270)
				(length 5.08)
				(name "VDDUSB")
				(number "73")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PA0")
				(number "22")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PA1")
				(number "23")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PA2")
				(number "24")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PA3")
				(number "25")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PA4")
				(number "28")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PA5")
				(number "29")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PA6")
				(number "30")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PA7")
				(number "31")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PA8")
				(number "67")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PA9")
				(number "68")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PA10")
				(number "69")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PA11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PA12")
				(number "71")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PA13")
				(number "72")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PA14")
				(number "76")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PA15")
				(number "77")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PB0")
				(number "32")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PB1")
				(number "33")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PB2")
				(number "34")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PB3")
				(number "89")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PB4")
				(number "90")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PB5")
				(number "91")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PB6")
				(number "92")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PB7")
				(number "93")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PB8")
				(number "95")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PB9")
				(number "96")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PB10")
				(number "44")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PB11")
				(number "45")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PB13")
				(number "52")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PB14")
				(number "53")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PB15")
				(number "54")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PC0")
				(number "15")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PC1")
				(number "16")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PC2")
				(number "17")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PC3")
				(number "18")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PC6")
				(number "63")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PC7")
				(number "64")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PC8")
				(number "65")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PC9")
				(number "66")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PC10")
				(number "78")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PC11")
				(number "79")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PC12")
				(number "80")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562ZETx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 90.17 0)
		)
		(property "Value" "STM32L562ZETx"
			(at 20.32 90.17 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -25.4 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 115 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562ZETx_0_1")
		(symbol "STM32L562ZETx_1_1"
			(pin input line
				(at -30.48 83.82 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin input line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "VREF+")
				(number "32")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin input line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "VREF-")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PH3")
				(number "138")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PG0")
				(number "56")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PG1")
				(number "57")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PG11")
				(number "126")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PG12")
				(number "127")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PG13")
				(number "128")
				(alternate "FMC_A24" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PG14")
				(number "129")
				(alternate "FMC_A25" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PG15")
				(number "132")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PF11")
				(number "49")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PF12")
				(number "50")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PF13")
				(number "53")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PF14")
				(number "54")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PF15")
				(number "55")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PE0")
				(number "141")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PE1")
				(number "142")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE7")
				(number "58")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE8")
				(number "59")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE9")
				(number "60")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PE10")
				(number "63")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PE11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "PE12")
				(number "65")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "PE13")
				(number "66")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "PE14")
				(number "67")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "PE15")
				(number "68")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -15.24 93.98 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -12.7 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -10.16 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at 0 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "130")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "143")
			)
			(pin power_in line
				(at 0 -93.98 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "38")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "61")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at 0 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 2.54 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 2.54 -93.98 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 7.62 93.98 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 10.16 93.98 270)
				(length 5.08)
				(name "VDDA")
				(number "33")
			)
			(pin power_in line
				(at 12.7 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "95")
			)
			(pin power_in line
				(at 15.24 93.98 270)
				(length 5.08)
				(name "VDDIO2")
				(number "131")
			)
			(pin power_in line
				(at 17.78 93.98 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 30.48 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "34")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PA1")
				(number "35")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PA2")
				(number "36")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "37")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "40")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "41")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "42")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PA7")
				(number "43")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "46")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "47")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "48")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PB3")
				(number "133")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "134")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "135")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "136")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PB7")
				(number "137")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "139")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "140")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "69")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "70")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "73")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PC4")
				(number "44")
				(alternate "ADC1_IN13" bidirectional line)
				(alternate "ADC2_IN13" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PC5")
				(number "45")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "ADC2_IN14" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "TAMP_OUT5" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 30.48 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L562ZETxQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 87.63 0)
		)
		(property "Value" "STM32L562ZETxQ"
			(at 20.32 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -30.48 -83.82 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l562ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 111 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32L562ZETxQ_0_1")
		(symbol "STM32L562ZETxQ_1_1"
			(pin input line
				(at -35.56 81.28 0)
				(length 5.08)
				(name "NRST")
				(number "25")
			)
			(pin power_in line
				(at -35.56 76.2 0)
				(length 5.08)
				(name "V15SMPS")
				(number "72")
			)
			(pin power_in line
				(at -35.56 73.66 0)
				(length 5.08)
				(name "V15SMPS")
				(number "143")
			)
			(pin power_in line
				(at -35.56 71.12 0)
				(length 5.08)
				(name "VLXSMPS")
				(number "69")
			)
			(pin input line
				(at -35.56 68.58 0)
				(length 5.08)
				(name "VREF+")
				(number "31")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 5.08)
				(name "PH0")
				(number "23")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 60.96 0)
				(length 5.08)
				(name "PH1")
				(number "24")
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 5.08)
				(name "PH3")
				(number "137")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 5.08)
				(name "PG0")
				(number "53")
				(alternate "FMC_A10" bidirectional line)
				(alternate "TSC_G8_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 5.08)
				(name "PG1")
				(number "54")
				(alternate "FMC_A11" bidirectional line)
				(alternate "TSC_G8_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 5.08)
				(name "PG2")
				(number "87")
				(alternate "FMC_A12" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 5.08)
				(name "PG3")
				(number "88")
				(alternate "FMC_A13" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 5.08)
				(name "PG4")
				(number "89")
				(alternate "FMC_A14" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 5.08)
				(name "PG5")
				(number "90")
				(alternate "FMC_A15" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 5.08)
				(name "PG6")
				(number "91")
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 5.08)
				(name "PG7")
				(number "92")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_INT" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "PG8")
				(number "93")
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "PG9")
				(number "124")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE2" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "PG10")
				(number "125")
				(alternate "FMC_NE3" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PG12")
				(number "126")
				(alternate "FMC_NE4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PG13")
				(number "127")
				(alternate "FMC_A24" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PG14")
				(number "128")
				(alternate "FMC_A25" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PG15")
				(number "131")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PF0")
				(number "10")
				(alternate "FMC_A0" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PF1")
				(number "11")
				(alternate "FMC_A1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PF2")
				(number "12")
				(alternate "FMC_A2" bidirectional line)
				(alternate "I2C2_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PF3")
				(number "13")
				(alternate "FMC_A3" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PF4")
				(number "14")
				(alternate "FMC_A4" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PF5")
				(number "15")
				(alternate "FMC_A5" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PF6")
				(number "18")
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM5_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PF7")
				(number "19")
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TAMP_IN6" bidirectional line)
				(alternate "TAMP_OUT3" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PF8")
				(number "20")
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TAMP_IN7" bidirectional line)
				(alternate "TAMP_OUT8" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PF9")
				(number "21")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TAMP_IN8" bidirectional line)
				(alternate "TAMP_OUT7" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PF10")
				(number "22")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_D3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PF11")
				(number "46")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PF12")
				(number "47")
				(alternate "FMC_A6" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PF13")
				(number "50")
				(alternate "FMC_A7" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PF14")
				(number "51")
				(alternate "FMC_A8" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "TSC_G8_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "PF15")
				(number "52")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_A9" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "TSC_G8_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "PE0")
				(number "140")
				(alternate "FMC_NBL0" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 5.08)
				(name "PE1")
				(number "141")
				(alternate "FMC_NBL1" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 5.08)
				(name "PE2")
				(number "1")
				(alternate "DEBUG_TRACECLK" bidirectional line)
				(alternate "FMC_A23" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "PE3")
				(number "2")
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "FMC_A19" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "PE4")
				(number "3")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "FMC_A20" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 5.08)
				(name "PE5")
				(number "4")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "FMC_A21" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 5.08)
				(name "PE6")
				(number "5")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "FMC_A22" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TAMP_OUT6" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 5.08)
				(name "PE7")
				(number "55")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "FMC_D4" bidirectional line)
				(alternate "FMC_DA4" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 5.08)
				(name "PE8")
				(number "56")
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "FMC_D5" bidirectional line)
				(alternate "FMC_DA5" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 5.08)
				(name "PE9")
				(number "57")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FMC_D6" bidirectional line)
				(alternate "FMC_DA6" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 5.08)
				(name "PE10")
				(number "60")
				(alternate "FMC_D7" bidirectional line)
				(alternate "FMC_DA7" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 5.08)
				(name "PE11")
				(number "61")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_D8" bidirectional line)
				(alternate "FMC_DA8" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 5.08)
				(name "PE12")
				(number "62")
				(alternate "FMC_D9" bidirectional line)
				(alternate "FMC_DA9" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 5.08)
				(name "PE13")
				(number "63")
				(alternate "FMC_D10" bidirectional line)
				(alternate "FMC_DA10" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 5.08)
				(name "PE14")
				(number "64")
				(alternate "FMC_D11" bidirectional line)
				(alternate "FMC_DA11" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at -35.56 -68.58 0)
				(length 5.08)
				(name "PE15")
				(number "65")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D12" bidirectional line)
				(alternate "FMC_DA12" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
			)
			(pin power_in line
				(at -17.78 91.44 270)
				(length 5.08)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at -15.24 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -12.7 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "59")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "73")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "84")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "107")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "120")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "129")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "142")
			)
			(pin power_in line
				(at -2.54 -88.9 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "58")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "71")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "83")
			)
			(pin passive line
				(at -2.54 -88.9 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "94")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "108")
			)
			(pin power_in line
				(at 0 -88.9 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "121")
			)
			(pin power_in line
				(at 2.54 -88.9 90)
				(length 5.08)
				(name "VSSSMPS")
				(number "70")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "144")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "32")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDDIO2")
				(number "95")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDIO2")
				(number "130")
			)
			(pin power_in line
				(at 15.24 91.44 270)
				(length 5.08)
				(name "VDDSMPS")
				(number "68")
			)
			(pin power_in line
				(at 17.78 91.44 270)
				(length 5.08)
				(name "VDDUSB")
				(number "106")
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 5.08)
				(name "PA0")
				(number "33")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "ADC2_IN5" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TAMP_OUT1" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM5_CH1" bidirectional line)
				(alternate "TIM8_ETR" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 5.08)
				(name "PA1")
				(number "34")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "ADC2_IN6" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TAMP_OUT4" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "TIM5_CH2" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 5.08)
				(name "PA2")
				(number "35")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "ADC2_IN7" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TIM5_CH3" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 5.08)
				(name "PA3")
				(number "36")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "ADC2_IN8" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TIM5_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 5.08)
				(name "PA4")
				(number "39")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "ADC2_IN9" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 5.08)
				(name "PA5")
				(number "40")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "ADC2_IN10" bidirectional line)
				(alternate "DAC1_OUT2" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 5.08)
				(name "PA6")
				(number "41")
				(alternate "ADC1_IN11" bidirectional line)
				(alternate "ADC2_IN11" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "OCTOSPI1_IO3" bidirectional line)
				(alternate "OPAMP2_VINP" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 5.08)
				(name "PA7")
				(number "42")
				(alternate "ADC1_IN12" bidirectional line)
				(alternate "ADC2_IN12" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "OCTOSPI1_IO2" bidirectional line)
				(alternate "OPAMP2_VINM" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 5.08)
				(name "PA8")
				(number "100")
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "SAI1_CK2" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 5.08)
				(name "PA9")
				(number "101")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 5.08)
				(name "PA10")
				(number "102")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 5.08)
				(name "PA11")
				(number "103")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 5.08)
				(name "PA12")
				(number "104")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 5.08)
				(name "PA13")
				(number "105")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 5.08)
				(name "PA14")
				(number "109")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 5.08)
				(name "PA15")
				(number "110")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SAI2_FS_B" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "UART4_DE" bidirectional line)
				(alternate "UART4_RTS" bidirectional line)
				(alternate "UCPD1_CC1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 5.08)
				(name "PB0")
				(number "43")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "ADC2_IN15" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO1" bidirectional line)
				(alternate "OPAMP2_VOUT" bidirectional line)
				(alternate "SAI1_EXTCLK" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 5.08)
				(name "PB1")
				(number "44")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "ADC2_IN16" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "OCTOSPI1_IO0" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 5.08)
				(name "PB2")
				(number "45")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "I2C3_SMBA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "OCTOSPI1_DQS" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
				(alternate "UCPD1_FRSTX1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 5.08)
				(name "PB3")
				(number "132")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "SAI1_SCK_B" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 5.08)
				(name "PB4")
				(number "133")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "DEBUG_JTRST" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "SAI1_MCLK_B" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM17_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "UART5_DE" bidirectional line)
				(alternate "UART5_RTS" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USART1_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PB5")
				(number "134")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C1_SMBA" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCLK" bidirectional line)
				(alternate "SAI1_SD_B" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "UART5_CTS" bidirectional line)
				(alternate "UCPD1_DBCC1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PB6")
				(number "135")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "SAI1_FS_B" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PB7")
				(number "136")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "FMC_NL" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TIM17_CH1N" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TIM8_BKIN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "UART4_CTS" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PB8")
				(number "138")
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "SAI1_CK1" bidirectional line)
				(alternate "SAI1_MCLK_A" bidirectional line)
				(alternate "SDMMC1_CKIN" bidirectional line)
				(alternate "SDMMC1_D4" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PB9")
				(number "139")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "SAI1_D2" bidirectional line)
				(alternate "SAI1_FS_A" bidirectional line)
				(alternate "SDMMC1_CDIR" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM17_CH1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PB10")
				(number "66")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_CLK" bidirectional line)
				(alternate "SAI1_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PB11")
				(number "67")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PB13")
				(number "74")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PB14")
				(number "75")
				(alternate "DFSDM1_DATIN2" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM8_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "UCPD1_DBCC2" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "76")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "DFSDM1_CKIN2" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM8_CH3N" bidirectional line)
				(alternate "UCPD1_CC2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "26")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "ADC2_IN1" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "SDMMC1_D5" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PC1")
				(number "27")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "ADC2_IN2" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_OUT" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "28")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "ADC2_IN3" bidirectional line)
				(alternate "DFSDM1_CKOUT" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "29")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "ADC2_IN4" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_OUT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PC6")
				(number "96")
				(alternate "DFSDM1_CKIN3" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "SDMMC1_D0DIR" bidirectional line)
				(alternate "SDMMC1_D6" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TIM8_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PC7")
				(number "97")
				(alternate "DFSDM1_DATIN3" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D123DIR" bidirectional line)
				(alternate "SDMMC1_D7" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TIM8_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PC8")
				(number "98")
				(alternate "SDMMC1_D0" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TIM8_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PC9")
				(number "99")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "DEBUG_TRACED0" bidirectional line)
				(alternate "SAI2_EXTCLK" bidirectional line)
				(alternate "SDMMC1_D1" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TIM8_BKIN2" bidirectional line)
				(alternate "TIM8_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PC10")
				(number "111")
				(alternate "DEBUG_TRACED1" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SAI2_SCK_B" bidirectional line)
				(alternate "SDMMC1_D2" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "UART4_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PC11")
				(number "112")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "OCTOSPI1_NCS" bidirectional line)
				(alternate "SAI2_MCLK_B" bidirectional line)
				(alternate "SDMMC1_D3" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "UART4_RX" bidirectional line)
				(alternate "UCPD1_FRSTX2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "PC12")
				(number "113")
				(alternate "DEBUG_TRACED3" bidirectional line)
				(alternate "SAI2_SD_B" bidirectional line)
				(alternate "SDMMC1_CK" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
				(alternate "UART5_TX" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "PC13")
				(number "7")
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
				(alternate "TAMP_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "PC14")
				(number "8")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "PC15")
				(number "9")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "PD0")
				(number "114")
				(alternate "FDCAN1_RX" bidirectional line)
				(alternate "FMC_D2" bidirectional line)
				(alternate "FMC_DA2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "PD1")
				(number "115")
				(alternate "FDCAN1_TX" bidirectional line)
				(alternate "FMC_D3" bidirectional line)
				(alternate "FMC_DA3" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "PD2")
				(number "116")
				(alternate "DEBUG_TRACED2" bidirectional line)
				(alternate "SDMMC1_CMD" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "UART5_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "PD3")
				(number "117")
				(alternate "DFSDM1_DATIN0" bidirectional line)
				(alternate "FMC_CLK" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "PD4")
				(number "118")
				(alternate "DFSDM1_CKIN0" bidirectional line)
				(alternate "FMC_NOE" bidirectional line)
				(alternate "OCTOSPI1_IO4" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "PD5")
				(number "119")
				(alternate "FMC_NWE" bidirectional line)
				(alternate "OCTOSPI1_IO5" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "PD6")
				(number "122")
				(alternate "DFSDM1_DATIN1" bidirectional line)
				(alternate "FMC_NWAIT" bidirectional line)
				(alternate "OCTOSPI1_IO6" bidirectional line)
				(alternate "SAI1_D1" bidirectional line)
				(alternate "SAI1_SD_A" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "PD7")
				(number "123")
				(alternate "DFSDM1_CKIN1" bidirectional line)
				(alternate "FMC_NCE" bidirectional line)
				(alternate "FMC_NE1" bidirectional line)
				(alternate "OCTOSPI1_IO7" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "PD8")
				(number "77")
				(alternate "FMC_D13" bidirectional line)
				(alternate "FMC_DA13" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "PD9")
				(number "78")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "FMC_D14" bidirectional line)
				(alternate "FMC_DA14" bidirectional line)
				(alternate "SAI2_MCLK_A" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "PD10")
				(number "79")
				(alternate "FMC_D15" bidirectional line)
				(alternate "FMC_DA15" bidirectional line)
				(alternate "SAI2_SCK_A" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "PD11")
				(number "80")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "ADC2_EXTI11" bidirectional line)
				(alternate "FMC_A16" bidirectional line)
				(alternate "FMC_CLE" bidirectional line)
				(alternate "I2C4_SMBA" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SAI2_SD_A" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
				(alternate "USART3_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 5.08)
				(name "PD12")
				(number "81")
				(alternate "FMC_A17" bidirectional line)
				(alternate "FMC_ALE" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "SAI2_FS_A" bidirectional line)
				(alternate "TIM4_CH1" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 5.08)
				(name "PD13")
				(number "82")
				(alternate "FMC_A18" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LPTIM2_OUT" bidirectional line)
				(alternate "TIM4_CH2" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 5.08)
				(name "PD14")
				(number "85")
				(alternate "FMC_D0" bidirectional line)
				(alternate "FMC_DA0" bidirectional line)
				(alternate "TIM4_CH3" bidirectional line)
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 5.08)
				(name "PD15")
				(number "86")
				(alternate "ADC1_EXTI15" bidirectional line)
				(alternate "ADC2_EXTI15" bidirectional line)
				(alternate "FMC_D1" bidirectional line)
				(alternate "FMC_DA1" bidirectional line)
				(alternate "TIM4_CH4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32L552CCTx"
		(extends "STM32L552C_C-E_Tx")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32L552CCTx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552CCUx"
		(extends "STM32L552C_C-E_Ux")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32L552CCUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552CETx"
		(extends "STM32L552C_C-E_Tx")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32L552CETx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 38 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552CEUx"
		(extends "STM32L552C_C-E_Ux")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "STM32L552CEUx"
			(at 7.62 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552ce.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 38 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552QCIxQ"
		(extends "STM32L552Q_C-E_IxQ")
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32L552QCIxQ"
			(at 15.24 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -30.48 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552qc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 106 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552QEIxQ"
		(extends "STM32L552Q_C-E_IxQ")
		(property "Reference" "U"
			(at -30.48 90.17 0)
		)
		(property "Value" "STM32L552QEIxQ"
			(at 15.24 90.17 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-132_7x7mm_Layout12x12_P0.5mm"
			(at -30.48 -88.9 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552qe.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 106 GPIO, UFBGA132"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*7x7mm*Layout12x12*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552RCTx"
		(extends "STM32L552R_C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L552RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552RETx"
		(extends "STM32L552R_C-E_Tx")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32L552RETx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552re.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 52 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552VCTxQ"
		(extends "STM32L552V_C-E_TxQ")
		(property "Reference" "U"
			(at -22.86 64.77 0)
		)
		(property "Value" "STM32L552VCTxQ"
			(at 12.7 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -22.86 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552vc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 79 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552VETxQ"
		(extends "STM32L552V_C-E_TxQ")
		(property "Reference" "U"
			(at -22.86 64.77 0)
		)
		(property "Value" "STM32L552VETxQ"
			(at 12.7 64.77 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at -22.86 -63.5 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552ve.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 79 GPIO, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552ZCTxQ"
		(extends "STM32L552Z_C-E_TxQ")
		(property "Reference" "U"
			(at -30.48 87.63 0)
		)
		(property "Value" "STM32L552ZCTxQ"
			(at 20.32 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -30.48 -83.82 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552zc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 256KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 111 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "STM32L552ZETxQ"
		(extends "STM32L552Z_C-E_TxQ")
		(property "Reference" "U"
			(at -30.48 87.63 0)
		)
		(property "Value" "STM32L552ZETxQ"
			(at 20.32 87.63 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -30.48 -83.82 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32l552ze.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M33 MCU, 512KB flash, 256KB RAM, 110 MHz, 1.71-3.6V, 111 GPIO, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M33 STM32L5 STM32L5x2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
