(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "STM32U031C6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U031C6Tx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031C6Tx_0_1")
		(symbol "STM32U031C6Tx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031C6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U031C6Ux"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031c6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031C6Ux_0_1")
		(symbol "STM32U031C6Ux_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U031C8Tx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 12KB RAM, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031C8Tx_0_1")
		(symbol "STM32U031C8Tx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U031C8Ux"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 12KB RAM, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031C8Ux_0_1")
		(symbol "STM32U031C8Ux_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031F4Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 19.05 0)
		)
		(property "Value" "STM32U031F4Px"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -25.4 -15.24 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031f4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 12KB RAM, 17 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031F4Px_0_1")
		(symbol "STM32U031F4Px_1_1"
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PF3")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "13")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB8/PB9")
				(number "1")
				(alternate "DAC1_EXTI9 (PB9)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "I2C2_SCL (PB8)" bidirectional line)
				(alternate "I2C2_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "LPTIM1_CH4 (PB9)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB8)" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "USART3_RX (PB9)" bidirectional line)
				(alternate "USART3_TX (PB8)" bidirectional line)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDDA")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA1/PA2")
				(number "9")
				(alternate "ADC1_IN5 (PA1)" bidirectional line)
				(alternate "ADC1_IN6 (PA2)" bidirectional line)
				(alternate "COMP1_INP (PA1)" bidirectional line)
				(alternate "LPTIM1_CH2 (PA1)" bidirectional line)
				(alternate "LPUART1_TX (PA2)" bidirectional line)
				(alternate "OPAMP1_VINM (PA1)" bidirectional line)
				(alternate "PA1" bidirectional line)
				(alternate "PA2" bidirectional line)
				(alternate "PWR_WKUP3 (PA1)" bidirectional line)
				(alternate "PWR_WKUP4 (PA2)" bidirectional line)
				(alternate "RCC_LSCO (PA2)" bidirectional line)
				(alternate "SPI1_SCK (PA1)" bidirectional line)
				(alternate "SPI2_SCK (PA1)" bidirectional line)
				(alternate "TAMP_IN5 (PA1)" bidirectional line)
				(alternate "TIM15_CH1 (PA2)" bidirectional line)
				(alternate "TIM15_CH1N (PA1)" bidirectional line)
				(alternate "TIM2_CH2 (PA1)" bidirectional line)
				(alternate "TIM2_CH3 (PA2)" bidirectional line)
				(alternate "USART2_DE (PA1)" bidirectional line)
				(alternate "USART2_RTS (PA1)" bidirectional line)
				(alternate "USART2_TX (PA2)" bidirectional line)
				(alternate "USART4_RX (PA1)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA3/PA4")
				(number "10")
				(alternate "ADC1_IN7 (PA3)" bidirectional line)
				(alternate "ADC1_IN8 (PA4)" bidirectional line)
				(alternate "COMP1_INM (PA4)" bidirectional line)
				(alternate "DAC1_OUT1 (PA4)" bidirectional line)
				(alternate "LPTIM2_CH1 (PA4)" bidirectional line)
				(alternate "LPUART1_RX (PA3)" bidirectional line)
				(alternate "OPAMP1_VOUT (PA3)" bidirectional line)
				(alternate "PA3" bidirectional line)
				(alternate "PA4" bidirectional line)
				(alternate "SPI1_NSS (PA4)" bidirectional line)
				(alternate "TIM15_CH2 (PA3)" bidirectional line)
				(alternate "TIM2_CH4 (PA3)" bidirectional line)
				(alternate "USART2_CK (PA4)" bidirectional line)
				(alternate "USART2_RX (PA3)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA5/PA6")
				(number "11")
				(alternate "ADC1_IN10 (PA6)" bidirectional line)
				(alternate "ADC1_IN9 (PA5)" bidirectional line)
				(alternate "COMP1_INM (PA5)" bidirectional line)
				(alternate "COMP1_OUT (PA6)" bidirectional line)
				(alternate "I2C2_SDA (PA6)" bidirectional line)
				(alternate "I2C3_SDA (PA6)" bidirectional line)
				(alternate "LPTIM2_ETR (PA5)" bidirectional line)
				(alternate "LPUART1_CTS (PA6)" bidirectional line)
				(alternate "PA5" bidirectional line)
				(alternate "PA6" bidirectional line)
				(alternate "SPI1_MISO (PA6)" bidirectional line)
				(alternate "SPI1_SCK (PA5)" bidirectional line)
				(alternate "TIM16_CH1 (PA6)" bidirectional line)
				(alternate "TIM1_BKIN (PA6)" bidirectional line)
				(alternate "TIM2_CH1 (PA5)" bidirectional line)
				(alternate "TIM2_ETR (PA5)" bidirectional line)
				(alternate "TIM3_CH1 (PA6)" bidirectional line)
				(alternate "TSC_G5_IO1 (PA6)" bidirectional line)
				(alternate "USART3_CTS (PA6)" bidirectional line)
				(alternate "USART3_TX (PA5)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA7/PB0")
				(number "12")
				(alternate "ADC1_IN14 (PA7)" bidirectional line)
				(alternate "ADC1_IN17 (PB0)" bidirectional line)
				(alternate "COMP1_OUT (PB0)" bidirectional line)
				(alternate "I2C2_SCL (PA7)" bidirectional line)
				(alternate "I2C3_SCL (PA7)" bidirectional line)
				(alternate "LPTIM2_CH2 (PA7)" bidirectional line)
				(alternate "LPUART2_CTS (PB0)" bidirectional line)
				(alternate "PA7" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "SPI1_MOSI (PA7)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "TIM1_CH1N (PA7)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM3_CH2 (PA7)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TSC_G5_IO2 (PB0)" bidirectional line)
				(alternate "USART3_CK (PB0)" bidirectional line)
				(alternate "USART3_RX (PA7)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA8/PA9/PA10")
				(number "14")
				(alternate "COMP1_INP (PA9)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "LPTIM2_CH1 (PA8)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "RCC_MCO2 (PA10)" bidirectional line)
				(alternate "RCC_MCO2 (PA8)" bidirectional line)
				(alternate "SPI2_NSS (PA10)" bidirectional line)
				(alternate "TIM15_BKIN (PA9)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TSC_G7_IO1 (PA8)" bidirectional line)
				(alternate "TSC_G7_IO2 (PA9)" bidirectional line)
				(alternate "TSC_G7_IO3 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA8)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA11")
				(number "15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA12")
				(number "16")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "17")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PA14/PB4/PB5/PB6")
				(number "18")
				(alternate "DEBUG_JTCK-SWCLK (PA14)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C2_SCL (PB6)" bidirectional line)
				(alternate "I2C2_SDA (PB4)" bidirectional line)
				(alternate "I2C3_SDA (PB4)" bidirectional line)
				(alternate "LPTIM1_CH1 (PA14)" bidirectional line)
				(alternate "LPTIM1_CH4 (PB4)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "LPUART2_TX (PB6)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "TIM16_BKIN (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "TSC_G2_IO1 (PB4)" bidirectional line)
				(alternate "TSC_G2_IO2 (PB5)" bidirectional line)
				(alternate "TSC_G2_IO3 (PB6)" bidirectional line)
				(alternate "TSC_G3_IO4 (PA14)" bidirectional line)
				(alternate "USART1_CK (PB5)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031F6Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 19.05 0)
		)
		(property "Value" "STM32U031F6Px"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -25.4 -15.24 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031f6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 17 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031F6Px_0_1")
		(symbol "STM32U031F6Px_1_1"
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PF3")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "13")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB8/PB9")
				(number "1")
				(alternate "DAC1_EXTI9 (PB9)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "I2C2_SCL (PB8)" bidirectional line)
				(alternate "I2C2_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "LPTIM1_CH4 (PB9)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB8)" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "USART3_RX (PB9)" bidirectional line)
				(alternate "USART3_TX (PB8)" bidirectional line)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDDA")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA1/PA2")
				(number "9")
				(alternate "ADC1_IN5 (PA1)" bidirectional line)
				(alternate "ADC1_IN6 (PA2)" bidirectional line)
				(alternate "COMP1_INP (PA1)" bidirectional line)
				(alternate "LPTIM1_CH2 (PA1)" bidirectional line)
				(alternate "LPUART1_TX (PA2)" bidirectional line)
				(alternate "OPAMP1_VINM (PA1)" bidirectional line)
				(alternate "PA1" bidirectional line)
				(alternate "PA2" bidirectional line)
				(alternate "PWR_WKUP3 (PA1)" bidirectional line)
				(alternate "PWR_WKUP4 (PA2)" bidirectional line)
				(alternate "RCC_LSCO (PA2)" bidirectional line)
				(alternate "SPI1_SCK (PA1)" bidirectional line)
				(alternate "SPI2_SCK (PA1)" bidirectional line)
				(alternate "TAMP_IN5 (PA1)" bidirectional line)
				(alternate "TIM15_CH1 (PA2)" bidirectional line)
				(alternate "TIM15_CH1N (PA1)" bidirectional line)
				(alternate "TIM2_CH2 (PA1)" bidirectional line)
				(alternate "TIM2_CH3 (PA2)" bidirectional line)
				(alternate "USART2_DE (PA1)" bidirectional line)
				(alternate "USART2_RTS (PA1)" bidirectional line)
				(alternate "USART2_TX (PA2)" bidirectional line)
				(alternate "USART4_RX (PA1)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA3/PA4")
				(number "10")
				(alternate "ADC1_IN7 (PA3)" bidirectional line)
				(alternate "ADC1_IN8 (PA4)" bidirectional line)
				(alternate "COMP1_INM (PA4)" bidirectional line)
				(alternate "DAC1_OUT1 (PA4)" bidirectional line)
				(alternate "LPTIM2_CH1 (PA4)" bidirectional line)
				(alternate "LPUART1_RX (PA3)" bidirectional line)
				(alternate "OPAMP1_VOUT (PA3)" bidirectional line)
				(alternate "PA3" bidirectional line)
				(alternate "PA4" bidirectional line)
				(alternate "SPI1_NSS (PA4)" bidirectional line)
				(alternate "TIM15_CH2 (PA3)" bidirectional line)
				(alternate "TIM2_CH4 (PA3)" bidirectional line)
				(alternate "USART2_CK (PA4)" bidirectional line)
				(alternate "USART2_RX (PA3)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA5/PA6")
				(number "11")
				(alternate "ADC1_IN10 (PA6)" bidirectional line)
				(alternate "ADC1_IN9 (PA5)" bidirectional line)
				(alternate "COMP1_INM (PA5)" bidirectional line)
				(alternate "COMP1_OUT (PA6)" bidirectional line)
				(alternate "I2C2_SDA (PA6)" bidirectional line)
				(alternate "I2C3_SDA (PA6)" bidirectional line)
				(alternate "LPTIM2_ETR (PA5)" bidirectional line)
				(alternate "LPUART1_CTS (PA6)" bidirectional line)
				(alternate "PA5" bidirectional line)
				(alternate "PA6" bidirectional line)
				(alternate "SPI1_MISO (PA6)" bidirectional line)
				(alternate "SPI1_SCK (PA5)" bidirectional line)
				(alternate "TIM16_CH1 (PA6)" bidirectional line)
				(alternate "TIM1_BKIN (PA6)" bidirectional line)
				(alternate "TIM2_CH1 (PA5)" bidirectional line)
				(alternate "TIM2_ETR (PA5)" bidirectional line)
				(alternate "TIM3_CH1 (PA6)" bidirectional line)
				(alternate "TSC_G5_IO1 (PA6)" bidirectional line)
				(alternate "USART3_CTS (PA6)" bidirectional line)
				(alternate "USART3_TX (PA5)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA7/PB0")
				(number "12")
				(alternate "ADC1_IN14 (PA7)" bidirectional line)
				(alternate "ADC1_IN17 (PB0)" bidirectional line)
				(alternate "COMP1_OUT (PB0)" bidirectional line)
				(alternate "I2C2_SCL (PA7)" bidirectional line)
				(alternate "I2C3_SCL (PA7)" bidirectional line)
				(alternate "LPTIM2_CH2 (PA7)" bidirectional line)
				(alternate "LPUART2_CTS (PB0)" bidirectional line)
				(alternate "PA7" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "SPI1_MOSI (PA7)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "TIM1_CH1N (PA7)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM3_CH2 (PA7)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TSC_G5_IO2 (PB0)" bidirectional line)
				(alternate "USART3_CK (PB0)" bidirectional line)
				(alternate "USART3_RX (PA7)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA8/PA9/PA10")
				(number "14")
				(alternate "COMP1_INP (PA9)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "LPTIM2_CH1 (PA8)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "RCC_MCO2 (PA10)" bidirectional line)
				(alternate "RCC_MCO2 (PA8)" bidirectional line)
				(alternate "SPI2_NSS (PA10)" bidirectional line)
				(alternate "TIM15_BKIN (PA9)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TSC_G7_IO1 (PA8)" bidirectional line)
				(alternate "TSC_G7_IO2 (PA9)" bidirectional line)
				(alternate "TSC_G7_IO3 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA8)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA11")
				(number "15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA12")
				(number "16")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "17")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PA14/PB4/PB5/PB6")
				(number "18")
				(alternate "DEBUG_JTCK-SWCLK (PA14)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C2_SCL (PB6)" bidirectional line)
				(alternate "I2C2_SDA (PB4)" bidirectional line)
				(alternate "I2C3_SDA (PB4)" bidirectional line)
				(alternate "LPTIM1_CH1 (PA14)" bidirectional line)
				(alternate "LPTIM1_CH4 (PB4)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "LPUART2_TX (PB6)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "TIM16_BKIN (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "TSC_G2_IO1 (PB4)" bidirectional line)
				(alternate "TSC_G2_IO2 (PB5)" bidirectional line)
				(alternate "TSC_G2_IO3 (PB6)" bidirectional line)
				(alternate "TSC_G3_IO4 (PA14)" bidirectional line)
				(alternate "USART1_CK (PB5)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031F8Px"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 19.05 0)
		)
		(property "Value" "STM32U031F8Px"
			(at 5.08 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at -25.4 -15.24 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031f8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 12KB RAM, 17 GPIO, TSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031F8Px_0_1")
		(symbol "STM32U031F8Px_1_1"
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "PF2")
				(number "6")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "PF3")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PC14")
				(number "4")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PC15")
				(number "5")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "13")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PB7")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "PB8/PB9")
				(number "1")
				(alternate "DAC1_EXTI9 (PB9)" bidirectional line)
				(alternate "I2C1_SCL (PB8)" bidirectional line)
				(alternate "I2C1_SDA (PB9)" bidirectional line)
				(alternate "I2C2_SCL (PB8)" bidirectional line)
				(alternate "I2C2_SDA (PB9)" bidirectional line)
				(alternate "IR_OUT (PB9)" bidirectional line)
				(alternate "LPTIM1_CH4 (PB9)" bidirectional line)
				(alternate "LPTIM1_IN2 (PB8)" bidirectional line)
				(alternate "PB8" bidirectional line)
				(alternate "PB9" bidirectional line)
				(alternate "SPI2_NSS (PB9)" bidirectional line)
				(alternate "TIM16_CH1 (PB8)" bidirectional line)
				(alternate "USART3_RX (PB9)" bidirectional line)
				(alternate "USART3_TX (PB8)" bidirectional line)
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDDA")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 2.54)
				(name "PA0")
				(number "8")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "PA1/PA2")
				(number "9")
				(alternate "ADC1_IN5 (PA1)" bidirectional line)
				(alternate "ADC1_IN6 (PA2)" bidirectional line)
				(alternate "COMP1_INP (PA1)" bidirectional line)
				(alternate "LPTIM1_CH2 (PA1)" bidirectional line)
				(alternate "LPUART1_TX (PA2)" bidirectional line)
				(alternate "OPAMP1_VINM (PA1)" bidirectional line)
				(alternate "PA1" bidirectional line)
				(alternate "PA2" bidirectional line)
				(alternate "PWR_WKUP3 (PA1)" bidirectional line)
				(alternate "PWR_WKUP4 (PA2)" bidirectional line)
				(alternate "RCC_LSCO (PA2)" bidirectional line)
				(alternate "SPI1_SCK (PA1)" bidirectional line)
				(alternate "SPI2_SCK (PA1)" bidirectional line)
				(alternate "TAMP_IN5 (PA1)" bidirectional line)
				(alternate "TIM15_CH1 (PA2)" bidirectional line)
				(alternate "TIM15_CH1N (PA1)" bidirectional line)
				(alternate "TIM2_CH2 (PA1)" bidirectional line)
				(alternate "TIM2_CH3 (PA2)" bidirectional line)
				(alternate "USART2_DE (PA1)" bidirectional line)
				(alternate "USART2_RTS (PA1)" bidirectional line)
				(alternate "USART2_TX (PA2)" bidirectional line)
				(alternate "USART4_RX (PA1)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "PA3/PA4")
				(number "10")
				(alternate "ADC1_IN7 (PA3)" bidirectional line)
				(alternate "ADC1_IN8 (PA4)" bidirectional line)
				(alternate "COMP1_INM (PA4)" bidirectional line)
				(alternate "DAC1_OUT1 (PA4)" bidirectional line)
				(alternate "LPTIM2_CH1 (PA4)" bidirectional line)
				(alternate "LPUART1_RX (PA3)" bidirectional line)
				(alternate "OPAMP1_VOUT (PA3)" bidirectional line)
				(alternate "PA3" bidirectional line)
				(alternate "PA4" bidirectional line)
				(alternate "SPI1_NSS (PA4)" bidirectional line)
				(alternate "TIM15_CH2 (PA3)" bidirectional line)
				(alternate "TIM2_CH4 (PA3)" bidirectional line)
				(alternate "USART2_CK (PA4)" bidirectional line)
				(alternate "USART2_RX (PA3)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PA5/PA6")
				(number "11")
				(alternate "ADC1_IN10 (PA6)" bidirectional line)
				(alternate "ADC1_IN9 (PA5)" bidirectional line)
				(alternate "COMP1_INM (PA5)" bidirectional line)
				(alternate "COMP1_OUT (PA6)" bidirectional line)
				(alternate "I2C2_SDA (PA6)" bidirectional line)
				(alternate "I2C3_SDA (PA6)" bidirectional line)
				(alternate "LPTIM2_ETR (PA5)" bidirectional line)
				(alternate "LPUART1_CTS (PA6)" bidirectional line)
				(alternate "PA5" bidirectional line)
				(alternate "PA6" bidirectional line)
				(alternate "SPI1_MISO (PA6)" bidirectional line)
				(alternate "SPI1_SCK (PA5)" bidirectional line)
				(alternate "TIM16_CH1 (PA6)" bidirectional line)
				(alternate "TIM1_BKIN (PA6)" bidirectional line)
				(alternate "TIM2_CH1 (PA5)" bidirectional line)
				(alternate "TIM2_ETR (PA5)" bidirectional line)
				(alternate "TIM3_CH1 (PA6)" bidirectional line)
				(alternate "TSC_G5_IO1 (PA6)" bidirectional line)
				(alternate "USART3_CTS (PA6)" bidirectional line)
				(alternate "USART3_TX (PA5)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "PA7/PB0")
				(number "12")
				(alternate "ADC1_IN14 (PA7)" bidirectional line)
				(alternate "ADC1_IN17 (PB0)" bidirectional line)
				(alternate "COMP1_OUT (PB0)" bidirectional line)
				(alternate "I2C2_SCL (PA7)" bidirectional line)
				(alternate "I2C3_SCL (PA7)" bidirectional line)
				(alternate "LPTIM2_CH2 (PA7)" bidirectional line)
				(alternate "LPUART2_CTS (PB0)" bidirectional line)
				(alternate "PA7" bidirectional line)
				(alternate "PB0" bidirectional line)
				(alternate "SPI1_MOSI (PA7)" bidirectional line)
				(alternate "SPI1_NSS (PB0)" bidirectional line)
				(alternate "TIM1_CH1N (PA7)" bidirectional line)
				(alternate "TIM1_CH2N (PB0)" bidirectional line)
				(alternate "TIM3_CH2 (PA7)" bidirectional line)
				(alternate "TIM3_CH3 (PB0)" bidirectional line)
				(alternate "TSC_G5_IO2 (PB0)" bidirectional line)
				(alternate "USART3_CK (PB0)" bidirectional line)
				(alternate "USART3_RX (PA7)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 2.54)
				(name "PA8/PA9/PA10")
				(number "14")
				(alternate "COMP1_INP (PA9)" bidirectional line)
				(alternate "DAC1_EXTI9 (PA9)" bidirectional line)
				(alternate "I2C1_SCL (PA9)" bidirectional line)
				(alternate "I2C1_SDA (PA10)" bidirectional line)
				(alternate "I2C2_SCL (PA9)" bidirectional line)
				(alternate "I2C2_SDA (PA10)" bidirectional line)
				(alternate "LPTIM2_CH1 (PA8)" bidirectional line)
				(alternate "PA10" bidirectional line)
				(alternate "PA8" bidirectional line)
				(alternate "PA9" bidirectional line)
				(alternate "RCC_MCO (PA8)" bidirectional line)
				(alternate "RCC_MCO (PA9)" bidirectional line)
				(alternate "RCC_MCO2 (PA10)" bidirectional line)
				(alternate "RCC_MCO2 (PA8)" bidirectional line)
				(alternate "SPI2_NSS (PA10)" bidirectional line)
				(alternate "TIM15_BKIN (PA9)" bidirectional line)
				(alternate "TIM1_CH1 (PA8)" bidirectional line)
				(alternate "TIM1_CH2 (PA9)" bidirectional line)
				(alternate "TIM1_CH3 (PA10)" bidirectional line)
				(alternate "TSC_G7_IO1 (PA8)" bidirectional line)
				(alternate "TSC_G7_IO2 (PA9)" bidirectional line)
				(alternate "TSC_G7_IO3 (PA10)" bidirectional line)
				(alternate "USART1_CK (PA8)" bidirectional line)
				(alternate "USART1_RX (PA10)" bidirectional line)
				(alternate "USART1_TX (PA9)" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "PA11")
				(number "15")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "PA12")
				(number "16")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PA13")
				(number "17")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "PA14/PB4/PB5/PB6")
				(number "18")
				(alternate "DEBUG_JTCK-SWCLK (PA14)" bidirectional line)
				(alternate "I2C1_SCL (PB6)" bidirectional line)
				(alternate "I2C2_SCL (PB6)" bidirectional line)
				(alternate "I2C2_SDA (PB4)" bidirectional line)
				(alternate "I2C3_SDA (PB4)" bidirectional line)
				(alternate "LPTIM1_CH1 (PA14)" bidirectional line)
				(alternate "LPTIM1_CH4 (PB4)" bidirectional line)
				(alternate "LPTIM1_ETR (PB6)" bidirectional line)
				(alternate "LPTIM1_IN1 (PB5)" bidirectional line)
				(alternate "LPUART2_TX (PB6)" bidirectional line)
				(alternate "PA14" bidirectional line)
				(alternate "PB4" bidirectional line)
				(alternate "PB5" bidirectional line)
				(alternate "PB6" bidirectional line)
				(alternate "SPI1_MISO (PB4)" bidirectional line)
				(alternate "SPI1_MOSI (PB5)" bidirectional line)
				(alternate "TIM16_BKIN (PB5)" bidirectional line)
				(alternate "TIM16_CH1N (PB6)" bidirectional line)
				(alternate "TIM3_CH1 (PB4)" bidirectional line)
				(alternate "TIM3_CH2 (PB5)" bidirectional line)
				(alternate "TSC_G2_IO1 (PB4)" bidirectional line)
				(alternate "TSC_G2_IO2 (PB5)" bidirectional line)
				(alternate "TSC_G2_IO3 (PB6)" bidirectional line)
				(alternate "TSC_G3_IO4 (PA14)" bidirectional line)
				(alternate "USART1_CK (PB5)" bidirectional line)
				(alternate "USART1_CTS (PB4)" bidirectional line)
				(alternate "USART1_TX (PB6)" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031G6Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32U031G6Yx"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-27_2.34x2.55mm_Layout9x6_P0.4mm_Stagger"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031g6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 24 GPIO, WLCSP27"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.34x2.55mm*Layout9x6*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32U031G6Yx_0_1")
		(symbol "STM32U031G6Yx_1_1"
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "D9")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF3")
				(number "A6")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "B9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "C8")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB1")
				(number "F1")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB5")
				(number "B3")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "A2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "B7")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "A8")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "F9")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "C6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "D7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "E8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "F7")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "E6")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "D5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "E2")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "D3")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "D1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA11")
				(number "C4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA12")
				(number "B5")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA14")
				(number "B1")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031G8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "STM32U031G8Yx"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-27_2.34x2.55mm_Layout9x6_P0.4mm_Stagger"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031g8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 12KB RAM, 24 GPIO, WLCSP27"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.34x2.55mm*Layout9x6*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32U031G8Yx_0_1")
		(symbol "STM32U031G8Yx_1_1"
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF2")
				(number "D9")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PF3")
				(number "A6")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC14")
				(number "B9")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PC15")
				(number "C8")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB0")
				(number "F3")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB1")
				(number "F1")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB5")
				(number "B3")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB6")
				(number "A2")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB7")
				(number "A4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "B7")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "A8")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "F9")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "C6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "D7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "E8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "F7")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "F5")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "E6")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "D5")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA7")
				(number "E4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA8")
				(number "E2")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA9")
				(number "D3")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA10")
				(number "D1")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA11")
				(number "C4")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA12")
				(number "B5")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA13")
				(number "C2")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA14")
				(number "B1")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031K4Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32U031K4Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031k4.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 16KB flash, 12KB RAM, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031K4Ux_0_1")
		(symbol "STM32U031K4Ux_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031K6Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32U031K6Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031k6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031K6Ux_0_1")
		(symbol "STM32U031K6Ux_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031K8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32U031K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 12KB RAM, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031K8Ux_0_1")
		(symbol "STM32U031K8Ux_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031R6Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U031R6Ix"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 53 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031R6Ix_0_1")
		(symbol "STM32U031R6Ix_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "E1")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031R6Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U031R6Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031r6.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 32KB flash, 12KB RAM, 53 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031R6Tx_0_1")
		(symbol "STM32U031R6Tx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031R8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U031R8Ix"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 12KB RAM, 53 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031R8Ix_0_1")
		(symbol "STM32U031R8Ix_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "E1")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U031R8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U031R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u031r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 12KB RAM, 53 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U031R8Tx_0_1")
		(symbol "STM32U031R8Tx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073C8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U073C8Tx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 40KB RAM, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073C8Tx_0_1")
		(symbol "STM32U073C8Tx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDUSB")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073C8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U073C8Ux"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073c8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 40KB RAM, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073C8Ux_0_1")
		(symbol "STM32U073C8Ux_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDUSB")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073CBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U073CBTx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 40KB RAM, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073CBTx_0_1")
		(symbol "STM32U073CBTx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDUSB")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073CBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U073CBUx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073cb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 40KB RAM, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073CBUx_0_1")
		(symbol "STM32U073CBUx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDUSB")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U073CCTx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 56 MHz, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073CCTx_0_1")
		(symbol "STM32U073CCTx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDUSB")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U073CCUx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 56 MHz, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073CCUx_0_1")
		(symbol "STM32U073CCUx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDUSB")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073H8Yx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "STM32U073H8Yx"
			(at 7.62 29.21 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-42_2.93x2.82mm_Layout12x7_P0.4mm_Stagger"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073h8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 40KB RAM, 33 GPIO, WLCSP42"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.93x2.82mm*Layout12x7*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32U073H8Yx_0_1")
		(symbol "STM32U073H8Yx_1_1"
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "PF0")
				(number "D11")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "PF1")
				(number "D9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "PF2")
				(number "E12")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "PF3")
				(number "C8")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "PC13")
				(number "D7")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "PC14")
				(number "C12")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "PC15")
				(number "C10")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 5.08)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "PB1")
				(number "F3")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "PB4")
				(number "C6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "PB6")
				(number "B7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "PB7")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "PB8")
				(number "A10")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "PB10")
				(number "G4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 5.08)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "B11")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A12")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 5.08)
				(name "VDDA")
				(number "F11")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 5.08)
				(name "VSSA")
				(number "E10")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "PA0")
				(number "F9")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "PA1")
				(number "E8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "PA2")
				(number "G12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "PA3")
				(number "E6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "PA4")
				(number "G10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "PA5")
				(number "E4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "PA6")
				(number "G8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PA7")
				(number "F7")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "PA8")
				(number "D3")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 5.08)
				(name "PA9")
				(number "C4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PA10")
				(number "E2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "PA11")
				(number "D1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "PA12")
				(number "C2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "PA13")
				(number "B3")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "PA14")
				(number "D5")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "PA15")
				(number "A4")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073HBYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "STM32U073HBYx"
			(at 7.62 29.21 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-42_2.93x2.82mm_Layout12x7_P0.4mm_Stagger"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073hb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 40KB RAM, 33 GPIO, WLCSP42"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.93x2.82mm*Layout12x7*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32U073HBYx_0_1")
		(symbol "STM32U073HBYx_1_1"
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "PF0")
				(number "D11")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "PF1")
				(number "D9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "PF2")
				(number "E12")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "PF3")
				(number "C8")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "PC13")
				(number "D7")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "PC14")
				(number "C12")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "PC15")
				(number "C10")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 5.08)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "PB1")
				(number "F3")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "PB4")
				(number "C6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "PB6")
				(number "B7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "PB7")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "PB8")
				(number "A10")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "PB10")
				(number "G4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 5.08)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "B11")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A12")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 5.08)
				(name "VDDA")
				(number "F11")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 5.08)
				(name "VSSA")
				(number "E10")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "PA0")
				(number "F9")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "PA1")
				(number "E8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "PA2")
				(number "G12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "PA3")
				(number "E6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "PA4")
				(number "G10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "PA5")
				(number "E4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "PA6")
				(number "G8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PA7")
				(number "F7")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "PA8")
				(number "D3")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 5.08)
				(name "PA9")
				(number "C4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PA10")
				(number "E2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "PA11")
				(number "D1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "PA12")
				(number "C2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "PA13")
				(number "B3")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "PA14")
				(number "D5")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "PA15")
				(number "A4")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073HCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "STM32U073HCYx"
			(at 7.62 29.21 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-42_2.93x2.82mm_Layout12x7_P0.4mm_Stagger"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073hc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 33 GPIO, WLCSP42"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.93x2.82mm*Layout12x7*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32U073HCYx_0_1")
		(symbol "STM32U073HCYx_1_1"
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "PF0")
				(number "D11")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "PF1")
				(number "D9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "PF2")
				(number "E12")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "PF3")
				(number "C8")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "PC13")
				(number "D7")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "PC14")
				(number "C12")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "PC15")
				(number "C10")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 5.08)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "PB1")
				(number "F3")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "PB4")
				(number "C6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "PB6")
				(number "B7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "PB7")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "PB8")
				(number "A10")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "PB10")
				(number "G4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 5.08)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "B11")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A12")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 5.08)
				(name "VDDA")
				(number "F11")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 5.08)
				(name "VSSA")
				(number "E10")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "PA0")
				(number "F9")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "PA1")
				(number "E8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "PA2")
				(number "G12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "PA3")
				(number "E6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "PA4")
				(number "G10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "PA5")
				(number "E4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "PA6")
				(number "G8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PA7")
				(number "F7")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "PA8")
				(number "D3")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 5.08)
				(name "PA9")
				(number "C4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PA10")
				(number "E2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "PA11")
				(number "D1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "PA12")
				(number "C2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "PA13")
				(number "B3")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "PA14")
				(number "D5")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "PA15")
				(number "A4")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073K8Ux"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32U073K8Ux"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073k8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 40KB RAM, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073K8Ux_0_1")
		(symbol "STM32U073K8Ux_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073KBUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32U073KBUx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073kb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 40KB RAM, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073KBUx_0_1")
		(symbol "STM32U073KBUx_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073KCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32U073KCUx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 56 MHz, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073KCUx_0_1")
		(symbol "STM32U073KCUx_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073M8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 59.69 0)
		)
		(property "Value" "STM32U073M8Ix"
			(at 10.16 59.69 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-81_5x5mm_Layout9x9_P0.5mm"
			(at -15.24 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073m8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 40KB RAM, 69 GPIO, UFBGA81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073M8Ix_0_1")
		(symbol "STM32U073M8Ix_1_1"
			(pin input line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "H1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 48.26 0)
				(length 2.54)
				(name "PF0")
				(number "D2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF3")
				(number "A2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PE3")
				(number "C3")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "G5")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "G6")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "H6")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "A6")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "C6")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "A5")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "C5")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "B5")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "H9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "G8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PD10")
				(number "G9")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD11")
				(number "F8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD12")
				(number "F9")
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD13")
				(number "E9")
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E1")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "J5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "G4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "E8")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "E6")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "E5")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "D9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "A8")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "B7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "A7")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "E3")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "C2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "C1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 2.54)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "G2")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 2.54)
				(name "VDDA")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 2.54)
				(name "VDDUSB")
				(number "C7")
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 2.54)
				(name "PA0")
				(number "F3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PA3")
				(number "J2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PA4")
				(number "J3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA5")
				(number "H3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA6")
				(number "J4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA8")
				(number "E7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA9")
				(number "D7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA10")
				(number "D8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA11")
				(number "C9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA12")
				(number "C8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA13")
				(number "B9")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA14")
				(number "B8")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A9")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB2")
				(number "J6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB7")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB8")
				(number "A1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB9")
				(number "B2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB10")
				(number "J7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB12")
				(number "J8")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB13")
				(number "H8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB14")
				(number "J9")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073M8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 57.15 0)
		)
		(property "Value" "STM32U073M8Tx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -15.24 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073m8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 40KB RAM, 68 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073M8Tx_0_1")
		(symbol "STM32U073M8Tx_1_1"
			(pin input line
				(at -17.78 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "15")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "PF0")
				(number "7")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "PF1")
				(number "8")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF2")
				(number "9")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF3")
				(number "78")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "32")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "33")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "34")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "66")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "67")
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "68")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "69")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "70")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "71")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "72")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "43")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "44")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PD10")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD11")
				(number "46")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD12")
				(number "47")
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD13")
				(number "48")
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "27")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "28")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "49")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "50")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "51")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "52")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "63")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "65")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "4")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "5")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "6")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "16")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDUSB")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "23")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "24")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "25")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "26")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "53")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "54")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "56")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "57")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "58")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "61")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "62")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "29")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "30")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB3")
				(number "73")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "74")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "75")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "76")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "77")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "79")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "80")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "35")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "36")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "39")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "40")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "41")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "42")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073MBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 59.69 0)
		)
		(property "Value" "STM32U073MBIx"
			(at 10.16 59.69 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-81_5x5mm_Layout9x9_P0.5mm"
			(at -15.24 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 40KB RAM, 69 GPIO, UFBGA81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073MBIx_0_1")
		(symbol "STM32U073MBIx_1_1"
			(pin input line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "H1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 48.26 0)
				(length 2.54)
				(name "PF0")
				(number "D2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF3")
				(number "A2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PE3")
				(number "C3")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "G5")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "G6")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "H6")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "A6")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "C6")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "A5")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "C5")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "B5")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "H9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "G8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PD10")
				(number "G9")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD11")
				(number "F8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD12")
				(number "F9")
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD13")
				(number "E9")
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E1")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "J5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "G4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "E8")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "E6")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "E5")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "D9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "A8")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "B7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "A7")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "E3")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "C2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "C1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 2.54)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "G2")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 2.54)
				(name "VDDA")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 2.54)
				(name "VDDUSB")
				(number "C7")
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 2.54)
				(name "PA0")
				(number "F3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PA3")
				(number "J2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PA4")
				(number "J3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA5")
				(number "H3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA6")
				(number "J4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA8")
				(number "E7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA9")
				(number "D7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA10")
				(number "D8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA11")
				(number "C9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA12")
				(number "C8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA13")
				(number "B9")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA14")
				(number "B8")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A9")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB2")
				(number "J6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB7")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB8")
				(number "A1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB9")
				(number "B2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB10")
				(number "J7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB12")
				(number "J8")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB13")
				(number "H8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB14")
				(number "J9")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073MBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 57.15 0)
		)
		(property "Value" "STM32U073MBTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -15.24 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073mb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 40KB RAM, 68 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073MBTx_0_1")
		(symbol "STM32U073MBTx_1_1"
			(pin input line
				(at -17.78 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "15")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "PF0")
				(number "7")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "PF1")
				(number "8")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF2")
				(number "9")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF3")
				(number "78")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "32")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "33")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "34")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "66")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "67")
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "68")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "69")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "70")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "71")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "72")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "43")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "44")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PD10")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD11")
				(number "46")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD12")
				(number "47")
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD13")
				(number "48")
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "27")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "28")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "49")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "50")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "51")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "52")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "63")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "65")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "4")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "5")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "6")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "16")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDUSB")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "23")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "24")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "25")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "26")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "53")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "54")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "56")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "57")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "58")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "61")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "62")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "29")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "30")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB3")
				(number "73")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "74")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "75")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "76")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "77")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "79")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "80")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "35")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "36")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "39")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "40")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "41")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "42")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073MCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 59.69 0)
		)
		(property "Value" "STM32U073MCIx"
			(at 10.16 59.69 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-81_5x5mm_Layout9x9_P0.5mm"
			(at -15.24 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 56 MHz, 69 GPIO, UFBGA81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073MCIx_0_1")
		(symbol "STM32U073MCIx_1_1"
			(pin input line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "H1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 48.26 0)
				(length 2.54)
				(name "PF0")
				(number "D2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF3")
				(number "A2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PE3")
				(number "C3")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "G5")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "G6")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "H6")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "A6")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "C6")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "A5")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "C5")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "B5")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "H9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "G8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PD10")
				(number "G9")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD11")
				(number "F8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD12")
				(number "F9")
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD13")
				(number "E9")
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E1")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "J5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "G4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "E8")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "E6")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "E5")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "D9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "A8")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "B7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "A7")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "E3")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "C2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "C1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 2.54)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "G2")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 2.54)
				(name "VDDA")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 2.54)
				(name "VDDUSB")
				(number "C7")
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 2.54)
				(name "PA0")
				(number "F3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PA3")
				(number "J2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PA4")
				(number "J3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA5")
				(number "H3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA6")
				(number "J4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA8")
				(number "E7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA9")
				(number "D7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA10")
				(number "D8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA11")
				(number "C9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA12")
				(number "C8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA13")
				(number "B9")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA14")
				(number "B8")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A9")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB2")
				(number "J6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB7")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB8")
				(number "A1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB9")
				(number "B2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB10")
				(number "J7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB12")
				(number "J8")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB13")
				(number "H8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB14")
				(number "J9")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073MCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 57.15 0)
		)
		(property "Value" "STM32U073MCTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -15.24 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 56 MHz, 68 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073MCTx_0_1")
		(symbol "STM32U073MCTx_1_1"
			(pin input line
				(at -17.78 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "15")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "PF0")
				(number "7")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "PF1")
				(number "8")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF2")
				(number "9")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF3")
				(number "78")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "32")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "33")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "34")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "66")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "67")
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "68")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "69")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "70")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "71")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "72")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "43")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "44")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PD10")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD11")
				(number "46")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD12")
				(number "47")
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD13")
				(number "48")
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "27")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "28")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "49")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "50")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "51")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "52")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "63")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "65")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "4")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "5")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "6")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "16")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDUSB")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "23")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "24")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "25")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "26")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "53")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "54")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "56")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "57")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "58")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "61")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "62")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "29")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "30")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB3")
				(number "73")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "74")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "75")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "76")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "77")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "79")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "80")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "35")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "36")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "39")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "40")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "41")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "42")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073R8Ix"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U073R8Ix"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 40KB RAM, 53 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073R8Ix_0_1")
		(symbol "STM32U073R8Ix_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "E1")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "E5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073R8Tx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U073R8Tx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073r8.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 40KB RAM, 53 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073R8Tx_0_1")
		(symbol "STM32U073R8Tx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073RBIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U073RBIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 40KB RAM, 53 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073RBIx_0_1")
		(symbol "STM32U073RBIx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "E1")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "E5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073RBTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U073RBTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073rb.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 40KB RAM, 53 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073RBTx_0_1")
		(symbol "STM32U073RBTx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073RCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U073RCIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 53 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073RCIx_0_1")
		(symbol "STM32U073RCIx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "E1")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "E5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U073RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U073RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u073rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 56 MHz, 53 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U073RCTx_0_1")
		(symbol "STM32U073RCTx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U083CCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U083CCTx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u083cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 39 GPIO, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U083CCTx_0_1")
		(symbol "STM32U083CCTx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDUSB")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U083CCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "STM32U083CCUx"
			(at 7.62 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm"
			(at -12.7 -35.56 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u083cc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 39 GPIO, UFQFPN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U083CCUx_0_1")
		(symbol "STM32U083CCUx_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF3")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB0")
				(number "18")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "19")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "20")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "39")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "40")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "41")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "42")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "43")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB8")
				(number "45")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB9")
				(number "46")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB10")
				(number "21")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PB11")
				(number "22")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PB12")
				(number "25")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PB13")
				(number "26")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PB14")
				(number "27")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PB15")
				(number "28")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "35")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDUSB")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "10")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "11")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "13")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "14")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "15")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "16")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "17")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA8")
				(number "29")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA9")
				(number "30")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "31")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "32")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA12")
				(number "33")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA13")
				(number "34")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA14")
				(number "37")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA15")
				(number "38")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U083HCYx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 29.21 0)
		)
		(property "Value" "STM32U083HCYx"
			(at 7.62 29.21 0)
		)
		(property "Footprint" "Package_CSP:ST_WLCSP-42_2.93x2.82mm_Layout12x7_P0.4mm_Stagger"
			(at -12.7 -27.94 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u083hc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 33 GPIO, WLCSP42"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*WLCSP*2.93x2.82mm*Layout12x7*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "STM32U083HCYx_0_1")
		(symbol "STM32U083HCYx_1_1"
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 5.08)
				(name "PF0")
				(number "D11")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "PF1")
				(number "D9")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "PF2")
				(number "E12")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "PF3")
				(number "C8")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 5.08)
				(name "PC13")
				(number "D7")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "PC14")
				(number "C12")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "PC15")
				(number "C10")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 5.08)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "PB1")
				(number "F3")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "PB3")
				(number "B5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 5.08)
				(name "PB4")
				(number "C6")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 5.08)
				(name "PB5")
				(number "A6")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "PB6")
				(number "B7")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "PB7")
				(number "A8")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "PB8")
				(number "A10")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 5.08)
				(name "PB10")
				(number "G4")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 5.08)
				(name "VBAT")
				(number "B9")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "B11")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "G2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "A12")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "A2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F1")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 5.08)
				(name "VDDA")
				(number "F11")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 5.08)
				(name "VSSA")
				(number "E10")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 5.08)
				(name "VDDUSB")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "PA0")
				(number "F9")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "PA1")
				(number "E8")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "PA2")
				(number "G12")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "PA3")
				(number "E6")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "PA4")
				(number "G10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "PA5")
				(number "E4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "PA6")
				(number "G8")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "PA7")
				(number "F7")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "PA8")
				(number "D3")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 5.08)
				(name "PA9")
				(number "C4")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "PA10")
				(number "E2")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "PA11")
				(number "D1")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "PA12")
				(number "C2")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "PA13")
				(number "B3")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "PA14")
				(number "D5")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "PA15")
				(number "A4")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U083KCUx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "STM32U083KCUx"
			(at 5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at -10.16 -22.86 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u083kc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 56 MHz, 27 GPIO, UFQFPN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U083KCUx_0_1")
		(symbol "STM32U083KCUx_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "4")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "PC14")
				(number "2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PC15")
				(number "3")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PB0")
				(number "14")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PB1")
				(number "15")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PB3")
				(number "26")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "27")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "28")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "29")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "30")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "32")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "6")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "7")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "8")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "9")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "10")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "11")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA8")
				(number "18")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA9")
				(number "19")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA10")
				(number "20")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA11")
				(number "21")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA12")
				(number "22")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA13")
				(number "23")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA14")
				(number "24")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA15")
				(number "25")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U083MCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 59.69 0)
		)
		(property "Value" "STM32U083MCIx"
			(at 10.16 59.69 0)
		)
		(property "Footprint" "Package_BGA:ST_UFBGA-81_5x5mm_Layout9x9_P0.5mm"
			(at -15.24 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u083mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 69 GPIO, UFBGA81"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*UFBGA*5x5mm*Layout9x9*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U083MCIx_0_1")
		(symbol "STM32U083MCIx_1_1"
			(pin input line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "VREF+")
				(number "H1")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 48.26 0)
				(length 2.54)
				(name "PF0")
				(number "D2")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "PF2")
				(number "E2")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF3")
				(number "A2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PE3")
				(number "C3")
				(alternate "TIM3_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "G5")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "G6")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "H6")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "A6")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "B6")
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "C6")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "D5")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "A5")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "C5")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "B5")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "H9")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "G8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PD10")
				(number "G9")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD11")
				(number "F8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD12")
				(number "F9")
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD13")
				(number "E9")
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "E1")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "F1")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "J5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "G4")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "E8")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "E6")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "E5")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "D9")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "A8")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "B7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "A7")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "E3")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "C2")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "C1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 60.96 270)
				(length 2.54)
				(name "VBAT")
				(number "B1")
			)
			(pin power_in line
				(at -2.54 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "D3")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "G3")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "F6")
			)
			(pin power_in line
				(at 2.54 60.96 270)
				(length 2.54)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "G2")
			)
			(pin power_in line
				(at 5.08 60.96 270)
				(length 2.54)
				(name "VDDA")
				(number "J1")
			)
			(pin power_in line
				(at 7.62 60.96 270)
				(length 2.54)
				(name "VDDUSB")
				(number "C7")
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 2.54)
				(name "PA0")
				(number "F3")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PA1")
				(number "E4")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PA2")
				(number "H2")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PA3")
				(number "J2")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PA4")
				(number "J3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA5")
				(number "H3")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA6")
				(number "J4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA8")
				(number "E7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA9")
				(number "D7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA10")
				(number "D8")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA11")
				(number "C9")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA12")
				(number "C8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA13")
				(number "B9")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA14")
				(number "B8")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA15")
				(number "A9")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB1")
				(number "H5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB2")
				(number "J6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB3")
				(number "C4")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB4")
				(number "A3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB5")
				(number "A4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB6")
				(number "B4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB7")
				(number "B3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB8")
				(number "A1")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB9")
				(number "B2")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB10")
				(number "J7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB12")
				(number "J8")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB13")
				(number "H8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB14")
				(number "J9")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U083MCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 57.15 0)
		)
		(property "Value" "STM32U083MCTx"
			(at 10.16 57.15 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at -15.24 -55.88 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u083mc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 68 GPIO, LQFP80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U083MCTx_0_1")
		(symbol "STM32U083MCTx_1_1"
			(pin input line
				(at -17.78 50.8 0)
				(length 2.54)
				(name "VREF+")
				(number "15")
				(alternate "VREFBUF_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "PF0")
				(number "7")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "PF1")
				(number "8")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF2")
				(number "9")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF3")
				(number "78")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PE7")
				(number "32")
				(alternate "LCD_SEG45" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PE8")
				(number "33")
				(alternate "LCD_SEG46" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PE9")
				(number "34")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG47" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PD0")
				(number "66")
				(alternate "LCD_SEG34" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PD1")
				(number "67")
				(alternate "LCD_SEG35" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PD2")
				(number "68")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PD3")
				(number "69")
				(alternate "LCD_SEG36" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PD4")
				(number "70")
				(alternate "LCD_SEG37" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PD5")
				(number "71")
				(alternate "LCD_SEG38" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PD6")
				(number "72")
				(alternate "LCD_SEG39" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PD8")
				(number "43")
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PD9")
				(number "44")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PD10")
				(number "45")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "TSC_G6_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD11")
				(number "46")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "TSC_G6_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD12")
				(number "47")
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG32" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "TSC_G6_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD13")
				(number "48")
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG33" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "TSC_G6_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC0")
				(number "10")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC1")
				(number "11")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC2")
				(number "12")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC3")
				(number "13")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC4")
				(number "27")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC5")
				(number "28")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC6")
				(number "49")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC7")
				(number "50")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC8")
				(number "51")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PC9")
				(number "52")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PC10")
				(number "63")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PC11")
				(number "64")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "PC12")
				(number "65")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "PC13")
				(number "4")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "PC14")
				(number "5")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -50.8 0)
				(length 2.54)
				(name "PC15")
				(number "6")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 58.42 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "37")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 2.54)
				(name "VSSA")
				(number "14")
			)
			(pin power_in line
				(at 5.08 58.42 270)
				(length 2.54)
				(name "VDDA")
				(number "16")
			)
			(pin power_in line
				(at 7.62 58.42 270)
				(length 2.54)
				(name "VDDUSB")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 2.54)
				(name "PA0")
				(number "17")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "PA1")
				(number "18")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PA2")
				(number "19")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PA3")
				(number "20")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA4")
				(number "23")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA5")
				(number "24")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA6")
				(number "25")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA7")
				(number "26")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA8")
				(number "53")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA9")
				(number "54")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA10")
				(number "55")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA11")
				(number "56")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA12")
				(number "57")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA13")
				(number "58")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "61")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "62")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "29")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "30")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "31")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB3")
				(number "73")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "74")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "75")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB6")
				(number "76")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB7")
				(number "77")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB8")
				(number "79")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB9")
				(number "80")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB10")
				(number "35")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB11")
				(number "36")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB12")
				(number "39")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB13")
				(number "40")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB14")
				(number "41")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB15")
				(number "42")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U083RCIx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U083RCIx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u083rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 53 GPIO, UFBGA64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U083RCIx_0_1")
		(symbol "STM32U083RCIx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "C1")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "D1")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "E1")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "B5")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "E3")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "E2")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "F2")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "G1")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "H5")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "H6")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "F6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "E7")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "E8")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "D8")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "B7")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "B6")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "C5")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "A2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "A1")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "B1")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E4")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "C2")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "D6")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "F1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "H1")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "E5")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "G2")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "H2")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "F3")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "G3")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "H3")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "F4")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "G4")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "H4")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "D7")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "C7")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "C6")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "C8")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "B8")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "A8")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "A7")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "A6")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "F5")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "G5")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "G6")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "A5")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "A4")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "C4")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "D3")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "B3")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "A3")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "G7")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "H7")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "H8")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "G8")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "F8")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "F7")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "STM32U083RCTx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "STM32U083RCTx"
			(at 10.16 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at -15.24 -45.72 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32u083rc.pdf"
			(at 0 0 0)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 256KB flash, 40KB RAM, 53 GPIO, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arm Cortex-M0+ STM32U0 STM32U0x3"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STM32U083RCTx_0_1")
		(symbol "STM32U083RCTx_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PF0")
				(number "5")
				(alternate "RCC_OSC_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PF1")
				(number "6")
				(alternate "RCC_OSC_EN" bidirectional line)
				(alternate "RCC_OSC_OUT" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PF2")
				(number "7")
				(alternate "RCC_MCO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PF3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PD2")
				(number "54")
				(alternate "LCD_COM7" bidirectional line)
				(alternate "LCD_SEG31" bidirectional line)
				(alternate "LCD_SEG51" bidirectional line)
				(alternate "TIM3_ETR" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PC0")
				(number "8")
				(alternate "ADC1_IN0" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG18" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PC1")
				(number "9")
				(alternate "ADC1_IN1" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG19" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC2")
				(number "10")
				(alternate "ADC1_IN2" bidirectional line)
				(alternate "LCD_SEG20" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PC3")
				(number "11")
				(alternate "ADC1_IN3" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PC4")
				(number "24")
				(alternate "ADC1_IN15" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG22" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PC5")
				(number "25")
				(alternate "ADC1_IN16" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG23" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_WKUP5" bidirectional line)
				(alternate "TAMP_IN4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PC6")
				(number "37")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG24" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G4_IO1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PC7")
				(number "38")
				(alternate "LCD_SEG25" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G4_IO2" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PC8")
				(number "39")
				(alternate "LCD_SEG26" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G4_IO3" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PC9")
				(number "40")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "LCD_SEG27" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_G4_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PC10")
				(number "51")
				(alternate "LCD_COM4" bidirectional line)
				(alternate "LCD_SEG28" bidirectional line)
				(alternate "LCD_SEG48" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TSC_G3_IO2" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PC11")
				(number "52")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "LCD_COM5" bidirectional line)
				(alternate "LCD_SEG29" bidirectional line)
				(alternate "LCD_SEG49" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TSC_G3_IO3" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PC12")
				(number "53")
				(alternate "LCD_COM6" bidirectional line)
				(alternate "LCD_SEG30" bidirectional line)
				(alternate "LCD_SEG50" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
				(alternate "USART4_CK" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PC13")
				(number "2")
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "PWR_WKUP2" bidirectional line)
				(alternate "RTC_OUT1" bidirectional line)
				(alternate "RTC_TS" bidirectional line)
				(alternate "TAMP_IN1" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PC14")
				(number "3")
				(alternate "RCC_OSC32_IN" bidirectional line)
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC15")
				(number "4")
				(alternate "RCC_OSC32_EN" bidirectional line)
				(alternate "RCC_OSC32_OUT" bidirectional line)
				(alternate "RCC_OSC_EN" bidirectional line)
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VBAT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "63")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDUSB")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA0")
				(number "14")
				(alternate "ADC1_IN4" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG42" bidirectional line)
				(alternate "OPAMP1_VINP" bidirectional line)
				(alternate "PWR_WKUP1" bidirectional line)
				(alternate "TAMP_IN2" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART2_CTS" bidirectional line)
				(alternate "USART4_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA1")
				(number "15")
				(alternate "ADC1_IN5" bidirectional line)
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_SEG0" bidirectional line)
				(alternate "LPTIM1_CH2" bidirectional line)
				(alternate "OPAMP1_VINM" bidirectional line)
				(alternate "PWR_WKUP3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TAMP_IN5" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART2_DE" bidirectional line)
				(alternate "USART2_RTS" bidirectional line)
				(alternate "USART4_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA2")
				(number "16")
				(alternate "ADC1_IN6" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG1" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "PWR_WKUP4" bidirectional line)
				(alternate "RCC_LSCO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "USART2_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA3")
				(number "17")
				(alternate "ADC1_IN7" bidirectional line)
				(alternate "COMP2_INP" bidirectional line)
				(alternate "LCD_SEG2" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "OPAMP1_VOUT" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA4")
				(number "20")
				(alternate "ADC1_IN8" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DAC1_OUT1" bidirectional line)
				(alternate "LCD_SEG43" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "USART2_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA5")
				(number "21")
				(alternate "ADC1_IN9" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "COMP2_INM" bidirectional line)
				(alternate "LCD_SEG44" bidirectional line)
				(alternate "LPTIM2_ETR" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA6")
				(number "22")
				(alternate "ADC1_IN10" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG3" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G5_IO1" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA7")
				(number "23")
				(alternate "ADC1_IN14" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG4" bidirectional line)
				(alternate "LPTIM2_CH2" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA8")
				(number "41")
				(alternate "LCD_COM0" bidirectional line)
				(alternate "LPTIM2_CH1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "TIM1_CH1" bidirectional line)
				(alternate "TSC_G7_IO1" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA9")
				(number "42")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_COM1" bidirectional line)
				(alternate "RCC_MCO" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_CH2" bidirectional line)
				(alternate "TSC_G7_IO2" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA10")
				(number "43")
				(alternate "CRS_SYNC" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_COM2" bidirectional line)
				(alternate "RCC_MCO2" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM1_CH3" bidirectional line)
				(alternate "TSC_G7_IO3" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA11")
				(number "44")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM1_BKIN2" bidirectional line)
				(alternate "TIM1_CH4" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
				(alternate "USB_DM" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA12")
				(number "45")
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TIM1_ETR" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
				(alternate "USB_DP" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA13")
				(number "46")
				(alternate "DEBUG_JTMS-SWDIO" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_SEG40" bidirectional line)
				(alternate "TSC_G7_IO4" bidirectional line)
				(alternate "USB_NOE" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA14")
				(number "49")
				(alternate "DEBUG_JTCK-SWCLK" bidirectional line)
				(alternate "LCD_SEG41" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "TSC_G3_IO4" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA15")
				(number "50")
				(alternate "DEBUG_JTDI" bidirectional line)
				(alternate "LCD_SEG17" bidirectional line)
				(alternate "LPTIM3_CH3" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "SPI3_NSS" bidirectional line)
				(alternate "TIM2_CH1" bidirectional line)
				(alternate "TIM2_ETR" bidirectional line)
				(alternate "TSC_G3_IO1" bidirectional line)
				(alternate "USART2_RX" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
				(alternate "USART4_DE" bidirectional line)
				(alternate "USART4_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "26")
				(alternate "ADC1_IN17" bidirectional line)
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "LCD_SEG5" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART2_CTS" bidirectional line)
				(alternate "SPI1_NSS" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TIM3_CH3" bidirectional line)
				(alternate "TSC_G5_IO2" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
				(alternate "ADC1_IN18" bidirectional line)
				(alternate "COMP1_INM" bidirectional line)
				(alternate "LCD_SEG6" bidirectional line)
				(alternate "LPTIM2_IN1" bidirectional line)
				(alternate "LPTIM3_CH2" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "LPUART2_DE" bidirectional line)
				(alternate "LPUART2_RTS" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TIM3_CH4" bidirectional line)
				(alternate "TSC_SYNC" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "28")
				(alternate "COMP1_INP" bidirectional line)
				(alternate "LCD_VLCD" bidirectional line)
				(alternate "LPTIM1_CH1" bidirectional line)
				(alternate "RTC_OUT2" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "55")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "DEBUG_JTDO-SWO" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C3_SCL" bidirectional line)
				(alternate "LCD_SEG7" bidirectional line)
				(alternate "LPTIM1_CH3" bidirectional line)
				(alternate "SPI1_SCK" bidirectional line)
				(alternate "SPI3_SCK" bidirectional line)
				(alternate "TIM2_CH2" bidirectional line)
				(alternate "USART1_DE" bidirectional line)
				(alternate "USART1_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "56")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C3_SDA" bidirectional line)
				(alternate "LCD_SEG8" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPUART3_DE" bidirectional line)
				(alternate "LPUART3_RTS" bidirectional line)
				(alternate "SPI1_MISO" bidirectional line)
				(alternate "SPI3_MISO" bidirectional line)
				(alternate "TIM3_CH1" bidirectional line)
				(alternate "TSC_G2_IO1" bidirectional line)
				(alternate "USART1_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "57")
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "LCD_SEG9" bidirectional line)
				(alternate "LPTIM1_IN1" bidirectional line)
				(alternate "LPUART3_CTS" bidirectional line)
				(alternate "SPI1_MOSI" bidirectional line)
				(alternate "SPI3_MOSI" bidirectional line)
				(alternate "TIM16_BKIN" bidirectional line)
				(alternate "TIM3_CH2" bidirectional line)
				(alternate "TSC_G2_IO2" bidirectional line)
				(alternate "USART1_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "58")
				(alternate "COMP2_INP" bidirectional line)
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LPTIM1_ETR" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "LPUART3_TX" bidirectional line)
				(alternate "TIM16_CH1N" bidirectional line)
				(alternate "TSC_G2_IO3" bidirectional line)
				(alternate "USART1_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "59")
				(alternate "COMP2_INM" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG21" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "LPUART3_RX" bidirectional line)
				(alternate "PWR_PVD_IN" bidirectional line)
				(alternate "TSC_G2_IO4" bidirectional line)
				(alternate "USART1_RX" bidirectional line)
				(alternate "USART4_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB8")
				(number "61")
				(alternate "I2C1_SCL" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG16" bidirectional line)
				(alternate "LPTIM1_IN2" bidirectional line)
				(alternate "LPTIM3_IN2" bidirectional line)
				(alternate "TIM16_CH1" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB9")
				(number "62")
				(alternate "DAC1_EXTI9" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "IR_OUT" bidirectional line)
				(alternate "LCD_COM3" bidirectional line)
				(alternate "LPTIM1_CH4" bidirectional line)
				(alternate "LPTIM3_CH4" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB10")
				(number "29")
				(alternate "COMP1_OUT" bidirectional line)
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "I2C4_SCL" bidirectional line)
				(alternate "LCD_SEG10" bidirectional line)
				(alternate "LPTIM3_CH1" bidirectional line)
				(alternate "LPUART1_RX" bidirectional line)
				(alternate "LPUART2_RX" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM2_CH3" bidirectional line)
				(alternate "TSC_G5_IO3" bidirectional line)
				(alternate "USART3_TX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB11")
				(number "30")
				(alternate "ADC1_EXTI11" bidirectional line)
				(alternate "COMP2_OUT" bidirectional line)
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "I2C4_SDA" bidirectional line)
				(alternate "LCD_SEG11" bidirectional line)
				(alternate "LPUART1_TX" bidirectional line)
				(alternate "LPUART2_TX" bidirectional line)
				(alternate "TIM2_CH4" bidirectional line)
				(alternate "TSC_G5_IO4" bidirectional line)
				(alternate "USART3_RX" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB12")
				(number "33")
				(alternate "LCD_SEG12" bidirectional line)
				(alternate "LPUART1_DE" bidirectional line)
				(alternate "LPUART1_RTS" bidirectional line)
				(alternate "SPI2_NSS" bidirectional line)
				(alternate "TIM15_BKIN" bidirectional line)
				(alternate "TIM1_BKIN" bidirectional line)
				(alternate "TSC_G1_IO1" bidirectional line)
				(alternate "USART3_CK" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB13")
				(number "34")
				(alternate "I2C2_SCL" bidirectional line)
				(alternate "LCD_SEG13" bidirectional line)
				(alternate "LPTIM3_IN1" bidirectional line)
				(alternate "LPUART1_CTS" bidirectional line)
				(alternate "SPI2_SCK" bidirectional line)
				(alternate "TIM15_CH1N" bidirectional line)
				(alternate "TIM1_CH1N" bidirectional line)
				(alternate "TSC_G1_IO2" bidirectional line)
				(alternate "USART3_CTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB14")
				(number "35")
				(alternate "I2C2_SDA" bidirectional line)
				(alternate "LCD_SEG14" bidirectional line)
				(alternate "LPTIM3_ETR" bidirectional line)
				(alternate "SPI2_MISO" bidirectional line)
				(alternate "TIM15_CH1" bidirectional line)
				(alternate "TIM1_CH2N" bidirectional line)
				(alternate "TSC_G1_IO3" bidirectional line)
				(alternate "USART3_DE" bidirectional line)
				(alternate "USART3_RTS" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PB15")
				(number "36")
				(alternate "LCD_SEG15" bidirectional line)
				(alternate "PWR_WKUP7" bidirectional line)
				(alternate "RTC_REFIN" bidirectional line)
				(alternate "SPI2_MOSI" bidirectional line)
				(alternate "TAMP_IN3" bidirectional line)
				(alternate "TIM15_CH2" bidirectional line)
				(alternate "TIM1_CH3N" bidirectional line)
				(alternate "TSC_G1_IO4" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
)
